# Irrigation with an ESP8266
Tested with D1 mini. Connect a pump with a relais. Relais activation on D4.

## Homeassistant integration
payload_on can also contain the duration of the pump in ms.
Example:
`
switch 5:
- platform: mqtt
  command_topic: greenhousino/pump
  state_topic: greenhousino/pumpstate
  payload_on: "on"
  payload_off: "off"
  name: "Pumpe"
`