(kicad_symbol_lib (version 20201005) (generator kicad_symbol_editor)
  (symbol "Amplifier_Audio:IR4301" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -7.62 20.955 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "IR4301" (id 1) (at -7.62 19.05 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:Infineon_PQFN-22-15-4EP_6x5mm_P0.65mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/ir4301.pdf?fileId=5546d462533600a4015355d5fc691819" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "integrated class d amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "PowIRaudio Integrated Analog Input Class D Audio Amplifier, 160W/4ohm, 80V, PQFN-22" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*PQFN*4EP*6x5mm*P0.65mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IR4301_0_1"
      (rectangle (start -7.62 -15.24) (end 7.62 17.78)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "IR4301_1_1"
      (pin power_in line (at -10.16 15.24 0) (length 2.54)
        (name "VAA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -17.78 90) (length 2.54)
        (name "VN" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "VS" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 20.32 270) (length 2.54)
        (name "VP" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 7.62 180) (length 2.54)
        (name "VB" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 10.16 180) (length 2.54)
        (name "CSH" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -17.78 90) (length 2.54) hide
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 0 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 12.7 0) (length 2.54)
        (name "IN+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 10.16 0) (length 2.54)
        (name "IN-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 7.62 0) (length 2.54)
        (name "COMP" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -2.54 0) (length 2.54)
        (name "CSD" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -12.7 0) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -7.62 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -17.78 90) (length 2.54)
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:IR4311" (extends "IR4301")
    (property "Reference" "U" (id 0) (at -7.62 20.955 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "IR4311" (id 1) (at -7.62 19.05 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:Infineon_PQFN-22-15-4EP_6x5mm_P0.65mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/ir4301.pdf?fileId=5546d462533600a4015355d5fc691819" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "integrated class d amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "PowIRaudio Integrated Analog Input Class D Audio Amplifier, 90W/4ohm, 60V, PQFN-22" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*PQFN*4EP*6x5mm*P0.65mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:IR4321" (extends "IR4301")
    (property "Reference" "U" (id 0) (at -7.62 20.955 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "IR4321" (id 1) (at -7.62 19.05 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:Infineon_PQFN-22-15-4EP_6x5mm_P0.65mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/ir4301.pdf?fileId=5546d462533600a4015355d5fc691819" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "integrated class d amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "PowIRaudio Integrated Analog Input Class D Audio Amplifier, 35W/4ohm, 40V, PQFN-22" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*PQFN*4EP*6x5mm*P0.65mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:IR4302" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -7.62 20.955 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "IR4302" (id 1) (at -7.62 19.05 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:Infineon_PQFN-44-31-5EP_7x7mm_P0.5mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/ir4302.pdf?fileId=5546d462533600a4015355d602a9181d" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "integrated class d amplifier 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "PowIRaudio 2 Channel Integrated Analog Input Class D Audio Amplifier, 130W/4ohm, 80V, PQFN-44" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*PQFN*5EP*7x7mm*P0.5mm*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IR4302_0_1"
      (rectangle (start -7.62 -15.24) (end 7.62 17.78)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "IR4302_1_1"
      (pin open_collector line (at -10.16 2.54 0) (length 2.54)
        (name "CLIP" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 7.62 0) (length 2.54)
        (name "COMP1" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -2.54 0) (length 2.54)
        (name "CSD" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -10.16 5.08 0) (length 2.54)
        (name "FAULT" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -5.08 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -7.62 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -17.78 90) (length 2.54)
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 10.16 180) (length 2.54)
        (name "CSH1" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 7.62 180) (length 2.54)
        (name "VB1" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "VS1" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 20.32 270) (length 2.54)
        (name "VP1" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54) hide
        (name "VS1" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -17.78 90) (length 2.54)
        (name "VN1" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -17.78 90) (length 2.54) hide
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -10.16 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -17.78 90) (length 2.54) hide
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 0 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -12.7 0) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 15.24 0) (length 2.54)
        (name "VAA" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 12.7 0) (length 2.54)
        (name "IN+1" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 10.16 0) (length 2.54)
        (name "IN-1" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "IR4302_2_1"
      (pin output line (at -10.16 7.62 0) (length 2.54)
        (name "COMP2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -17.78 90) (length 2.54)
        (name "VN2" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "VS2" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 20.32 270) (length 2.54)
        (name "VP2" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54) hide
        (name "VS2" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 7.62 180) (length 2.54)
        (name "VB2" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 10.16 180) (length 2.54)
        (name "CSH2" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 10.16 0) (length 2.54)
        (name "IN-2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 12.7 0) (length 2.54)
        (name "IN+2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:IR4312" (extends "IR4302")
    (property "Reference" "U" (id 0) (at -7.62 20.955 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "IR4312" (id 1) (at -7.62 19.05 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:Infineon_PQFN-44-31-5EP_7x7mm_P0.5mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/ir4302.pdf?fileId=5546d462533600a4015355d602a9181d" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "integrated class d amplifier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "PowIRaudio 2 Channel Integrated Analog Input Class D Audio Amplifier, 100W/4ohm, 60V, PQFN-44" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*PQFN*5EP*7x7mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:IR4322" (extends "IR4302")
    (property "Reference" "U" (id 0) (at -7.62 20.955 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "IR4322" (id 1) (at -7.62 19.05 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:Infineon_PQFN-44-31-5EP_7x7mm_P0.5mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/ir4302.pdf?fileId=5546d462533600a4015355d602a9181d" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "integrated class d amplifier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "PowIRaudio 2 Channel Integrated Analog Input Class D Audio Amplifier, 35W/4ohm, 40V, PQFN-44" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*PQFN*5EP*7x7mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:IRS2052M" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 26.035 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "IRS2052M" (id 1) (at 0 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:Infineon_MLPQ-48-1EP_7x7mm_P0.5mm_EP5.55x5.55mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/irs2052mpbf.pdf?fileId=5546d462533600a401535675d3b32788" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "Gate Driver Class D 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2 CH Digital Audio Amplifier, PWM Modulator, +/-100V, 0.5/0.6A, MLPQ-48" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*MLPQ*1EP*7x7mm*P0.5mm*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IRS2052M_0_1"
      (rectangle (start -7.62 -20.32) (end 7.62 22.86)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "IRS2052M_1_1"
      (pin no_connect line (at -7.62 17.78 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 10.16 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54)
        (name "VS1" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 0 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "HO1" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 17.78 180) (length 2.54)
        (name "VB1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 20.32 180) (length 2.54)
        (name "CSH1" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -15.24 180) (length 2.54)
        (name "LO1" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -5.08 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 15.24 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 12.7 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 10.16 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -10.16 0) (length 2.54)
        (name "OTP" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -22.86 90) (length 2.54)
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -5.08 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -17.78 0) (length 2.54)
        (name "DT" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -15.24 0) (length 2.54)
        (name "OCSET" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -10.16 -12.7 0) (length 2.54)
        (name "VREF" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 2.54 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 0 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 -2.54 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 5.08 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -7.62 0) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 20.32 0) (length 2.54)
        (name "VAA" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "IN1" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 12.7 0) (length 2.54)
        (name "COMP1" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -10.16 7.62 0) (length 2.54)
        (name "CLIP1" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 2.54 0) (length 2.54)
        (name "CSD" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 -7.62 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "IRS2052M_2_1"
      (pin power_in line (at 10.16 -5.08 180) (length 2.54)
        (name "VCC2" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -10.16 5.08 0) (length 2.54)
        (name "OTW" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -15.24 180) (length 2.54)
        (name "LO2" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 20.32 180) (length 2.54)
        (name "CSH2" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 17.78 180) (length 2.54)
        (name "VB2" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "HO2" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54)
        (name "VS2" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -10.16 2.54 0) (length 2.54)
        (name "FAULT" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -10.16 7.62 0) (length 2.54)
        (name "CLIP2" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 12.7 0) (length 2.54)
        (name "COMP2" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -17.78 0) (length 2.54)
        (name "CKO" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "IN2" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -5.08 0) (length 2.54)
        (name "X1B" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "X1A" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -12.7 0) (length 2.54)
        (name "X2B" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -7.62 0) (length 2.54)
        (name "X2A" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -15.24 0) (length 2.54)
        (name "XSL" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:IRS2092" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 26.035 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "IRS2092" (id 1) (at 0 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DIP:DIP-16_W7.62mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.infineon.com/dgdl/irs2092.pdf?fileId=5546d462533600a401535675f1be2790" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Gate Driver Class D" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Protected Digital Audio Amplifier, PWM Modulator, +/-100V, 1.0/1.2A, PDIP-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IRS2092_0_1"
      (rectangle (start -7.62 -20.32) (end 7.62 22.86)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "IRS2092_1_1"
      (pin power_in line (at -10.16 20.32 0) (length 2.54)
        (name "VAA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -22.86 90) (length 2.54)
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -15.24 180) (length 2.54)
        (name "LO" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -5.08 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54)
        (name "VS" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "HO" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 17.78 180) (length 2.54)
        (name "VB" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 20.32 180) (length 2.54)
        (name "CSH" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 5.08 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "IN-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 12.7 0) (length 2.54)
        (name "COMP" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 2.54 0) (length 2.54)
        (name "CSD" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -7.62 0) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -10.16 -12.7 0) (length 2.54)
        (name "VREF" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -15.24 0) (length 2.54)
        (name "OCSET" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -17.78 0) (length 2.54)
        (name "DT" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:IRS2092S" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 26.035 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "IRS2092S" (id 1) (at 0 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.infineon.com/dgdl/irs2092.pdf?fileId=5546d462533600a401535675f1be2790" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Gate Driver Class D" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Protected Digital Audio Amplifier, PWM Modulator, +/-100V, 1.0/1.2A, SOIC-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IRS2092S_0_1"
      (rectangle (start -7.62 -20.32) (end 7.62 22.86)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "IRS2092S_1_1"
      (pin power_in line (at -10.16 20.32 0) (length 2.54)
        (name "VAA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -22.86 90) (length 2.54)
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -15.24 180) (length 2.54)
        (name "LO" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -5.08 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54)
        (name "VS" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "HO" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 17.78 180) (length 2.54)
        (name "VB" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 20.32 180) (length 2.54)
        (name "CSH" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 5.08 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "IN-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 12.7 0) (length 2.54)
        (name "COMP" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 2.54 0) (length 2.54)
        (name "CSD" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -7.62 0) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -10.16 -12.7 0) (length 2.54)
        (name "VREF" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -15.24 0) (length 2.54)
        (name "OCSET" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -17.78 0) (length 2.54)
        (name "DT" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:IRS2093M" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 26.035 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "IRS2093M" (id 1) (at 0 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:Infineon_MLPQ-48-1EP_7x7mm_P0.5mm_EP5.55x5.55mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/irs2093mpbf.pdf?fileId=5546d462533600a401535675fb892793" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "Gate Driver Class D 4ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "4 CH Digital Audio Amplifier, PWM Modulator, +/-100V, 0.5/0.6A, MLPQ-48" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*MLPQ*1EP*7x7mm*P0.5mm*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IRS2093M_0_1"
      (rectangle (start -7.62 -20.32) (end 7.62 22.86)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "IRS2093M_1_1"
      (pin input line (at -10.16 7.62 0) (length 2.54)
        (name "DS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54)
        (name "VS1" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "HO1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 17.78 180) (length 2.54)
        (name "VB1" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 20.32 180) (length 2.54)
        (name "CSH1" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -15.24 180) (length 2.54)
        (name "LO1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 15.24 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 12.7 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 17.78 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 10.16 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 10.16 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -22.86 90) (length 2.54)
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -5.08 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -17.78 0) (length 2.54)
        (name "DT" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -15.24 0) (length 2.54)
        (name "OCSET" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -10.16 -12.7 0) (length 2.54)
        (name "VREF" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 0 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 5.08 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -7.62 0) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 20.32 0) (length 2.54)
        (name "VAA" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "IN1" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 12.7 0) (length 2.54)
        (name "COMP1" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 2.54 0) (length 2.54)
        (name "CSD" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -5.08 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "IRS2093M_2_1"
      (pin passive line (at 10.16 5.08 180) (length 2.54)
        (name "VS2" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -15.24 180) (length 2.54)
        (name "LO2" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -5.08 180) (length 2.54)
        (name "VCC2" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "IN2" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 12.7 0) (length 2.54)
        (name "COMP2" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 20.32 180) (length 2.54)
        (name "CSH2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 17.78 180) (length 2.54)
        (name "VB2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "HO2" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "IRS2093M_3_1"
      (pin output line (at 10.16 -15.24 180) (length 2.54)
        (name "LO3" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 20.32 180) (length 2.54)
        (name "CSH3" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 17.78 180) (length 2.54)
        (name "VB3" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "HO3" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54)
        (name "VS3" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 12.7 0) (length 2.54)
        (name "COMP3" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "IN3" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "IRS2093M_4_1"
      (pin output line (at 10.16 -15.24 180) (length 2.54)
        (name "LO4" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54)
        (name "VS4" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "HO4" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 17.78 180) (length 2.54)
        (name "VB4" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 20.32 180) (length 2.54)
        (name "CSH4" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 12.7 0) (length 2.54)
        (name "COMP4" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "IN4" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:IRS20957S" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "IRS20957S" (id 1) (at 0 21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.infineon.com/dgdl/irs20957spbf.pdf?fileId=5546d462533600a401535676143e2799" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Gate Driver Class D" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Protected Digital Audio Driver, +/-100V, 1.0/1.2A, SOIC-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IRS20957S_0_1"
      (rectangle (start -7.62 -17.78) (end 7.62 20.32)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "IRS20957S_1_1"
      (pin power_in line (at -10.16 17.78 0) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -12.7 180) (length 2.54)
        (name "LO" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -2.54 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 0 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54)
        (name "VS" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "HO" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 15.24 180) (length 2.54)
        (name "VB" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 17.78 180) (length 2.54)
        (name "CSH" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 5.08 0) (length 2.54)
        (name "CSD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 12.7 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -5.08 0) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 0 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -10.16 -10.16 0) (length 2.54)
        (name "VREF" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -12.7 0) (length 2.54)
        (name "OCSET" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -15.24 0) (length 2.54)
        (name "DT" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -20.32 90) (length 2.54)
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:IRS20965S" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "IRS20965S" (id 1) (at 0 21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/irs20965spbf.pdf?fileId=5546d462533600a4015356761d8b279b" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Gate Driver Class D" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Class D Audio Driver, +/-100V, 2.0/2.0A, SOIC-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IRS20965S_0_1"
      (rectangle (start -7.62 -17.78) (end 7.62 20.32)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "IRS20965S_1_1"
      (pin power_in line (at -10.16 17.78 0) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -12.7 180) (length 2.54)
        (name "LO" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -2.54 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -15.24 0) (length 2.54)
        (name "STP" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54)
        (name "VS" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "HO" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 15.24 180) (length 2.54)
        (name "VB" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 17.78 180) (length 2.54)
        (name "CSH" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 5.08 0) (length 2.54)
        (name "CSD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -10.16 7.62 0) (length 2.54)
        (name "OC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "HIN" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 12.7 0) (length 2.54)
        (name "LIN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -5.08 0) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -10.16 -10.16 0) (length 2.54)
        (name "VREF" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -12.7 0) (length 2.54)
        (name "OCSET" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -20.32 90) (length 2.54)
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:IRS2452AM" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 26.035 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "IRS2452AM" (id 1) (at 0 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:Infineon_MLPQ-40-32-1EP_7x7mm_P0.5mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRS2452AM-DS-v01_00-EN.pdf?fileId=5546d462584d1d4a01584ee4f1f00713" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "Gate Driver Class D 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Class D Audio IC, PWM Modulator, +/-200V, 0.5/0.6A, MLPQ-32" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Infineon*MLPQ*1EP*7x7mm*P0.5mm*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IRS2452AM_0_1"
      (rectangle (start -7.62 -20.32) (end 7.62 22.86)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "IRS2452AM_1_1"
      (pin output line (at -10.16 12.7 0) (length 2.54)
        (name "COMP1" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 2.54 0) (length 2.54)
        (name "CSD" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 10.16 0) (length 2.54)
        (name "BTL" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 20.32 180) (length 2.54)
        (name "CSH1" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 17.78 180) (length 2.54)
        (name "VB1" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "HO1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54)
        (name "VS1" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -2.54 180) (length 2.54)
        (name "CSL1" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -15.24 180) (length 2.54)
        (name "LO1" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -22.86 90) (length 2.54)
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -5.08 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -5.08 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -10.16 0) (length 2.54)
        (name "OTP" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -17.78 0) (length 2.54)
        (name "DT" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 7.62 0) (length 2.54)
        (name "A/B" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -7.62 0) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 20.32 0) (length 2.54)
        (name "VAA" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 0 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 5.08 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 17.78 0) (length 2.54)
        (name "IN+1" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "IN-1" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "IRS2452AM_2_1"
      (pin output line (at -10.16 12.7 0) (length 2.54)
        (name "COMP2" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "IN-2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -15.24 180) (length 2.54)
        (name "LO2" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -2.54 180) (length 2.54)
        (name "CSL2" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 5.08 180) (length 2.54)
        (name "VS2" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "HO2" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 17.78 180) (length 2.54)
        (name "VB2" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 17.78 0) (length 2.54)
        (name "IN+2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 20.32 180) (length 2.54)
        (name "CSH2" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 7.62 0) (length 2.54)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:IS31AP4991-GRLS2" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "IS31AP4991-GRLS2" (id 1) (at 10.16 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.issi.com/WW/pdf/31AP4991.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "ultra low consumption distortion" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1.2W, 2.7-5.5V, Audio Power Amplifier, Active-Low Standby, SOP-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOP*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IS31AP4991-GRLS2_0_1"
      (polyline
        (pts
          (xy 3.81 -3.302)
          (xy 4.826 -3.302)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 4.318 3.81)
          (xy 4.318 2.794)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 4.826 3.302)
          (xy 3.81 3.302)
        )
        (stroke (width 0)) (fill (type none))
      )
    )
    (symbol "IS31AP4991-GRLS2_1_1"
      (polyline
        (pts
          (xy 3.81 -0.635)
          (xy 3.81 -2.54)
          (xy 5.08 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 2.54)
          (xy 3.81 2.54)
          (xy 3.81 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08)
        (name "BYP" (effects (font (size 0.508 0.508))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "~SDB" (effects (font (size 0.508 0.508))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:IS31AP4991-SLS2" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "IS31AP4991-SLS2" (id 1) (at 10.16 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.issi.com/WW/pdf/31AP4991.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "ultra low consumption distortion" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1.2W, 2.7-5.5V, Audio Power Amplifier, Active-Low Standby, MSOP-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IS31AP4991-SLS2_0_1"
      (polyline
        (pts
          (xy 3.81 -3.302)
          (xy 4.826 -3.302)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 3.302)
          (xy 4.826 3.302)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 4.318 2.794)
          (xy 4.318 3.81)
        )
        (stroke (width 0)) (fill (type none))
      )
    )
    (symbol "IS31AP4991-SLS2_1_1"
      (polyline
        (pts
          (xy 3.81 -0.635)
          (xy 3.81 -2.54)
          (xy 5.08 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 2.54)
          (xy 3.81 2.54)
          (xy 3.81 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "~SDB" (effects (font (size 0.508 0.508))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08)
        (name "BYP" (effects (font (size 0.508 0.508))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM1875" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.81 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM1875" (id 1) (at 3.81 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1875.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "20W Audio Power Amplifier, TO-220-5" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM1875_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM1875_1_1"
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM1876" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 7.62 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM1876" (id 1) (at 7.62 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1876.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Overture Audio Power Amplifier Series Dual 20W Audio Power Amplifier with Mute and Standby Modes, TO-220-15" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM1876_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM1876_1_1"
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "STBY" (effects (font (size 0.508 0.508))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LM1876_2_1"
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "STBY" (effects (font (size 0.508 0.508))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM1877" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM1877" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1877.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dual Audio Power Amplifier, PDIP-14/SOIC-14" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm* DIP*W7.62mm*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM1877_1_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "BIAS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LM1877_2_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LM1877_3_1"
      (pin passive line (at -2.54 -7.62 90) (length 3.81) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -7.62 90) (length 3.81) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -7.62 90) (length 3.81) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -7.62 90) (length 3.81) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -7.62 90) (length 3.81) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM2876" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM2876" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2876.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Overture Audio Power Amplifier Series High-Performance 40W Audio Power Amplifier w/Mute, TO-220-11" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM2876_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM2876_1_1"
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 -2.54 270) (length 3.81) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM380N" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 6.35 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM380N" (id 1) (at 6.35 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DIP:DIP-14_W7.62mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm380.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2.5W Audio Power Amplifier, PDIP-14" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM380N_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM380N_1_1"
      (pin passive line (at 0 7.62 270) (length 5.08)
        (name "BYPASS" (effects (font (size 0.508 0.508))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 -2.54 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "VS" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM380N-8" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 6.35 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM380N-8" (id 1) (at 6.35 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DIP:DIP-8_W7.62mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm380.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2.5W Audio Power Amplifier, PDIP-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM380N-8_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM380N-8_1_1"
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "VS" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 7.62 270) (length 5.08)
        (name "BYPASS" (effects (font (size 0.508 0.508))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM384" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM384" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DIP:DIP-14_W7.62mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm384.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "5W Audio Power Amplifier, PDIP-14" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM384_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM384_1_1"
      (pin passive line (at 0 7.62 270) (length 5.08)
        (name "BYPASS" (effects (font (size 0.508 0.508))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "VS" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM386" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "LM386" (id 1) (at 1.27 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 2.54 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm386.pdf" (id 3) (at 5.08 5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "single Power opamp" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low Voltage Audio Power Amplifier, DIP-8/SOIC-8/SSOP-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* MSSOP*P0.65mm* TSSOP*3x3mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM386_0_1"
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM386_1_1"
      (pin input line (at 0 -7.62 90) (length 5.08)
        (name "GAIN" (effects (font (size 0.508 0.508))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "BYPASS" (effects (font (size 0.508 0.508))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -7.62 90) (length 6.35)
        (name "GAIN" (effects (font (size 0.508 0.508))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM3886" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM3886" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3886.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Overture Audio Power Amplifier Series High-Performance 68W Audio Power Amplifier w/Mute, TO-220-11" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM3886_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM3886_1_1"
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 7.62 270) (length 3.81) hide
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM4752TS" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM4752TS" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin4" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4752.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Stereo 11W Audio Power Amplifier, TO-263-7" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?263*TabPin4*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM4752TS_1_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at 0 -7.62 90) (length 5.08)
        (name "BIAS" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LM4752TS_2_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LM4752TS_3_1"
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM4755TS" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM4755TS" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:TO-263-9_TabPin5" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4755.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Stereo 11W Audio Power Amplifier with Mute, TO-263-9" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?263*TabPin5*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM4755TS_1_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -7.62 90) (length 5.08)
        (name "BIAS" (effects (font (size 0.508 0.508))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LM4755TS_2_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LM4755TS_3_1"
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM4766" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM4766" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4766.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Overture Audio Power Amplifier Series Dual 40W Audio Power Amplifier with Mute, TO-220-15" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM4766_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM4766_1_1"
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LM4766_2_1"
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM4810" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -6.35 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM4810" (id 1) (at 5.08 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4810.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier headphone" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Boomer Dual 105mW Headphone Amplifier with Active-High Shutdown Mode, VSSOP-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM4810_0_1"
      (rectangle (start -7.62 10.16) (end 7.62 -10.16)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM4810_1_1"
      (pin output line (at 10.16 5.08 180) (length 2.54)
        (name "VOUT1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "VIN1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -5.08 180) (length 2.54)
        (name "BYPASS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "SHDN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "VIN2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "VOUT2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM4811" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -6.35 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM4811" (id 1) (at 5.08 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4811.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier headphone 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Boomer Dual 105mW Headphone Amplifier with Digital Volume Control and Shutdown Mode, VSSOP-10" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM4811_0_1"
      (rectangle (start -7.62 10.16) (end 7.62 -10.16)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM4811_1_1"
      (pin output line (at 10.16 5.08 180) (length 2.54)
        (name "VOUT1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "VIN1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -5.08 180) (length 2.54)
        (name "BYPASS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -7.62 0) (length 2.54)
        (name "CLOCK" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "UP/DN" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "SHDN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "VIN2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "VOUT2" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM4950TA" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM4950TA" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4950.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Boomer Audio Power Amplifier Series 7.5W Mono-BTL or 3.1W Stereo Audio Power Amplifier, TO-220-9" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM4950TA_1_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "VINA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "~SHDN" (effects (font (size 0.508 0.508))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08)
        (name "BYP" (effects (font (size 0.508 0.508))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LM4950TA_2_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "VINB" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LM4950TA_3_1"
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -7.62 90) (length 3.81) hide
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM4950TS" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM4950TS" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:TO-263-9_TabPin5" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4950.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Boomer Audio Power Amplifier Series 7.5W Mono-BTL or 3.1W Stereo Audio Power Amplifier, TO-263-9" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?263*TabPin5*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM4950TS_1_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "VINA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "~SHDN" (effects (font (size 0.508 0.508))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08)
        (name "BYP" (effects (font (size 0.508 0.508))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LM4950TS_2_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "VINB" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LM4950TS_3_1"
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -7.62 90) (length 3.81) hide
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM4990ITL" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM4990ITL" (id 1) (at 5.08 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_BGA:Texas_DSBGA-9_1.4715x1.4715mm_Layout3x3_P0.5mm" (id 2) (at 2.54 -11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4990.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier class d" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Boomer 2 Watt Audio Power Amplifier with Selectable Shutdown Logic Level, DSBGA-9" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "*DSBGA*1.4715x1.4715mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM4990ITL_0_1"
      (polyline
        (pts
          (xy 3.81 -0.635)
          (xy 3.81 -2.54)
          (xy 5.08 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 2.54)
          (xy 3.81 2.54)
          (xy 3.81 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM4990ITL_1_1"
      (polyline
        (pts
          (xy 3.81 -3.302)
          (xy 4.826 -3.302)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 4.318 3.81)
          (xy 4.318 2.794)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 4.826 3.302)
          (xy 3.81 3.302)
        )
        (stroke (width 0)) (fill (type none))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "A1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "A2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "A3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "B1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -7.62 90) (length 3.81) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "B2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "B3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -7.62 90) (length 5.08)
        (name "BYP" (effects (font (size 0.508 0.508))))
        (number "C1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "C2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 7.62 270) (length 5.08)
        (name "~SHDN" (effects (font (size 0.508 0.508))))
        (number "C3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LM4990ITL_2_1"
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM4990LD" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 7.62 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM4990LD" (id 1) (at 7.62 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SON:WSON-10-1EP_4x3mm_P0.5mm_EP2.2x2mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4990.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier class d" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Boomer 2 Watt Audio Power Amplifier with Selectable Shutdown Logic Level, WSON-10" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "WSON*EP*4x3mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM4990LD_0_1"
      (polyline
        (pts
          (xy 3.81 -0.635)
          (xy 3.81 -2.54)
          (xy 5.08 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 2.54)
          (xy 3.81 2.54)
          (xy 3.81 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM4990LD_1_1"
      (polyline
        (pts
          (xy 3.81 -3.302)
          (xy 4.826 -3.302)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 4.318 3.81)
          (xy 4.318 2.794)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 4.826 3.302)
          (xy 3.81 3.302)
        )
        (stroke (width 0)) (fill (type none))
      )
      (pin output line (at 0 7.62 270) (length 5.08)
        (name "SHDN" (effects (font (size 0.508 0.508))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -7.62 90) (length 6.35)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -7.62 90) (length 5.08)
        (name "BYP" (effects (font (size 0.508 0.508))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "SD" (effects (font (size 0.508 0.508))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM4990MH" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 7.62 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM4990MH" (id 1) (at 7.62 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4990.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier class d" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Boomer 2 Watt Audio Power Amplifier with Selectable Shutdown Logic Level, MSOP-10" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "MSOP*EP*3x3mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM4990MH_0_1"
      (polyline
        (pts
          (xy 3.81 -0.635)
          (xy 3.81 -2.54)
          (xy 5.08 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 2.54)
          (xy 3.81 2.54)
          (xy 3.81 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM4990MH_1_1"
      (polyline
        (pts
          (xy 3.81 -3.302)
          (xy 4.826 -3.302)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 4.318 3.81)
          (xy 4.318 2.794)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 4.826 3.302)
          (xy 3.81 3.302)
        )
        (stroke (width 0)) (fill (type none))
      )
      (pin output line (at 0 7.62 270) (length 5.08)
        (name "~SHDN" (effects (font (size 0.508 0.508))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -7.62 90) (length 6.35)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -7.62 90) (length 5.08)
        (name "BYP" (effects (font (size 0.508 0.508))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "SD" (effects (font (size 0.508 0.508))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LM4990MM" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LM4990MM" (id 1) (at 5.08 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm4990.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier class d" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Boomer 2 Watt Audio Power Amplifier with Selectable Shutdown Logic Level, VSSOP-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LM4990MM_0_1"
      (polyline
        (pts
          (xy 3.81 -0.635)
          (xy 3.81 -2.54)
          (xy 5.08 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 2.54)
          (xy 3.81 2.54)
          (xy 3.81 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LM4990MM_1_1"
      (polyline
        (pts
          (xy 3.81 -3.302)
          (xy 4.826 -3.302)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 4.318 3.81)
          (xy 4.318 2.794)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 4.826 3.302)
          (xy 3.81 3.302)
        )
        (stroke (width 0)) (fill (type none))
      )
      (pin output line (at 0 7.62 270) (length 5.08)
        (name "~SHDN" (effects (font (size 0.508 0.508))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -7.62 90) (length 5.08)
        (name "BYP" (effects (font (size 0.508 0.508))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:LME49600" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 6.35 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LME49600" (id 1) (at 6.35 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lme49600.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio buffer amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "High-Performance, High-Fidelity, High-Current Headphone Buffer, 250mA, TO-263" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?263*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LME49600_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "LME49600_1_1"
      (pin passive line (at 0 -7.62 90) (length 5.08)
        (name "BW" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:MA12040" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -10.16 44.45 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MA12040" (id 1) (at 3.81 44.45 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.45x5.45mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/Infineon-MA12040-DS-v01_00-EN.pdf?fileId=5546d46264a8de7e0164b7467a3d617c" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "integrated class d amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Filterless and High-Efficiency +4V to +18V Audio Amplifier with Analog Input, QFN-64" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MA12040_0_1"
      (rectangle (start -10.16 -43.18) (end 10.16 43.18)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "MA12040_1_1"
      (pin power_in line (at 2.54 -45.72 90) (length 2.54)
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 20.32 180) (length 2.54)
        (name "OUT0B" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 20.32 180) (length 2.54) hide
        (name "OUT0B" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 22.86 180) (length 2.54)
        (name "CF0BN" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 5.08 0) (length 2.54)
        (name "~CLIP" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 2.54 0) (length 2.54)
        (name "~ERROR" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 45.72 270) (length 2.54)
        (name "AVDD" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -38.1 0) (length 2.54)
        (name "CMSE" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -45.72 90) (length 2.54)
        (name "AVSS" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -40.64 0) (length 2.54)
        (name "CREF" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 33.02 0) (length 2.54)
        (name "IN0A" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 27.94 0) (length 2.54)
        (name "IN0B" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 22.86 0) (length 2.54)
        (name "IN1A" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 17.78 0) (length 2.54)
        (name "IN1B" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -45.72 90) (length 2.54) hide
        (name "AVSS" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -45.72 90) (length 2.54)
        (name "DVSS" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -10.16 0) (length 2.54)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -17.78 0) (length 2.54)
        (name "AD0" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -20.32 0) (length 2.54)
        (name "AD1" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 35.56 180) (length 2.54)
        (name "CF0AN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -12.7 0) (length 2.54)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 2.54)
        (name "CLKM/S" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 12.7 0) (length 2.54)
        (name "CLKIO" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.54 0) (length 2.54)
        (name "~ENABLE" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 2.54)
        (name "~MUTE" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -2.54 180) (length 2.54)
        (name "CF1BN" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -5.08 180) (length 2.54)
        (name "OUT1B" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -5.08 180) (length 2.54) hide
        (name "OUT1B" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 33.02 180) (length 2.54)
        (name "OUT0A" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 2.54 180) (length 2.54)
        (name "CF1BP" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 45.72 270) (length 2.54)
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 45.72 270) (length 2.54) hide
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 15.24 180) (length 2.54)
        (name "CF1AP" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 7.62 180) (length 2.54)
        (name "OUT1A" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 7.62 180) (length 2.54) hide
        (name "OUT1A" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 10.16 180) (length 2.54)
        (name "CF1AN" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 40.64 0) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 33.02 180) (length 2.54) hide
        (name "OUT0A" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -27.94 0) (length 2.54)
        (name "MSEL1" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -25.4 0) (length 2.54)
        (name "MSEL0" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -17.78 180) (length 2.54)
        (name "CGD1N" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -12.7 180) (length 2.54)
        (name "CGD1P" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -33.02 0) (length 2.54)
        (name "VGDC" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 45.72 270) (length 2.54)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -35.56 0) (length 2.54)
        (name "CDC" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -20.32 180) (length 2.54)
        (name "CFDCP" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -25.4 180) (length 2.54)
        (name "CFDCN" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -45.72 90) (length 2.54) hide
        (name "DVSS" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 40.64 180) (length 2.54)
        (name "CF0AP" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -27.94 180) (length 2.54)
        (name "CGD0P" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -33.02 180) (length 2.54)
        (name "CGD0N" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -35.56 180) (length 2.54)
        (name "CFGDP" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -40.64 180) (length 2.54)
        (name "CFGDN" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 38.1 0) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 45.72 270) (length 2.54)
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 45.72 270) (length 2.54) hide
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 27.94 180) (length 2.54)
        (name "CF0BP" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:MA12070" (extends "MA12040")
    (property "Reference" "U" (id 0) (at -10.16 44.45 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MA12070" (id 1) (at 3.81 44.45 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.45x5.45mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/Infineon-MA12070-DS-v01_00-EN.pdf?fileId=5546d46264a8de7e0164b750002861a5" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "integrated class d amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Filterless and High-Efficiency +4V to +26V Audio Amplifier with Analog Input, QFN-64" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:MA12040P" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -10.16 44.45 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MA12040P" (id 1) (at 3.81 44.45 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.45x5.45mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/Infineon-MA12040P-DS-v01_00-EN.pdf?fileId=5546d46264a8de7e0164b74ff0e561a2" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "integrated class d amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Filterless and High-Efficiency +4V to +18V Audio Amplifier with I2S Digital Input, QFN-64" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MA12040P_0_1"
      (rectangle (start -10.16 -43.18) (end 10.16 43.18)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "MA12040P_1_1"
      (pin power_in line (at 2.54 -45.72 90) (length 2.54)
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 20.32 180) (length 2.54)
        (name "OUT0B" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 20.32 180) (length 2.54) hide
        (name "OUT0B" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 22.86 180) (length 2.54)
        (name "CF0BN" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 5.08 0) (length 2.54)
        (name "~CLIP" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 2.54 0) (length 2.54)
        (name "~ERROR" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 45.72 270) (length 2.54)
        (name "AVDD" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -38.1 0) (length 2.54)
        (name "CMSE" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -45.72 90) (length 2.54)
        (name "AVSS" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -40.64 0) (length 2.54)
        (name "CREF" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 33.02 0) (length 2.54)
        (name "SCLK" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 27.94 0) (length 2.54)
        (name "WS" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 22.86 0) (length 2.54)
        (name "SD0" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 17.78 0) (length 2.54)
        (name "SD1" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -45.72 90) (length 2.54) hide
        (name "AVSS" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -45.72 90) (length 2.54)
        (name "DVSS" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -10.16 0) (length 2.54)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -17.78 0) (length 2.54)
        (name "AD0" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -20.32 0) (length 2.54)
        (name "AD1" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 35.56 180) (length 2.54)
        (name "CF0AN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -12.7 0) (length 2.54)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 2.54)
        (name "CLKM/S" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 12.7 0) (length 2.54)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.54 0) (length 2.54)
        (name "~ENABLE" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 2.54)
        (name "~MUTE" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -2.54 180) (length 2.54)
        (name "CF1BN" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -5.08 180) (length 2.54)
        (name "OUT1B" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -5.08 180) (length 2.54) hide
        (name "OUT1B" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 33.02 180) (length 2.54)
        (name "OUT0A" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 2.54 180) (length 2.54)
        (name "CF1BP" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 45.72 270) (length 2.54)
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 45.72 270) (length 2.54) hide
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 15.24 180) (length 2.54)
        (name "CF1AP" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 7.62 180) (length 2.54)
        (name "OUT1A" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 7.62 180) (length 2.54) hide
        (name "OUT1A" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 10.16 180) (length 2.54)
        (name "CF1AN" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -45.72 90) (length 2.54) hide
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 40.64 0) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 33.02 180) (length 2.54) hide
        (name "OUT0A" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -27.94 0) (length 2.54)
        (name "MSEL1" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -25.4 0) (length 2.54)
        (name "MSEL0" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -17.78 180) (length 2.54)
        (name "CGD1N" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -12.7 180) (length 2.54)
        (name "CGD1P" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -33.02 0) (length 2.54)
        (name "VGDC" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 45.72 270) (length 2.54)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -35.56 0) (length 2.54)
        (name "CDC" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -20.32 180) (length 2.54)
        (name "CFDCP" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -25.4 180) (length 2.54)
        (name "CFDCN" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -45.72 90) (length 2.54) hide
        (name "DVSS" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 40.64 180) (length 2.54)
        (name "CF0AP" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -27.94 180) (length 2.54)
        (name "CGD0P" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -33.02 180) (length 2.54)
        (name "CGD0N" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -35.56 180) (length 2.54)
        (name "CFGDP" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -40.64 180) (length 2.54)
        (name "CFGDN" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 38.1 0) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 45.72 270) (length 2.54)
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 45.72 270) (length 2.54) hide
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 27.94 180) (length 2.54)
        (name "CF0BP" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:MA12070P" (extends "MA12040P")
    (property "Reference" "U" (id 0) (at -10.16 44.45 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MA12070P" (id 1) (at 3.81 44.45 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.45x5.45mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.infineon.com/dgdl/Infineon-MA12070P-DS-v01_00-EN.pdf?fileId=5546d46264a8de7e0164b761f2f261e4" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "integrated class d amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Filterless and High-Efficiency +4V to +26V Audio Amplifier with I2S Digital Input, QFN-64" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:MAX9715ETE+" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -7.62 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX9715ETE+" (id 1) (at 8.89 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:TQFN-16-1EP_5x5mm_P0.8mm_EP3.1x3.1mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX9715.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Class-D Stereo" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2.8W, Low-EMI, Stereo, Filterless Class D Audio Amplifier, TQFN-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TQFN*1EP*5x5mm*P0.8mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX9715ETE+_0_1"
      (rectangle (start -10.16 10.16) (end 10.16 -10.16)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "MAX9715ETE+_1_1"
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -5.08 180) (length 2.54)
        (name "OUTR-" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -2.54 180) (length 2.54)
        (name "OUTR+" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -12.7 90) (length 2.54) hide
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -7.62 0) (length 2.54)
        (name "BIAS" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 12.7 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 2.54)
        (name "INR" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 2.54)
        (name "INL" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -12.7 90) (length 2.54)
        (name "PAD" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 2.54)
        (name "OUTL+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 2.54 180) (length 2.54)
        (name "OUTL-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 12.7 0 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 2.54)
        (name "GAIN" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.54 0) (length 2.54)
        (name "~SHDN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 12.7 270) (length 2.54) hide
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:MAX9814" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -20.32 13.97 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MAX9814" (id 1) (at 11.43 13.97 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x3mm_P0.4mm_EP1.78x2.35mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX9814.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio microphone amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microphone Amplifier with AGC and Low-Noise Microphone Bias, TDFN-14" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "*DFN*EP*3x3mm*P0.4mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX9814_0_0"
      (text "AGC" (at 1.27 3.81 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "Gain" (at 8.89 -2.54 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "LN ref" (at -7.62 3.81 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "LNA" (at -8.89 -2.54 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "VGA" (at 0 -2.54 0)
        (effects (font (size 1.27 1.27)))
      )
      (rectangle (start -11.43 5.08) (end -3.81 2.54)
        (stroke (width 0.254)) (fill (type none))
      )
      (rectangle (start -2.54 5.08) (end 5.08 2.54)
        (stroke (width 0.254)) (fill (type none))
      )
      (polyline
        (pts
          (xy -11.43 -2.54)
          (xy -13.97 -2.54)
        )
        (stroke (width 0.254)) (fill (type none))
      )
      (polyline
        (pts
          (xy -8.89 2.54)
          (xy -8.89 0)
        )
        (stroke (width 0.254)) (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 -2.54)
          (xy -5.08 -2.54)
        )
        (stroke (width 0.254)) (fill (type none))
      )
      (polyline
        (pts
          (xy 0 2.54)
          (xy 0 0)
        )
        (stroke (width 0.254)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 -2.54)
          (xy 6.35 -2.54)
        )
        (stroke (width 0.254)) (fill (type none))
      )
      (polyline
        (pts
          (xy -11.43 3.81)
          (xy -13.97 3.81)
          (xy -13.97 1.27)
        )
        (stroke (width 0.254)) (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 -2.54)
          (xy -11.43 1.27)
          (xy -11.43 -6.35)
          (xy -5.08 -2.54)
        )
        (stroke (width 0.254)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 -2.54)
          (xy -2.54 1.27)
          (xy -2.54 -6.35)
          (xy 3.81 -2.54)
        )
        (stroke (width 0.254)) (fill (type none))
      )
      (polyline
        (pts
          (xy 12.7 -2.54)
          (xy 6.35 1.27)
          (xy 6.35 -6.35)
          (xy 12.7 -2.54)
        )
        (stroke (width 0.254)) (fill (type none))
      )
    )
    (symbol "MAX9814_0_1"
      (rectangle (start -20.32 12.7) (end 20.32 -12.7)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "MAX9814_1_1"
      (pin input line (at -22.86 10.16 0) (length 2.54)
        (name "CT" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -5.08 0) (length 2.54)
        (name "GAIN" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -22.86 -7.62 0) (length 2.54)
        (name "BIAS" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -22.86 0 0) (length 2.54)
        (name "MICBIAS" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 5.08 0) (length 2.54)
        (name "TH" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 15.24 270) (length 2.54)
        (name "~SHDN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -22.86 -10.16 0) (length 2.54)
        (name "CG" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 15.24 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 -2.54 180) (length 2.54)
        (name "MICOUT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -15.24 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -2.54 0) (length 2.54)
        (name "MICIN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 7.62 0) (length 2.54)
        (name "A/R" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:MAX98306xDT" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 10.16 14.605 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX98306xDT" (id 1) (at 10.16 12.065 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:TDFN-14-1EP_3x3mm_P0.4mm_EP1.78x2.35mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX98306.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Class-D stereo amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Stereo 3.7 W Class D Amplifier, TDFN-14" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TDFN*1EP*3x3mm*P0.4mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX98306xDT_0_1"
      (rectangle (start -10.16 10.16) (end 10.16 -10.16)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "MAX98306xDT_1_1"
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 -2.54 180) (length 2.54)
        (name "OUTR+" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54) hide
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 5.08 180) (length 2.54)
        (name "OUTL+" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 2.54 180) (length 2.54)
        (name "OUTL-" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54) hide
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -7.62 0) (length 2.54)
        (name "~{SHDN}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 2.54)
        (name "INL+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 2.54)
        (name "INL-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 2.54)
        (name "GAIN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 2.54)
        (name "INR-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 2.54)
        (name "INR+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54) hide
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 -5.08 180) (length 2.54)
        (name "OUTR-" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:MAX9850xTI" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 19.05 25.4 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MAX9850xTI" (id 1) (at 16.51 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:TQFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm_ThermalVias" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX9850.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio ampflifier stereo i2s" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Stereo audio DAC with headphone amplifier, TQFN-28" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TQFN*1EP*5x5mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX9850xTI_0_1"
      (rectangle (start -12.7 22.86) (end 12.7 -22.86)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "MAX9850xTI_1_1"
      (pin bidirectional line (at -15.24 10.16 0) (length 2.54)
        (name "LRCLK" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 2.54 0) (length 2.54)
        (name "INL" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 2.54 180) (length 2.54)
        (name "OUTR" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 5.08 180) (length 2.54)
        (name "OUTL" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 15.24 15.24 180) (length 2.54)
        (name "REF" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -25.4 90) (length 2.54)
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 15.24 10.16 180) (length 2.54)
        (name "NREG" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 15.24 12.7 180) (length 2.54)
        (name "PREG" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 25.4 270) (length 2.54)
        (name "AVDD" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 -15.24 180) (length 2.54)
        (name "HPR" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 -10.16 180) (length 2.54)
        (name "HPL" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 12.7 0) (length 2.54)
        (name "BCLK" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 -25.4 90) (length 2.54)
        (name "SVSS" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 -12.7 180) (length 2.54)
        (name "HPS" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -25.4 90) (length 2.54)
        (name "PVSS" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 -5.08 180) (length 2.54)
        (name "C1N" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -25.4 90) (length 2.54)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 -2.54 180) (length 2.54)
        (name "C1P" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 25.4 270) (length 2.54)
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -7.62 0) (length 2.54)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -5.08 0) (length 2.54)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -25.4 90) (length 2.54) hide
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 7.62 0) (length 2.54)
        (name "SDIN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 25.4 270) (length 2.54)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 15.24 0) (length 2.54)
        (name "MCLK" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -25.4 90) (length 2.54)
        (name "DGND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -10.16 0) (length 2.54)
        (name "ADD" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -15.24 0) (length 2.54)
        (name "GPIO" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 2.54)
        (name "INR" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:OPA1622" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.81 6.35 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "OPA1622" (id 1) (at 3.81 3.81 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SON:Texas_S-PVSON-N10" (id 2) (at 0 -10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa1622.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "dual opamp audio" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "High-Fidelity, Bipolar-Input, Audio Operational Amplifier, VSON-10" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Texas*PVSON*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "OPA1622_1_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "EN" (effects (font (size 0.508 0.508))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "OPA1622_2_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "OPA1622_3_1"
      (pin passive line (at -2.54 -7.62 90) (length 3.81) hide
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:PAM8301" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 6.35 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "PAM8301" (id 1) (at 6.35 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-6" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM8301.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier class d" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Filterless Class-D Mono Audio Amplifier, 1.5W, TSOT-26" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "PAM8301_0_1"
      (rectangle (start -7.62 5.08) (end 7.62 -5.08)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "PAM8301_1_1"
      (pin output line (at 10.16 -2.54 180) (length 2.54)
        (name "OUT-" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "~SD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 7.62 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 2.54 180) (length 2.54)
        (name "OUT+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:PAM8302AAD" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 7.62 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "PAM8302AAD" (id 1) (at 7.62 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM8302A.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier class d" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2.5W Filterless Class-D Mono Audio Amplifier, SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "PAM8302AAD_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "PAM8302AAD_1_1"
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "~SD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 -5.08 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "IN+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "IN-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 5.08 180) (length 2.54)
        (name "OUT+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "OUT-" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:PAM8302AAS" (extends "PAM8302AAD")
    (property "Reference" "U" (id 0) (at 7.62 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "PAM8302AAS" (id 1) (at 7.62 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM8302A.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier class d" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2.5W Filterless Class-D Mono Audio Amplifier, MSOP-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:PAM8302AAY" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 7.62 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "PAM8302AAY" (id 1) (at 7.62 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM8302A.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier class d" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2.5W Filterless Class-D Mono Audio Amplifier, DFN-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DFN*EP*3x3mm*P0.65mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "PAM8302AAY_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "PAM8302AAY_1_1"
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "~SD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 -5.08 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "IN+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "IN-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 5.08 180) (length 2.54)
        (name "OUT+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "OUT-" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:PAM8403D" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 16.51 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "PAM8403D" (id 1) (at 6.096 14.224 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:SOP-16_3.9x9.9mm_P1.27mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/PAM8403.pdf" (id 3) (at -5.08 5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier class d" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "3W Filterless Class-D Stereo Audio Amplifier, SOP-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOP*3.9x9.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "PAM8403D_0_1"
      (rectangle (start -10.16 12.7) (end 10.16 -12.7)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "PAM8403D_1_1"
      (pin output line (at 12.7 7.62 180) (length 2.54)
        (name "LOUT+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 2.54)
        (name "INR" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -15.24 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 2.54)
        (name "~SHDN" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 15.24 270) (length 2.54) hide
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -5.08 180) (length 2.54)
        (name "ROUT-" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -7.62 180) (length 2.54)
        (name "ROUT+" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -15.24 90) (length 2.54)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 2.54)
        (name "LOUT-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 15.24 270) (length 2.54)
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -7.62 0) (length 2.54)
        (name "~MUTE" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 15.24 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 2.54)
        (name "INL" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 2.54)
        (name "VREF" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 -10.16 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:SSM2017P" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 7.62 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SSM2017P" (id 1) (at 7.62 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DIP:DIP-8_W7.62mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/obsolete-data-sheets/139484016SSM2017.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio preamplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Self-Contained Audio Preamplifier, DIP-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SSM2017P_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "SSM2017P_1_1"
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "RG1" (effects (font (size 0.508 0.508))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -7.62 90) (length 5.08)
        (name "REF" (effects (font (size 0.508 0.508))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "RG2" (effects (font (size 0.508 0.508))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:SSM2018" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -8.89 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SSM2018" (id 1) (at 6.35 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DIP:DIP-16_W7.62mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/SSM2018.pdf" (id 3) (at -1.27 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio VCA" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Trimless Voltage Controlled Amplifier, DIP-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SSM2018_0_0"
      (text "+" (at -5.08 1.905 0)
        (effects (font (size 0.762 0.762)))
      )
      (text "+" (at 1.905 -1.905 0)
        (effects (font (size 0.762 0.762)))
      )
      (text "+" (at 1.905 5.715 0)
        (effects (font (size 0.762 0.762)))
      )
      (text "-" (at -5.08 0.635 0)
        (effects (font (size 0.762 0.762)))
      )
      (text "-" (at 1.905 -3.175 0)
        (effects (font (size 0.762 0.762)))
      )
      (text "-" (at 1.905 4.445 0)
        (effects (font (size 0.762 0.762)))
      )
    )
    (symbol "SSM2018_0_1"
      (text "GAIN CORE" (at -1.27 0 900)
        (effects (font (size 1.27 1.27)))
      )
      (rectangle (start -10.16 10.16) (end 10.16 -10.16)
        (stroke (width 0.254)) (fill (type background))
      )
      (rectangle (start -2.54 6.35) (end 0 -5.715)
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -5.715 0.635)
          (xy -6.35 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -5.715 1.905)
          (xy -6.35 1.905)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -5.715 7.62)
          (xy -6.985 7.62)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -3.175 1.27)
          (xy -2.54 1.27)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -1.905)
          (xy 1.27 -1.905)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 0 5.715)
          (xy 1.27 5.715)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -3.175)
          (xy 0 -3.175)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 4.445)
          (xy 0 4.445)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 -2.54)
          (xy 4.445 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 5.08)
          (xy 7.62 5.08)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -3.175 7.62)
          (xy -1.27 7.62)
          (xy -1.27 6.35)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 0.635 -3.175)
          (xy 0.635 -5.08)
          (xy 3.175 -5.08)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 0.635 4.445)
          (xy 0.635 2.54)
          (xy 6.35 2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -5.715 3.175)
          (xy -3.175 1.27)
          (xy -5.715 -0.635)
          (xy -5.715 3.175)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -5.715 9.525)
          (xy -3.175 7.62)
          (xy -5.715 5.715)
          (xy -5.715 9.525)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -0.635)
          (xy 3.81 -2.54)
          (xy 1.27 -4.445)
          (xy 1.27 -0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 6.985)
          (xy 3.81 5.08)
          (xy 1.27 3.175)
          (xy 1.27 6.985)
        )
        (stroke (width 0)) (fill (type none))
      )
      (pin passive line (at -12.7 -7.62 0) (length 2.54)
        (name "COMP3" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SSM2018_1_1"
      (pin output line (at 12.7 -7.62 180) (length 2.54)
        (name "+I1-G" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 2.54)
        (name "VC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 7.62 180) (length 2.54)
        (name "MODE" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 2.54)
        (name "VG" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 0 180) (length 2.54)
        (name "BAL" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -2.54 180) (length 2.54)
        (name "V1-G" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 2.54 180) (length 2.54)
        (name "-IG" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -5.08 180) (length 2.54)
        (name "-I1-G" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -2.54 0) (length 2.54)
        (name "COMP1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 2.54)
        (name "+IN" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 2.54)
        (name "-IN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -5.08 0) (length 2.54)
        (name "COMP2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:SSM2120" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 8.89 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SSM2120" (id 1) (at 10.16 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DIP:DIP-22_W7.62mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/obsolete-data-sheets/105738070SSM2120.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio VCA" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dynamic Range Pprocessor/Dual VCA, DIP-22" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SSM2120_1_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "CFT" (effects (font (size 0.508 0.508))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SSM2120_2_1"
      (rectangle (start -5.08 7.62) (end 5.08 -5.08)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 5.08 0) (length 2.54)
        (name "THRESH" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "LOGAV" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 7.62 0 180) (length 2.54)
        (name "CONOUT" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "RECIN" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SSM2120_3_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "CFT" (effects (font (size 0.508 0.508))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SSM2120_4_1"
      (rectangle (start -5.08 7.62) (end 5.08 -5.08)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 5.08 0) (length 2.54)
        (name "THRESH" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "LOGAV" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 7.62 0 180) (length 2.54)
        (name "CONOUT" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "RECIN" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SSM2120_5_0"
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "IREF" (effects (font (size 0.508 0.508))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:SSM2122" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 7.62 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SSM2122" (id 1) (at 7.62 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DIP:DIP-16_W7.62mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/obsolete-data-sheets/105738070SSM2120.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio VCA" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Dynamic Range Pprocessor/Dual VCA, DIP-16" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SSM2122_1_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "CFT" (effects (font (size 0.508 0.508))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SSM2122_2_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "CFT" (effects (font (size 0.508 0.508))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SSM2122_3_0"
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "IREF" (effects (font (size 0.508 0.508))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:SSM2165" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -6.35 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SSM2165" (id 1) (at 5.08 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/obsolete-data-sheets/SSM2165.PDF" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio microphone preamplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microphone Preamplifier with Variable Compression and Noise Gating, DIP-8/SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SSM2165_0_1"
      (rectangle (start -7.62 7.62) (end 7.62 -7.62)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "SSM2165_1_1"
      (pin power_in line (at 0 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "VCAIN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 2.54 0) (length 2.54)
        (name "BUFOUT" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "IN+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -2.54 180) (length 2.54)
        (name "AVG" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -5.08 180) (length 2.54)
        (name "COMP" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 2.54 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:SSM2167" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -6.35 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SSM2167" (id 1) (at 5.08 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/SSM2167.pdf" (id 3) (at -8.89 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio microphone amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low Voltage Microphone Preamplifier with Variable Compression and Noise Gating, MSOP-10" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SSM2167_0_1"
      (rectangle (start -7.62 10.16) (end 7.62 -10.16)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "SSM2167_1_1"
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "VCAIN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -7.62 0) (length 2.54)
        (name "~SD" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 5.08 0) (length 2.54)
        (name "BUFOUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 7.62 0) (length 2.54)
        (name "IN+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 0 180) (length 2.54)
        (name "AVG" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -2.54 180) (length 2.54)
        (name "GATE" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -5.08 180) (length 2.54)
        (name "COMP" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 5.08 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:SSM2211CP" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -7.62 12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SSM2211CP" (id 1) (at 5.08 12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_CSP:LFCSP-8-1EP_3x3mm_P0.5mm_EP1.45x1.74mm" (id 2) (at 2.54 -22.86 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/SSM2211.pdf" (id 3) (at -2.54 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1.5W BTL or 250mW SE 4MHz-bandwidth high performance amplifier, LFCSP-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "LFCSP*1EP*3x3mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SSM2211CP_0_1"
      (polyline
        (pts
          (xy -7.62 10.16)
          (xy -7.62 -10.16)
          (xy 12.7 0)
          (xy -7.62 10.16)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "SSM2211CP_1_1"
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "SHUTDOWN" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -2.54 0) (length 2.54)
        (name "BYPASS" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "IN+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "IN-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 2.54 180) (length 2.54)
        (name "VoutA" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 10.16 270) (length 2.54)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -10.16 90) (length 2.54)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -2.54 180) (length 2.54)
        (name "VoutB" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -10.16 90) (length 2.54) hide
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:SSM2211S" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -7.62 12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SSM2211S" (id 1) (at 5.08 12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (id 2) (at 0 -20.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/SSM2211.pdf" (id 3) (at -2.54 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1.5W BTL or 250mW SE 4MHz-bandwidth high performance amplifier, SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SSM2211S_0_1"
      (polyline
        (pts
          (xy -7.62 10.16)
          (xy -7.62 -10.16)
          (xy 12.7 0)
          (xy -7.62 10.16)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "SSM2211S_1_1"
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "SHUTDOWN" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -2.54 0) (length 2.54)
        (name "BYPASS" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "IN+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "IN-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 2.54 180) (length 2.54)
        (name "VoutA" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 10.16 270) (length 2.54)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -10.16 90) (length 2.54)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -2.54 180) (length 2.54)
        (name "VoutB" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:STK433_Sanyo" (pin_names (offset 0.0254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.81 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "STK433_Sanyo" (id 1) (at 3.81 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SIP:Sanyo_STK4xx-15_59.2x8.0mm_P2.54mm" (id 2) (at 7.62 -8.89 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2-Channel 5 Wmin Audio Frequency Power Amplifier, 4010, SIP-15" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Sanyo*59.2x8.0mm*P2.54mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "STK433_Sanyo_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "STK433_Sanyo_1_1"
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 5.08 270) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 7.62 270) (length 5.08)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -5.08 90) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STK433_Sanyo_2_1"
      (pin passive line (at 2.54 5.08 270) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:STK435_Sanyo" (extends "STK433_Sanyo")
    (property "Reference" "U" (id 0) (at 3.81 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "STK435_Sanyo" (id 1) (at 3.81 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SIP:Sanyo_STK4xx-15_59.2x8.0mm_P2.54mm" (id 2) (at 7.62 -8.89 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2-Channel 7 Wmin Audio Frequency Power Amplifier, 4010, SIP-15" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Sanyo*59.2x8.0mm*P2.54mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:STK436_Sanyo" (extends "STK433_Sanyo")
    (property "Reference" "U" (id 0) (at 3.81 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "STK436_Sanyo" (id 1) (at 3.81 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SIP:Sanyo_STK4xx-15_59.2x8.0mm_P2.54mm" (id 2) (at 7.62 -8.89 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2-Channel 10 Wmin Audio Frequency Power Amplifier, 4010, SIP-15" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Sanyo*59.2x8.0mm*P2.54mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:STK437_Sanyo" (pin_names (offset 0.0254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.81 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "STK437_Sanyo" (id 1) (at 3.81 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SIP:Sanyo_STK4xx-15_78.0x8.0mm_P2.54mm" (id 2) (at 0 -10.16 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2-Channel 12 Wmin Audio Frequency Power Amplifier, 4010, SIP-15" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Sanyo*78.0x8.0mm*P2.54mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "STK437_Sanyo_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "STK437_Sanyo_1_1"
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 5.08 270) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 7.62 270) (length 5.08)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -5.08 90) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "STK437_Sanyo_2_1"
      (pin passive line (at 2.54 5.08 270) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:STK439_Sanyo" (extends "STK437_Sanyo")
    (property "Reference" "U" (id 0) (at 3.81 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "STK439_Sanyo" (id 1) (at 3.81 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SIP:Sanyo_STK4xx-15_78.0x8.0mm_P2.54mm" (id 2) (at 0 -10.16 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2-Channel 16 Wmin Audio Frequency Power Amplifier, 4010, SIP-15" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Sanyo*78.0x8.0mm*P2.54mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:STK441_Sanyo" (extends "STK437_Sanyo")
    (property "Reference" "U" (id 0) (at 3.81 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "STK441_Sanyo" (id 1) (at 3.81 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SIP:Sanyo_STK4xx-15_78.0x8.0mm_P2.54mm" (id 2) (at 0 -10.16 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2-Channel 24 Wmin Audio Frequency Power Amplifier, 4010, SIP-15" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Sanyo*78.0x8.0mm*P2.54mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:STK443_Sanyo" (extends "STK437_Sanyo")
    (property "Reference" "U" (id 0) (at 3.81 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "STK443_Sanyo" (id 1) (at 3.81 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SIP:Sanyo_STK4xx-15_78.0x8.0mm_P2.54mm" (id 2) (at 0 -10.16 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://datasheet.octopart.com/STK430-Sanyo-datasheet-107060.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2-Channel 28 Wmin Audio Frequency Power Amplifier, 4010, SIP-15" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Sanyo*78.0x8.0mm*P2.54mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:Si8241BB" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -5.08 11.43 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "Si8241BB" (id 1) (at 1.27 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si824x.pdf" (id 3) (at 0 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "class d gate driver" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Class D Audio Driver With Precision Dead-Time Generator, 8V UVLO, +/-750V, +0.5/-0.5A, SOIC-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x9.9*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Si8241BB_0_1"
      (rectangle (start -7.62 10.16) (end 7.62 -10.16)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "Si8241BB_1_1"
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "PWM" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -5.08 180) (length 2.54)
        (name "VOB" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -2.54 180) (length 2.54)
        (name "VDDB" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 -7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 2.54 180) (length 2.54)
        (name "GNDA" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 5.08 180) (length 2.54)
        (name "VOA" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 7.62 180) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "VDDI" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "GNDI" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "DISABLE" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -5.08 0) (length 2.54)
        (name "DT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 12.7 270) (length 2.54) hide
        (name "VDDI" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -7.62 180) (length 2.54)
        (name "GNDB" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:Si8241CB" (extends "Si8241BB")
    (property "Reference" "U" (id 0) (at -5.08 11.43 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "Si8241CB" (id 1) (at 1.27 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCD5702-D.PDF" (id 3) (at 0 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "class d gate driver" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Class D Audio Driver With Precision Dead-Time Generator, 10V UVLO, +/-750V, +0.5/-0.5A, SOIC-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x9.9*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:Si8244BB" (extends "Si8241BB")
    (property "Reference" "U" (id 0) (at -5.08 11.43 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "Si8244BB" (id 1) (at 1.27 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCD5702-D.PDF" (id 3) (at 0 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "class d gate driver" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Class D Audio Driver With Precision Dead-Time Generator, 8V UVLO, +/-750V, +4/-4A, SOIC-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x9.9*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:Si8244CB" (extends "Si8241BB")
    (property "Reference" "U" (id 0) (at -5.08 11.43 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "Si8244CB" (id 1) (at 1.27 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCD5702-D.PDF" (id 3) (at 0 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "class d gate driver" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Class D Audio Driver With Precision Dead-Time Generator, 10V UVLO, +/-750V, +4/-4A, SOIC-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x9.9*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:TAS5825MRHB" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -11.43 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TAS5825MRHB" (id 1) (at 13.97 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:VQFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm" (id 2) (at 0 -34.29 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "www.ti.com/lit/ds/symlink/tas5825m.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Class-D Stereo" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "38-W Stereo, Inductor-Less, Digital Input, Closed-Loop Class-D Audio Amplifier with 192-kHz Extended Audio Processing, VQFN-32" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "VQFN*1EP*5x5mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TAS5825MRHB_0_1"
      (rectangle (start -12.7 22.86) (end 12.7 -22.86)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "TAS5825MRHB_1_1"
      (pin passive line (at 15.24 15.24 180) (length 2.54)
        (name "BST_A+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -12.7 0) (length 2.54)
        (name "GPIO1" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -15.24 0) (length 2.54)
        (name "GPIO2" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 10.16 0) (length 2.54)
        (name "LRCLK" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 7.62 0) (length 2.54)
        (name "SCLK" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 5.08 0) (length 2.54)
        (name "SDIN" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 0 0) (length 2.54)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -2.54 0) (length 2.54)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 15.24 0) (length 2.54)
        (name "~PDN" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 25.4 270) (length 2.54)
        (name "GVDD" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 25.4 270) (length 2.54)
        (name "AVDD" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 12.7 180) (length 2.54)
        (name "OUT_A+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -25.4 90) (length 2.54)
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 25.4 270) (length 2.54) hide
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 25.4 270) (length 2.54) hide
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 -7.62 180) (length 2.54)
        (name "OUT_B+" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 -5.08 180) (length 2.54)
        (name "BST_B+" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -25.4 90) (length 2.54)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -25.4 90) (length 2.54) hide
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 -12.7 180) (length 2.54)
        (name "OUT_B-" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 -15.24 180) (length 2.54)
        (name "BST_B-" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 5.08 180) (length 2.54)
        (name "BST_A-" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 25.4 270) (length 2.54)
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 7.62 180) (length 2.54)
        (name "OUT_A-" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -25.4 90) (length 2.54) hide
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -25.4 90) (length 2.54) hide
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 -25.4 90) (length 2.54)
        (name "EP" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 25.4 270) (length 2.54) hide
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -25.4 90) (length 2.54)
        (name "DGND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 25.4 270) (length 2.54)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 25.4 270) (length 2.54)
        (name "VR_DIG" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -15.24 -5.08 0) (length 2.54)
        (name "ADR" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -10.16 0) (length 2.54)
        (name "GPIO0" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TDA1308" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA1308" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TDA1308.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Class-AB Stereo Headphone Driver, SOIC-8/TSSOP-8" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* TSSOP*3x3mm*P0.65mm*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TDA1308_1_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA1308_2_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA1308_3_1"
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TDA2003" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.81 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA2003" (id 1) (at 3.81 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/cd00000123.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "10W Car Radio Audio Amplifier, TO-220-5" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO*220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TDA2003_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "TDA2003_1_1"
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TDA2005" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 7.62 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA2005" (id 1) (at 7.62 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/cd00000124.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "20W Bridge/Stereo Amplifier for Car Radio, TO-220-11" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TDA2005_1_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 5.08 270) (length 3.81)
        (name "BOOT" (effects (font (size 0.508 0.508))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 7.62 270) (length 5.08)
        (name "SVRR" (effects (font (size 0.762 0.762))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA2005_2_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 5.08 270) (length 3.81)
        (name "BOOT" (effects (font (size 0.508 0.508))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA2005_3_1"
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TDA2030" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.81 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA2030" (id 1) (at 3.81 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/cd00000128.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "14W Hi-Fi Audio Amplifier, TO-220-5" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO*220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TDA2030_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "TDA2030_1_1"
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "-Vs" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "+Vs" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TDA2050" (extends "TDA2030")
    (property "Reference" "U" (id 0) (at 3.81 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA2050" (id 1) (at 3.81 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/cd00000131.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "32W Hi-Fi Audio Amplifier, TO-220-5" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO*220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:TDA7052A" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7052A" (id 1) (at 5.08 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TDA7052A_AT.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1W BTL mono audio amplifier with DC volume control, DIP-8/SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*7.5x9mm*P1.27mm* DIP*W7.62mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TDA7052A_0_1"
      (polyline
        (pts
          (xy 1.27 -3.175)
          (xy 2.54 -3.175)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -1.27)
          (xy 2.54 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 2.54)
          (xy 2.54 1.27)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "TDA7052A_1_1"
      (polyline
        (pts
          (xy 1.778 3.81)
          (xy 1.778 2.794)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 3.302)
          (xy 1.27 3.302)
        )
        (stroke (width 0)) (fill (type none))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "VP" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "V" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 2.54 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 5.08)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TDA7264" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 2.54 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7264" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-8_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7264.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "25W + 25W stereo amplifier with mute and standby, TO-220-8" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TDA7264_1_1"
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA7264_2_1"
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA7264_3_1"
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TDA7265" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 2.54 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7265" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7265.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "25W +25W Stereo Amplifier with Mute & St-by, TO-220-11" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TDA7265_1_1"
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA7265_2_1"
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA7265_3_1"
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -7.62 90) (length 3.81) hide
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TDA7265B" (extends "TDA7265")
    (property "Reference" "U" (id 0) (at 2.54 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7265B" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7265b.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "30W + 30W Stereo Amplifier with Mute and Standby, TO-220-11" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:TDA7269A" (extends "TDA7265")
    (property "Reference" "U" (id 0) (at 2.54 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7269A" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7269a.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplfier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "14W+14W Stereo Amplifier with Mute & St-by, TO-220-11" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:TDA7292" (extends "TDA7265")
    (property "Reference" "U" (id 0) (at 2.54 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7292" (id 1) (at 5.08 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7292.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "40W + 40W stereo amplifier with mute and standby, TO-220-11" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:TDA7266" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7266" (id 1) (at 5.08 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7266.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "7+7W Dual Bridge Amplifier, TO-220-15" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TDA7266_1_1"
      (polyline
        (pts
          (xy 3.048 3.175)
          (xy 3.81 3.175)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.175 -3.175)
          (xy 3.81 -3.175)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.429 2.794)
          (xy 3.429 3.556)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 -0.635)
          (xy 3.81 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 2.54)
          (xy 3.81 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 7.62 2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "STBY" (effects (font (size 0.508 0.508))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA7266_2_1"
      (polyline
        (pts
          (xy 3.048 3.175)
          (xy 3.81 3.175)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.175 -3.175)
          (xy 3.81 -3.175)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.429 2.794)
          (xy 3.429 3.556)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 -0.635)
          (xy 3.81 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 2.54)
          (xy 3.81 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA7266_3_1"
      (pin passive line (at -2.54 7.62 270) (length 3.81) hide
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "PG" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "SG" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TDA7297" (extends "TDA7266")
    (property "Reference" "U" (id 0) (at 5.08 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7297" (id 1) (at 5.08 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7297.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "15+15W Dual Bridge Amplifier, TO-220-15" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:TDA7266D" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7266D" (id 1) (at 5.08 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:HSOP-20-1EP_11.0x15.9mm_P1.27mm_SlugDown" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7266d.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "5W+5W Dual Bridge Amplifier, PowerSO-20" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HSOP*EP*11.0x15.9mm*P1.27mm*SlugDown*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TDA7266D_1_1"
      (polyline
        (pts
          (xy 3.81 -0.635)
          (xy 3.81 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 2.54)
          (xy 3.81 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin no_connect line (at 2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 -2.54 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 -2.54 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "STBY" (effects (font (size 0.508 0.508))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA7266D_2_1"
      (polyline
        (pts
          (xy 3.81 -0.635)
          (xy 3.81 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 2.54)
          (xy 3.81 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA7266D_3_1"
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "PG" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "PG" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "PG" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "SG" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 7.62 270) (length 3.81) hide
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "PG" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TDA7266M" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7266M" (id 1) (at 5.08 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7266m.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "7W Mono Bridge Amplifier, TO-220-15" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TDA7266M_0_1"
      (polyline
        (pts
          (xy 3.81 -0.635)
          (xy 3.81 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 2.54)
          (xy 3.81 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "TDA7266M_1_1"
      (pin output line (at 7.62 2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 -2.54 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 7.62 270) (length 3.81) hide
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 -2.54 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 -2.54 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "STBY" (effects (font (size 0.508 0.508))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "PG" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "SG" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TDA7266P" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.08 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7266P" (id 1) (at 5.08 -5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:ST_PowerSSO-24_SlugDown" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7266p.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "3W+3W Dual Bridge Amplifier, PowerSSO-24" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "ST*PowerSSO*SlugDown*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TDA7266P_1_1"
      (polyline
        (pts
          (xy 3.81 -0.635)
          (xy 3.81 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 2.54)
          (xy 3.81 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "STBY" (effects (font (size 0.508 0.508))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 0 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 0 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 0 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -5.08 -2.54 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -5.08 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 -2.54 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 -2.54 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 -2.54 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA7266P_2_1"
      (polyline
        (pts
          (xy 3.81 -0.635)
          (xy 3.81 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 2.54)
          (xy 3.81 0.635)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 -2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 2.54 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA7266P_3_1"
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "PG" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "SG" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 7.62 270) (length 3.81) hide
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "PG" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TDA7293" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 10.16 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7293" (id 1) (at 10.16 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7293.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "120-volt, 100-watt, DMOS Audio Amplifier with Mute and Standby, TO-220-15" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TDA7293_0_1"
      (polyline
        (pts
          (xy -7.62 7.62)
          (xy 7.62 0)
          (xy -7.62 -7.62)
          (xy -7.62 7.62)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "TDA7293_1_1"
      (pin power_in line (at 2.54 -5.08 90) (length 2.54)
        (name "SGND" (effects (font (size 0.508 0.508))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 3.81)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 10.16 270) (length 5.08)
        (name "+Vs" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -10.16 90) (length 5.08)
        (name "-Vs" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 3.81)
        (name "SIG_GND" (effects (font (size 0.508 0.508))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 5.08 270) (length 3.81)
        (name "BOOT" (effects (font (size 0.508 0.508))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 10.16 270) (length 3.81)
        (name "+Vs" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -10.16 90) (length 3.81)
        (name "-Vs" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 5.08 270) (length 2.54)
        (name "STBY" (effects (font (size 0.508 0.508))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TDA7294" (extends "TDA7293")
    (property "Reference" "U" (id 0) (at 10.16 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7294" (id 1) (at 10.16 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7294.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "100V - 100W DMOS Audio Amplifier with Mute/St-by, TO-220-15" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:TDA7295" (extends "TDA7293")
    (property "Reference" "U" (id 0) (at 10.16 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7295" (id 1) (at 10.16 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7295.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "80V - 80W DMOS Audio Amplifier with Mute/St-by, TO-220-15" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:TDA7296" (extends "TDA7293")
    (property "Reference" "U" (id 0) (at 10.16 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7296" (id 1) (at 10.16 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7296.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "70V - 60W DMOS Audio Amplifier with Mute/St-by, TO-220-15" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "Amplifier_Audio:TDA7496" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 6.35 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TDA7496" (id 1) (at 7.62 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.st.com/resource/en/datasheet/tda7297.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "audio amplifier 2ch" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "5W+5W Amplifier with DC Volume Control, TO-220-15" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TO?220*StaggerOdd*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TDA7496_1_1"
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "MUTE" (effects (font (size 0.508 0.508))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "V" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -7.62 -2.54 0) (length 2.54)
        (name "O" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 0 2.54 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "STBY" (effects (font (size 0.508 0.508))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA7496_2_1"
      (polyline
        (pts
          (xy 5.08 0)
          (xy -5.08 5.08)
          (xy -5.08 -5.08)
          (xy 5.08 0)
        )
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -7.62 -2.54 0) (length 2.54)
        (name "O" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -7.62 90) (length 6.35)
        (name "SVR" (effects (font (size 0.508 0.508))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TDA7496_3_1"
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "PG" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -7.62 90) (length 5.08) hide
        (name "PG" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "SG" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TFA9879HN" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -7.62 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TFA9879HN" (id 1) (at -12.7 25.4 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:HVQFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm_ThermalVias" (id 2) (at 7.62 -38.1 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TFA9879.pdf" (id 3) (at -12.7 27.94 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Audio Amplifier Class D NXP Semiconductors" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Mono BTL class-D audio amplifier for portable applications with digital input, HVQFN-24" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HVQFN*1EP*4x4mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TFA9879HN_0_1"
      (polyline
        (pts
          (xy -10.16 22.86)
          (xy 10.16 22.86)
          (xy 10.16 -22.86)
          (xy -10.16 -22.86)
          (xy -10.16 22.86)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "TFA9879HN_1_1"
      (pin bidirectional line (at -12.7 -2.54 0) (length 2.54)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 7.62 180) (length 2.54)
        (name "OUTA" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -25.4 90) (length 2.54) hide
        (name "GNDP" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -25.4 90) (length 2.54)
        (name "GNDP" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -2.54 180) (length 2.54)
        (name "STABA" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 -10.16 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -17.78 0) (length 2.54)
        (name "TEST2" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -7.62 0) (length 2.54)
        (name "ADSEL1" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 2.54)
        (name "SDI2" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 2.54)
        (name "SCK2" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 2.54)
        (name "LRCK2" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 2.54)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 15.24 0) (length 2.54)
        (name "SDI1" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 17.78 0) (length 2.54)
        (name "SCK1" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 20.32 0) (length 2.54)
        (name "LRCK1" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 25.4 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -25.4 90) (length 2.54)
        (name "GNDD" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -25.4 90) (length 2.54)
        (name "EP" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -15.24 0) (length 2.54)
        (name "TEST1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -10.16 0) (length 2.54)
        (name "ADSEL2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -20.32 0) (length 2.54)
        (name "TEST3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 -12.7 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 25.4 270) (length 2.54) hide
        (name "VDDP" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 25.4 270) (length 2.54)
        (name "VDDP" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 2.54 180) (length 2.54)
        (name "OUTB" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:THAT2180" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 7.62 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "THAT2180" (id 1) (at 7.62 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SIP:SIP-8_19x3mm_P2.54mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.thatcorp.com/datashts/THAT_2180-Series_Datasheet.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio vca" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Blackmer Pre-Trimmed IC Voltage Controlled Amplifiers, SIP-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SIP*19x3mm*P2.54mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "THAT2180_0_0"
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "THAT2180_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "THAT2180_1_1"
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "E+" (effects (font (size 0.508 0.508))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -7.62 90) (length 6.35)
        (name "E-" (effects (font (size 0.508 0.508))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "SYM" (effects (font (size 0.508 0.508))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:THAT2181" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 7.62 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "THAT2181" (id 1) (at 7.62 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.thatcorp.com/datashts/THAT_2181-Series_Datasheet.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio vca" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Blackmer Trimmable IC Voltage Controlled Amplifiers, SIP-8/SOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SIP*19x3mm*P2.54mm* SOIC*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "THAT2181_0_0"
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 5.08)
        (name "GND" (effects (font (size 0.508 0.508))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "THAT2181_0_1"
      (polyline
        (pts
          (xy -5.08 5.08)
          (xy 5.08 0)
          (xy -5.08 -5.08)
          (xy -5.08 5.08)
        )
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "THAT2181_1_1"
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 7.62 270) (length 6.35)
        (name "E+" (effects (font (size 0.508 0.508))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -7.62 90) (length 6.35)
        (name "E-" (effects (font (size 0.508 0.508))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 7.62 270) (length 5.08)
        (name "SYM" (effects (font (size 0.508 0.508))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TPA3251" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -8.89 19.05 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TPA3251" (id 1) (at 3.81 19.05 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SO:HTSSOP-44_6.1x14mm_P0.635mm_TopEP4.14x7.01mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpa3251.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "stereo class d amplifier" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "175-W Stereo, 350-W Mono PurePath Ultra-HD Analog-Input Class-D Amplifier, HTSSOP-44" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HTSSOP*6.1x14mm*P0.635mm*" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPA3251_0_1"
      (rectangle (start -10.16 -17.78) (end 10.16 17.78)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "TPA3251_1_1"
      (pin power_in line (at 0 20.32 270) (length 2.54)
        (name "GVDD_AB" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 2.54 0) (length 2.54)
        (name "OSC_IOP" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -7.62 0) (length 2.54)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -20.32 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -20.32 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -10.16 0) (length 2.54)
        (name "AVDD" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -12.7 0) (length 2.54)
        (name "C_START" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 20.32 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -15.24 0) (length 2.54)
        (name "VBG" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -20.32 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -20.32 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -20.32 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -20.32 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -7.62 180) (length 2.54)
        (name "OUT_B" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 20.32 270) (length 2.54)
        (name "PVDD_AB" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 20.32 270) (length 2.54) hide
        (name "PVDD_AB" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 20.32 270) (length 2.54) hide
        (name "PVDD_AB" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 7.62 180) (length 2.54)
        (name "OUT_A" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 7.62 180) (length 2.54) hide
        (name "OUT_A" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -20.32 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -20.32 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -15.24 180) (length 2.54)
        (name "BST_B" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 15.24 180) (length 2.54)
        (name "BST_A" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 12.7 0) (length 2.54)
        (name "INPUT_A" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 2.54)
        (name "INPUT_B" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 0 0) (length 2.54)
        (name "OC_ADJ" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -2.54 0) (length 2.54)
        (name "FREQ_ADJ" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 5.08 0) (length 2.54)
        (name "OSC_IOM" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TPA3251_2_1"
      (pin input line (at -12.7 12.7 0) (length 2.54)
        (name "INPUT_C" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 2.54)
        (name "INPUT_D" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -10.16 0) (length 2.54)
        (name "~RESET" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -12.7 -12.7 0) (length 2.54)
        (name "~FAULT" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -12.7 -15.24 0) (length 2.54)
        (name "~CLIP_OTW" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 20.32 270) (length 2.54)
        (name "GVDD_CD" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -15.24 180) (length 2.54)
        (name "BST_D" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 15.24 180) (length 2.54)
        (name "BST_C" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -7.62 180) (length 2.54)
        (name "OUT_D" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -7.62 180) (length 2.54) hide
        (name "OUT_D" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 20.32 270) (length 2.54)
        (name "PVDD_CD" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.54 0) (length 2.54)
        (name "M1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 20.32 270) (length 2.54) hide
        (name "PVDD_CD" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 20.32 270) (length 2.54) hide
        (name "PVDD_CD" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 7.62 180) (length 2.54)
        (name "OUT_C" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 2.54)
        (name "M2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:TPA6132A2RTE" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -7.62 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TPA6132A2RTE" (id 1) (at 8.89 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:WQFN-16-1EP_3x3mm_P0.5mm_EP1.6x1.6mm_ThermalVias" (id 2) (at 2.54 -13.97 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tpa6132a2.pdf" (id 3) (at -7.62 13.97 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "DirectPath audio amplifier Stereo" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "25mW, Stereo, DirectPath Audio Amplifier, WQFN-16" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "WQFN*1EP*3x3mm*P0.5mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPA6132A2RTE_0_1"
      (rectangle (start -10.16 12.7) (end 10.16 -12.7)
        (stroke (width 0.254)) (fill (type background))
      )
    )
    (symbol "TPA6132A2RTE_1_1"
      (pin input line (at -12.7 0 0) (length 2.54)
        (name "INL-" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -15.24 90) (length 2.54)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -5.08 180) (length 2.54)
        (name "CPP" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 15.24 270) (length 2.54)
        (name "HPVDD" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -10.16 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 15.24 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -15.24 90) (length 2.54)
        (name "SGND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 2.54 180) (length 2.54)
        (name "OUTL" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -15.24 90) (length 2.54)
        (name "EP" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 2.54)
        (name "INL+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 2.54)
        (name "INR+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 2.54)
        (name "INR-" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 7.62 180) (length 2.54)
        (name "OUTR" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 2.54)
        (name "G0" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -7.62 0) (length 2.54)
        (name "G1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -15.24 90) (length 2.54)
        (name "HPVSS" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -7.62 180) (length 2.54)
        (name "CPN" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Amplifier_Audio:MAX98357" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 1.27 13.97 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "MAX98357" (id 1) (at 1.27 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "Package_DFN_QFN:TQFN-16-1EP_3x3mm_P0.5mm_EP1.23x1.23mm_ThermalVias" (id 2) (at -39.37 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX98357A-MAX98357B.pdf" (id 3) (at -39.37 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "ki_description" "PCM Class D Amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX98357_0_0"
      (rectangle (start -10.16 10.16) (end 10.16 -10.16)
        (stroke (width 0.4064)) (fill (type background))
      )
      (pin input line (at -15.24 2.54 0) (length 5.08)
        (name "DIN" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 15.24 5.08 180) (length 5.08)
        (name "OUT-" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 0 -15.24 90) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin input clock (at -15.24 -2.54 0) (length 5.08)
        (name "LRCLK" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 0 -15.24 90) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin input clock (at -15.24 5.08 0) (length 5.08)
        (name "BCLK" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 15.24 -5.08 180) (length 5.08)
        (name "EP" (effects (font (size 1.016 1.016))))
        (number "17" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -15.24 0 0) (length 5.08)
        (name "GAIN" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 0 -15.24 90) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -15.24 -5.08 0) (length 5.08)
        (name "~{SHDN}" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 0 15.24 270) (length 5.08)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 0 15.24 270) (length 5.08)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 15.24 2.54 180) (length 5.08)
        (name "OUT+" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
