[2025-01-19 22:58:09] debug: 	z2m: Removing old log directory '/app/data/log/2024-12-21.00-35-12'
[2025-01-19 22:58:09] info: 	z2m: Logging to console, file (filename: log.log)
[2025-01-19 22:58:09] debug: 	z2m: Loaded state from file /app/data/state.json
[2025-01-19 22:58:09] info: 	z2m: Starting Zigbee2MQTT version 2.0.0 (commit #060ae99cff715cc9ef6a0cfa7cae0cdcb17f0c8a)
[2025-01-19 22:58:09] debug: 	z2m: sd-notify loaded
[2025-01-19 22:58:09] info: 	z2m: Starting zigbee-herdsman (3.2.1)
[2025-01-19 22:58:09] debug: 	z2m: Using zigbee-herdsman with settings: '"{\"network\":{\"panID\":6754,\"extendedPanID\":[221,221,221,221,221,221,221,221],\"channelList\":[11],\"networkKey\":\"HIDDEN\"},\"databasePath\":\"/app/data/database.db\",\"databaseBackupPath\":\"/app/data/database.db.backup\",\"backupPath\":\"/app/data/coordinator_backup.json\",\"serialPort\":{},\"adapter\":{\"disableLED\":false}}"'
[2025-01-19 22:58:10] debug: 	zh:adapter:discovery: Connected devices: [{"path":"/dev/ttyACM0","manufacturer":"dresden elektronik ingenieurtechnik GmbH","serialNumber":"DE2130316","pnpId":"usb-dresden_elektronik_ingenieurtechnik_GmbH_ConBee_II_DE2130316-if00","vendorId":"1cf1","productId":"0030"},{"path":"/dev/ttyS0"}]
[2025-01-19 22:58:10] info: 	zh:adapter:discovery: Matched adapter: {"path":"/dev/ttyACM0","manufacturer":"dresden elektronik ingenieurtechnik GmbH","serialNumber":"DE2130316","pnpId":"usb-dresden_elektronik_ingenieurtechnik_GmbH_ConBee_II_DE2130316-if00","vendorId":"1cf1","productId":"0030"} => deconz: path=/dev/ttyACM0, score=4
[2025-01-19 22:58:10] debug: 	zh:deconz:driver: Set delay to 0
[2025-01-19 22:58:10] debug: 	zh:controller: Starting with options '{"network":{"networkKeyDistribute":false,"networkKey":"HIDDEN","panID":6754,"extendedPanID":[221,221,221,221,221,221,221,221],"channelList":[11]},"serialPort":{"path":"/dev/ttyACM0","adapter":"deconz"},"adapter":{"disableLED":false},"databasePath":"/app/data/database.db","databaseBackupPath":"/app/data/database.db.backup","backupPath":"/app/data/coordinator_backup.json"}'
[2025-01-19 22:58:10] debug: 	zh:deconz:driver: Opening with /dev/ttyACM0
[2025-01-19 22:58:10] debug: 	zh:deconz:driver: Serialport opened
[2025-01-19 22:58:10] debug: 	zh:deconz:driver: send read parameter request from queue. seqNr: 1 paramId: 5
[2025-01-19 22:58:10] debug: 	zh:deconz:frameparser: PANID: 1a62
[2025-01-19 22:58:10] debug: 	zh:deconz:driver: send read parameter request from queue. seqNr: 2 paramId: 11
[2025-01-19 22:58:10] debug: 	zh:deconz:frameparser: APS_EXT_PANID: 0xdddddddddddddddd
[2025-01-19 22:58:10] debug: 	zh:deconz:driver: send read parameter request from queue. seqNr: 3 paramId: 28
[2025-01-19 22:58:10] debug: 	zh:deconz:frameparser: CHANNEL: 11
[2025-01-19 22:58:10] debug: 	zh:deconz:driver: send read parameter request from queue. seqNr: 4 paramId: 24
[2025-01-19 22:58:10] debug: 	zh:deconz:frameparser: NETWORK_KEY: hidden
[2025-01-19 22:58:10] debug: 	zh:deconz:driver: send write parameter request from queue. seqNr: 5 paramId: 19 param: 5,2,5,0,0,32,0,1,4,5,1,0,25,0,10,6,0,0,0,5,1,0,5,1,4,1,0
[2025-01-19 22:58:10] debug: 	zh:deconz:frameparser: write parameter response - parameter id: 19 - status: 0
[2025-01-19 22:58:10] debug: 	zh:controller: Started with result 'resumed'
[2025-01-19 22:58:10] debug: 	zh:deconz:driver: send read parameter request from queue. seqNr: 6 paramId: 5
[2025-01-19 22:58:10] debug: 	zh:deconz:frameparser: PANID: 1a62
[2025-01-19 22:58:10] debug: 	zh:deconz:driver: send read parameter request from queue. seqNr: 7 paramId: 11
[2025-01-19 22:58:10] debug: 	zh:deconz:frameparser: APS_EXT_PANID: 0xdddddddddddddddd
[2025-01-19 22:58:10] debug: 	zh:deconz:driver: send read parameter request from queue. seqNr: 8 paramId: 28
[2025-01-19 22:58:10] debug: 	zh:deconz:frameparser: CHANNEL: 11
[2025-01-19 22:58:10] debug: 	zh:controller: Injected database: true, adapter: true
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0x00212effff04fc2c): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0x000d6f00109eb214): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0xf0d1b800001ffcf2): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0xa4c138570b1956d9): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0xa4c1383ec7aa7d95): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0xa4c1383db5531833): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0x00212effff0cb8b6): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0x0ceff6fffebf4739): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0xa4c138541ec8ddd2): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0xa4c1384187f0960d): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0x001788010d1c884e): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0x001788010e8a8be7): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0x00158d00053a1aab): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0x00158d00053c6311): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0xa4c13864e6c8c400): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0xa4c138ef60e2fdbe): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0xf0d1b800001388f0): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0x7cb03eaa0a0176bd): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0x000d6f001417c142): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0xa4c138e68023f4c6): default expiration timeout set to 1740000
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0xa4c13838ba59a1b2): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:device: Request Queue (0xa4c1389d42e94844): default expiration timeout set to 0
[2025-01-19 22:58:10] debug: 	zh:controller:database: Writing database to '/app/data/database.db'
[2025-01-19 22:58:10] debug: 	zh:deconz:driver: send read parameter request from queue. seqNr: 9 paramId: 1
[2025-01-19 22:58:10] debug: 	zh:deconz:frameparser: MAC: 0x00212effff04fc2c
[2025-01-19 22:58:10] info: 	z2m: zigbee-herdsman started (resumed)
[2025-01-19 22:58:10] debug: 	zh:deconz:driver: send read firmware version request from queue. seqNr: 10
[2025-01-19 22:58:10] debug: 	zh:deconz:frameparser: read firmware version response - version: 0,7,88,38
[2025-01-19 22:58:10] info: 	z2m: Coordinator firmware version: '{"meta":{"maintrel":0,"majorrel":38,"minorrel":88,"product":0,"revision":"0x26580700","transportrev":0},"type":"ConBee2/RaspBee2"}'
[2025-01-19 22:58:10] debug: 	z2m: Zigbee network parameters: {"channel":11,"extendedPanID":"0xdddddddddddddddd","panID":6754}
[2025-01-19 22:58:10] info: 	z2m: Fernbedienung (0x000d6f00109eb214): AC0251100NJ/AC0251600NJ/AC0251700NJ - OSRAM Smart+ switch mini (EndDevice)
[2025-01-19 22:58:10] info: 	z2m: Bogenlampe (0xf0d1b800001ffcf2): 4058075208391 - LEDVANCE SMART+ lamp E27 RGBW (Router)
[2025-01-19 22:58:10] info: 	z2m: 0xa4c138570b1956d9 (0xa4c138570b1956d9): RSH-HS06_1 - Tuya Temperature & humidity sensor (EndDevice)
[2025-01-19 22:58:10] info: 	z2m: 0xa4c1383ec7aa7d95 (0xa4c1383ec7aa7d95): RSH-HS06_1 - Tuya Temperature & humidity sensor (EndDevice)
[2025-01-19 22:58:10] info: 	z2m: 0xa4c1383db5531833 (0xa4c1383db5531833): TS0201 - Tuya Temperature & humidity sensor with display (EndDevice)
[2025-01-19 22:58:10] info: 	z2m: Lichtschlauch (0x00212effff0cb8b6): Not supported (Router)
[2025-01-19 22:58:10] info: 	z2m: 0x0ceff6fffebf4739 (0x0ceff6fffebf4739): TS0207_repeater - Tuya Repeater (Router)
[2025-01-19 22:58:10] info: 	z2m: Flur (0xa4c138541ec8ddd2): 33951/33948 - AwoX LED white (Router)
[2025-01-19 22:58:10] info: 	z2m: Wasser Sensor Spüle (0xa4c1384187f0960d): IH-K665 - Aubess Water leak sensor (EndDevice)
[2025-01-19 22:58:10] info: 	z2m: Badlampe (0x001788010d1c884e): 915005997601 - Philips Hue Devere M white ambiance white & dimmer (Router)
[2025-01-19 22:58:10] info: 	z2m: Fernbedienung Bad (0x001788010e8a8be7): 929002398602 - Philips Hue dimmer switch (EndDevice)
[2025-01-19 22:58:10] info: 	z2m: 0x00158d00053a1aab (0x00158d00053a1aab): 50064 - Paulmann SmartHome led spot (Router)
[2025-01-19 22:58:10] info: 	z2m: 0x00158d00053c6311 (0x00158d00053c6311): 50064 - Paulmann SmartHome led spot (Router)
[2025-01-19 22:58:10] info: 	z2m: Bewegungsmelder 1 (0xa4c13864e6c8c400): 809WZT - Tuya Motion sensor (EndDevice)
[2025-01-19 22:58:10] info: 	z2m: Sensor Terassentür (0xa4c138ef60e2fdbe): TS0203 - Tuya Door sensor (EndDevice)
[2025-01-19 22:58:10] info: 	z2m: Flurlicht (0xf0d1b800001388f0): AC08562 - OSRAM SMART+ Candle E14 Dimmable White (Router)
[2025-01-19 22:58:10] info: 	z2m: Küchentisch (0x7cb03eaa0a0176bd): AC03641 - OSRAM LIGHTIFY LED Classic A60 clear (Router)
[2025-01-19 22:58:10] info: 	z2m: Fernbedienung 2 (0x000d6f001417c142): AC0251100NJ/AC0251600NJ/AC0251700NJ - OSRAM Smart+ switch mini (EndDevice)
[2025-01-19 22:58:10] info: 	z2m: Wassersensor Keller (0xa4c138e68023f4c6): SNZB-05 - eWeLink Zigbee water sensor (EndDevice)
[2025-01-19 22:58:10] info: 	z2m: Medienschrank Wohnzimmer (0xa4c13838ba59a1b2): ZG-227Z - Tuya Temperature and humidity sensor (EndDevice)
[2025-01-19 22:58:10] info: 	z2m: Temperatur Keller (0xa4c1389d42e94844): ZG-227Z - Tuya Temperature and humidity sensor (EndDevice)
[2025-01-19 22:58:10] info: 	z2m: Currently 21 devices are joined.
[2025-01-19 22:58:10] info: 	z2m: Connecting to MQTT server at mqtt://mqtt:1883
[2025-01-19 22:58:10] debug: 	z2m: Using MQTT anonymous login
[2025-01-19 22:58:11] info: 	z2m: Connected to MQTT server
[2025-01-19 22:58:11] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/state', payload '{"state":"online"}'
[2025-01-19 22:58:11] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/bridge/info' with data '{"commit":"060ae99cff715cc9ef6a0cfa7cae0cdcb17f0c8a","config":{"advanced":{"cache_state":true,"cache_state_persistent":true,"cache_state_send_on_startup":true,"channel":11,"elapsed":false,"ext_pan_id":[221,221,221,221,221,221,221,221],"last_seen":"disable","log_debug_namespace_ignore":"","log_debug_to_mqtt_frontend":false,"log_directory":"/app/data/log/%TIMESTAMP%","log_file":"log.log","log_level":"debug","log_namespaced_levels":{},"log_output":["console","file"],"log_rotation":true,"log_symlink_current":false,"log_syslog":{},"output":"json","pan_id":6754,"timestamp_format":"YYYY-MM-DD HH:mm:ss"},"availability":{"active":{"timeout":10},"enabled":false,"passive":{"timeout":1500}},"blocklist":[],"device_options":{},"devices":{"0x000d6f00109eb214":{"friendly_name":"Fernbedienung"},"0x000d6f001417c142":{"friendly_name":"Fernbedienung 2"},"0x00158d00053a1aab":{"friendly_name":"0x00158d00053a1aab"},"0x00158d00053c6311":{"friendly_name":"0x00158d00053c6311"},"0x001788010d1c884e":{"friendly_name":"Badlampe"},"0x001788010e8a8be7":{"friendly_name":"Fernbedienung Bad"},"0x00212effff0cb8b6":{"friendly_name":"Lichtschlauch"},"0x0ceff6fffebf4739":{"friendly_name":"0x0ceff6fffebf4739"},"0x7cb03eaa0a0176bd":{"friendly_name":"Küchentisch"},"0xa4c13838ba59a1b2":{"friendly_name":"Medienschrank Wohnzimmer"},"0xa4c1383db5531833":{"friendly_name":"0xa4c1383db5531833"},"0xa4c1383ec7aa7d95":{"friendly_name":"0xa4c1383ec7aa7d95"},"0xa4c1384187f0960d":{"friendly_name":"Wasser Sensor Spüle"},"0xa4c138541ec8ddd2":{"friendly_name":"Flur"},"0xa4c138570b1956d9":{"friendly_name":"0xa4c138570b1956d9"},"0xa4c13864e6c8c400":{"friendly_name":"Bewegungsmelder 1"},"0xa4c1389d42e94844":{"friendly_name":"Temperatur Keller"},"0xa4c138e68023f4c6":{"friendly_name":"Wassersensor Keller"},"0xa4c138ef60e2fdbe":{"friendly_name":"Sensor Terassentür"},"0xf0d1b800001388f0":{"friendly_name":"Flurlicht"},"0xf0d1b800001ffcf2":{"friendly_name":"Bogenlampe"}},"frontend":{"base_url":"/","enabled":true,"port":8080},"groups":{},"homeassistant":{"discovery_topic":"homeassistant","enabled":true,"experimental_event_entities":false,"legacy_action_sensor":false,"status_topic":"homeassistant/status"},"map_options":{"graphviz":{"colors":{"fill":{"coordinator":"#e04e5d","enddevice":"#fff8ce","router":"#4ea3e0"},"font":{"coordinator":"#ffffff","enddevice":"#000000","router":"#ffffff"},"line":{"active":"#009900","inactive":"#994444"}}}},"mqtt":{"base_topic":"zigbee2mqtt","force_disable_retain":false,"include_device_information":false,"maximum_packet_size":1048576,"serial":{"port":"/dev/ttyACM0"},"server":"mqtt://mqtt:1883"},"ota":{"default_maximum_data_size":50,"disable_automatic_update_check":false,"image_block_response_delay":250,"update_check_interval":1440},"passlist":[],"serial":{"disable_led":false},"version":4},"config_schema":{"definitions":{"device":{"properties":{"debounce":{"description":"Debounces messages of this device","title":"Debounce","type":"number"},"debounce_ignore":{"description":"Protects unique payload values of specified payload properties from overriding within debounce time","examples":["action"],"items":{"type":"string"},"title":"Ignore debounce","type":"array"},"disabled":{"description":"Disables the device (excludes device from network scans, availability and group state updates)","requiresRestart":true,"title":"Disabled","type":"boolean"},"filtered_attributes":{"description":"Filter attributes with regex from published payload.","examples":["^temperature$","^battery$","^action$"],"items":{"type":"string"},"title":"Filtered publish attributes","type":"array"},"filtered_cache":{"description":"Filter attributes with regex from being added to the cache, this prevents the attribute from being in the published payload when the value didn't change.","examples":["^input_actions$"],"items":{"type":"string"},"title":"Filtered attributes from cache","type":"array"},"filtered_optimistic":{"description":"Filter attributes with regex from optimistic publish payload when calling /set. (This has no effect if optimistic is set to false).","examples":["^color_(mode|temp)$","color"],"items":{"type":"string"},"title":"Filtered optimistic attributes","type":"array"},"friendly_name":{"description":"Used in the MQTT topic of a device. By default this is the device ID","readOnly":true,"title":"Friendly name","type":"string"},"homeassistant":{"properties":{"name":{"description":"Name of the device in Home Assistant","title":"Home Assistant name","type":"string"}},"title":"Home Assistant","type":["object","null"]},"icon":{"description":"The user-defined device icon for the frontend. It can be a full URL link to an image (e.g. https://SOME.SITE/MODEL123.jpg) or a path to a local file inside the `device_icons` directory.","title":"Icon","type":"string"},"optimistic":{"default":true,"description":"Publish optimistic state after set","title":"Optimistic","type":"boolean"},"qos":{"description":"QoS level for MQTT messages of this device","title":"QoS","type":"number"},"retain":{"description":"Retain MQTT messages of this device","title":"Retain","type":"boolean"},"retention":{"description":"Sets the MQTT Message Expiry in seconds, Make sure to set mqtt.version to 5","title":"Retention","type":"number"}},"required":["friendly_name"],"type":"object"},"group":{"properties":{"filtered_attributes":{"items":{"type":"string"},"type":"array"},"friendly_name":{"type":"string"},"off_state":{"default":"auto","description":"Control when to publish state OFF or CLOSE for a group. 'all_members_off': only publish state OFF/CLOSE when all group members are in state OFF/CLOSE,  'last_member_state': publish state OFF whenever one of its members changes to OFF","enum":["all_members_off","last_member_state"],"requiresRestart":true,"title":"Group off state","type":["string"]},"optimistic":{"type":"boolean"},"qos":{"type":"number"},"retain":{"type":"boolean"}},"required":["friendly_name"],"type":"object"}},"properties":{"advanced":{"properties":{"adapter_concurrent":{"description":"Adapter concurrency (e.g. 2 for CC2531 or 16 for CC26X2R1) (default: null, uses recommended value)","maximum":64,"minimum":1,"requiresRestart":true,"title":"Adapter concurrency","type":["number","null"]},"adapter_delay":{"description":"Adapter delay","maximum":1000,"minimum":0,"requiresRestart":true,"title":"Adapter delay","type":["number","null"]},"cache_state":{"default":true,"description":"MQTT message payload will contain all attributes, not only changed ones. Has to be true when integrating via Home Assistant","title":"Cache state","type":"boolean"},"cache_state_persistent":{"default":true,"description":"Persist cached state, only used when cache_state: true","title":"Persist cache state","type":"boolean"},"cache_state_send_on_startup":{"default":true,"description":"Send cached state on startup, only used when cache_state: true","title":"Send cached state on startup","type":"boolean"},"channel":{"default":11,"description":"Zigbee channel, changing might require re-pairing some devices! (Note: use a ZLL channel: 11, 15, 20, or 25 to avoid problems)","examples":[15,20,25],"maximum":26,"minimum":11,"requiresRestart":true,"title":"ZigBee channel","type":"number"},"elapsed":{"default":false,"description":"Add an elapsed attribute to MQTT messages, contains milliseconds since the previous msg","title":"Elapsed","type":"boolean"},"ext_pan_id":{"description":"Zigbee extended pan ID, changing requires re-pairing all devices!","oneOf":[{"title":"Extended pan ID (string)","type":"string"},{"items":{"type":"number"},"title":"Extended pan ID (array)","type":"array"}],"requiresRestart":true,"title":"Ext Pan ID"},"last_seen":{"default":"disable","description":"Add a last_seen attribute to MQTT messages, contains date/time of last Zigbee message","enum":["disable","ISO_8601","ISO_8601_local","epoch"],"title":"Last seen","type":"string"},"log_debug_namespace_ignore":{"default":"","description":"Do not log these namespaces (regex-based) for debug level","examples":["^zhc:legacy:fz:(tuya|moes)","^zhc:legacy:fz:(tuya|moes)|^zh:ember:uart:|^zh:controller"],"title":"Log debug namespace ignore","type":"string"},"log_debug_to_mqtt_frontend":{"default":false,"description":"Log debug level to MQTT and frontend (may decrease overall performance)","requiresRestart":true,"title":"Log debug to MQTT and frontend","type":"boolean"},"log_directory":{"description":"Location of log directory","examples":["data/log/%TIMESTAMP%"],"requiresRestart":true,"title":"Log directory","type":"string"},"log_file":{"default":"log.txt","description":"Log file name, can also contain timestamp","examples":["zigbee2mqtt_%TIMESTAMP%.log"],"requiresRestart":true,"title":"Log file","type":"string"},"log_level":{"default":"info","description":"Logging level","enum":["error","warning","info","debug","warn"],"title":"Log level","type":"string"},"log_namespaced_levels":{"additionalProperties":{"enum":["error","warning","info","debug"],"type":"string"},"default":{},"description":"Set individual log levels for certain namespaces","examples":[{"z2m:mqtt":"warning"},{"zh:ember:uart:ash":"info"}],"propertyNames":{"pattern":"^(z2m|zhc|zh)(:[a-z0-9]{1,})*$"},"title":"Log Namespaced Levels","type":"object"},"log_output":{"description":"Output location of the log, leave empty to suppress logging","items":{"enum":["console","file","syslog"],"type":"string"},"requiresRestart":true,"title":"Log output","type":"array"},"log_rotation":{"default":true,"description":"Log rotation","requiresRestart":true,"title":"Log rotation","type":"boolean"},"log_symlink_current":{"default":false,"description":"Create symlink to current logs in the log directory","requiresRestart":true,"title":"Log symlink current","type":"boolean"},"log_syslog":{"oneOf":[{"title":"syslog (disabled)","type":"null"},{"properties":{"app_name":{"default":"Zigbee2MQTT","description":"The name of the application (Default: Zigbee2MQTT).","title":"Localhost","type":"string"},"eol":{"default":"/n","description":"The end of line character to be added to the end of the message (Default: Message without modifications).","title":"eol","type":"string"},"host":{"default":"localhost","description":"The host running syslogd, defaults to localhost.","title":"Host","type":"string"},"localhost":{"default":"localhost","description":"Host to indicate that log messages are coming from (Default: localhost).","title":"Localhost","type":"string"},"path":{"default":"/dev/log","description":"The path to the syslog dgram socket (i.e. /dev/log or /var/run/syslog for OS X).","examples":["/var/run/syslog"],"title":"Path","type":"string"},"pid":{"default":"process.pid","description":"PID of the process that log messages are coming from (Default process.pid).","title":"PID","type":"string"},"port":{"default":514,"description":"The port on the host that syslog is running on, defaults to syslogd's default port.","title":"Port","type":"number"},"protocol":{"default":"udp4","description":"The network protocol to log over (e.g. tcp4, udp4, tls4, unix, unix-connect, etc).","examples":["udp4","tls4","unix","unix-connect"],"title":"Protocol","type":"string"},"type":{"default":"5424","description":"The type of the syslog protocol to use (Default: BSD, also valid: 5424).","title":"Type","type":"string"}},"title":"syslog (enabled)","type":"object"}],"requiresRestart":true},"network_key":{"description":"Network encryption key, changing requires re-pairing all devices!","oneOf":[{"title":"Network key(string)","type":"string"},{"items":{"type":"number"},"title":"Network key(array)","type":"array"}],"requiresRestart":true,"title":"Network key"},"output":{"description":"Examples when 'state' of a device is published json: topic: 'zigbee2mqtt/my_bulb' payload '{\"state\": \"ON\"}' attribute: topic 'zigbee2mqtt/my_bulb/state' payload 'ON' attribute_and_json: both json and attribute (see above)","enum":["attribute_and_json","attribute","json"],"title":"MQTT output type","type":"string"},"pan_id":{"description":"ZigBee pan ID, changing requires re-pairing all devices!","oneOf":[{"title":"Pan ID (string)","type":"string"},{"title":"Pan ID (number)","type":"number"}],"requiresRestart":true,"title":"Pan ID"},"timestamp_format":{"description":"Log timestamp format","examples":["YYYY-MM-DD HH:mm:ss"],"requiresRestart":true,"title":"Timestamp format","type":"string"},"transmit_power":{"description":"Transmit power of adapter, only available for Z-Stack (CC253*/CC2652/CC1352) adapters, CC2652 = 5dbm, CC1352 max is = 20dbm (5dbm default)","maximum":127,"minimum":-128,"requiresRestart":true,"title":"Transmit power","type":["number","null"]}},"title":"Advanced","type":"object"},"availability":{"description":"Checks whether devices are online/offline","properties":{"active":{"description":"Options for active devices (routers/mains powered)","properties":{"timeout":{"default":10,"description":"Time after which an active device will be marked as offline in minutes","requiresRestart":true,"title":"Timeout","type":"number"}},"required":["timeout"],"requiresRestart":true,"title":"Active","type":"object"},"enabled":{"default":false,"description":"Enable availability checks","requiresRestart":true,"title":"Enabled","type":"boolean"},"passive":{"description":"Options for passive devices (mostly battery powered)","properties":{"timeout":{"default":1500,"description":"Time after which an passive device will be marked as offline in minutes","requiresRestart":true,"title":"Timeout","type":"number"}},"required":["timeout"],"requiresRestart":true,"title":"Passive","type":"object"}},"required":[],"title":"Availability","type":"object"},"blocklist":{"description":"Block devices from the network (by ieeeAddr)","items":{"type":"string"},"requiresRestart":true,"title":"Blocklist","type":"array"},"device_options":{"title":"Options that are applied to all devices","type":"object"},"devices":{"patternProperties":{"^.*$":{"$ref":"#/definitions/device"}},"propertyNames":{"pattern":"^0x[\\d\\w]{16}$"},"type":"object"},"frontend":{"properties":{"auth_token":{"description":"Enables authentication, disabled by default","requiresRestart":true,"title":"Auth token","type":["string","null"]},"base_url":{"default":"/","description":"Base URL for the frontend. If hosted under a subpath, e.g. 'http://localhost:8080/z2m', set this to '/z2m'","pattern":"^\\/.*","requiresRestart":true,"title":"Base URL","type":"string"},"enabled":{"default":false,"description":"Enable frontend","requiresRestart":true,"title":"Enabled","type":"boolean"},"host":{"description":"Frontend binding host. Binds to a unix socket when an absolute path is given instead.","examples":["127.0.0.1","::1","/run/zigbee2mqtt/zigbee2mqtt.sock"],"requiresRestart":true,"title":"Bind host","type":["string","null"]},"port":{"default":8080,"description":"Frontend binding port. Ignored when using a unix domain socket","requiresRestart":true,"title":"Port","type":"number"},"ssl_cert":{"description":"SSL Certificate file path for exposing HTTPS. The sibling property 'ssl_key' must be set for HTTPS to be activated.","requiresRestart":true,"title":"Certificate file path","type":["string","null"]},"ssl_key":{"description":"SSL key file path for exposing HTTPS. The sibling property 'ssl_cert' must be set for HTTPS to be activated.","requiresRestart":true,"title":"key file path","type":["string","null"]},"url":{"description":"URL on which the frontend can be reached, currently only used for the Home Assistant device configuration page","requiresRestart":true,"title":"URL","type":["string","null"]}},"required":[],"title":"Frontend","type":"object"},"groups":{"patternProperties":{"^.*$":{"$ref":"#/definitions/group"}},"propertyNames":{"pattern":"^[\\w].*$"},"type":"object"},"homeassistant":{"description":"Home Assistant integration (MQTT discovery)","properties":{"discovery_topic":{"default":"homeassistant","description":"Home Assistant discovery topic","examples":["homeassistant"],"requiresRestart":true,"title":"Homeassistant discovery topic","type":"string"},"enabled":{"default":false,"description":"Enable Home Assistant integration","requiresRestart":true,"title":"Enabled","type":"boolean"},"experimental_event_entities":{"default":false,"description":"Home Assistant experimental event entities, when enabled Zigbee2MQTT will add event entities for exposed actions. The events and attributes are currently deemed experimental and subject to change.","title":"Home Assistant experimental event entities","type":"boolean"},"legacy_action_sensor":{"default":false,"description":"Home Assistant legacy actions sensor, when enabled a action sensor will be discoverd and an empty `action` will be send after every published action.","title":"Home Assistant legacy action sensors","type":"boolean"},"status_topic":{"default":"homeassistant/status","description":"Home Assistant status topic","examples":["homeassistant/status"],"requiresRestart":true,"title":"Home Assistant status topic","type":"string"}},"required":[],"title":"Home Assistant integration","type":"object"},"map_options":{"properties":{"graphviz":{"properties":{"colors":{"properties":{"fill":{"properties":{"coordinator":{"type":"string"},"enddevice":{"type":"string"},"router":{"type":"string"}},"type":"object"},"font":{"properties":{"coordinator":{"type":"string"},"enddevice":{"type":"string"},"router":{"type":"string"}},"type":"object"},"line":{"properties":{"active":{"type":"string"},"inactive":{"type":"string"}},"type":"object"}},"type":"object"}},"type":"object"}},"title":"Networkmap","type":"object"},"mqtt":{"properties":{"base_topic":{"default":"zigbee2mqtt","description":"MQTT base topic for Zigbee2MQTT MQTT messages","examples":["zigbee2mqtt"],"requiresRestart":true,"title":"Base topic","type":"string"},"ca":{"description":"Absolute path to SSL/TLS certificate of CA used to sign server and client certificates","examples":["/etc/ssl/mqtt-ca.crt"],"requiresRestart":true,"title":"Certificate authority","type":"string"},"cert":{"description":"Absolute path to SSL/TLS certificate for client-authentication","examples":["/etc/ssl/mqtt-client.crt"],"requiresRestart":true,"title":"SSL/TLS certificate","type":"string"},"client_id":{"description":"MQTT client ID","examples":["MY_CLIENT_ID"],"requiresRestart":true,"title":"Client ID","type":"string"},"force_disable_retain":{"default":false,"description":"Disable retain for all send messages. ONLY enable if your MQTT broker doesn't support retained message (e.g. AWS IoT core, Azure IoT Hub, Google Cloud IoT core, IBM Watson IoT Platform). Enabling will break the Home Assistant integration","requiresRestart":true,"title":"Force disable retain","type":"boolean"},"include_device_information":{"default":false,"description":"Include device information to mqtt messages","title":"Include device information","type":"boolean"},"keepalive":{"default":60,"description":"MQTT keepalive in second","requiresRestart":true,"title":"Keepalive","type":"number"},"key":{"description":"Absolute path to SSL/TLS key for client-authentication","examples":["/etc/ssl/mqtt-client.key"],"requiresRestart":true,"title":"SSL/TLS key","type":"string"},"maximum_packet_size":{"default":1048576,"description":"Specifies the maximum allowed packet length (in bytes) that the server can send to Zigbee2MQTT. NOTE: The same value exists in your MQTT broker but for the length the client can send to it instead.","maximum":268435456,"minimum":20,"requiresRestart":true,"title":"Maximum packet size","type":"number"},"password":{"description":"MQTT server authentication password","examples":["ILOVEPELMENI"],"requiresRestart":true,"title":"Password","type":"string"},"reject_unauthorized":{"default":true,"description":"Disable self-signed SSL certificate","requiresRestart":true,"title":"Reject unauthorized","type":"boolean"},"server":{"description":"MQTT server URL (use mqtts:// for SSL/TLS connection)","examples":["mqtt://localhost:1883"],"requiresRestart":true,"title":"MQTT server","type":"string"},"user":{"description":"MQTT server authentication user","examples":["johnnysilverhand"],"requiresRestart":true,"title":"User","type":"string"},"version":{"default":4,"description":"MQTT protocol version","examples":[5],"requiresRestart":true,"title":"Version","type":["number","null"]}},"required":["server"],"title":"MQTT","type":"object"},"ota":{"properties":{"default_maximum_data_size":{"default":50,"description":"The size of file chunks sent during an update (in bytes). Note: This value may get ignored for manufacturers that require specific values.","maximum":100,"minimum":10,"requiresRestart":true,"title":"Default maximum data size","type":"number"},"disable_automatic_update_check":{"default":false,"description":"Zigbee devices may request a firmware update, and do so frequently, causing Zigbee2MQTT to reach out to third party servers. If you disable these device initiated checks, you can still initiate a firmware update check manually.","title":"Disable automatic update check","type":"boolean"},"image_block_response_delay":{"default":250,"description":"Limits the rate of requests (in milliseconds) during OTA updates to reduce network congestion. You can increase this value if your network appears unstable during OTA.","minimum":50,"requiresRestart":true,"title":"Image block response delay","type":"number"},"update_check_interval":{"default":1440,"description":"Your device may request a check for a new firmware update. This value determines how frequently third party servers may actually be contacted to look for firmware updates. The value is set in minutes, and the default is 1 day.","title":"Update check interval","type":"number"},"zigbee_ota_override_index_location":{"description":"Location of override OTA index file","examples":["index.json"],"requiresRestart":true,"title":"OTA index override file name","type":["string","null"]}},"title":"OTA updates","type":"object"},"passlist":{"description":"Allow only certain devices to join the network (by ieeeAddr). Note that all devices not on the passlist will be removed from the network!","items":{"type":"string"},"requiresRestart":true,"title":"Passlist","type":"array"},"serial":{"properties":{"adapter":{"default":"auto","description":"Adapter type, not needed unless you are experiencing problems","enum":["deconz","zstack","zigate","ezsp","auto","ember","zboss"],"requiresRestart":true,"title":"Adapter","type":["string"]},"baudrate":{"description":"Baud rate speed for serial port, this can be anything firmware support but default is 115200 for Z-Stack and EZSP, 38400 for Deconz, however note that some EZSP firmware need 57600","examples":[38400,57600,115200],"requiresRestart":true,"title":"Baudrate","type":"number"},"disable_led":{"default":false,"description":"Disable LED of the adapter if supported","requiresRestart":true,"title":"Disable led","type":"boolean"},"port":{"description":"Location of the adapter. To autodetect the port, set null","examples":["/dev/ttyACM0"],"requiresRestart":true,"title":"Port","type":["string","null"]},"rtscts":{"description":"RTS / CTS Hardware Flow Control for serial port","requiresRestart":true,"title":"RTS / CTS","type":"boolean"}},"title":"Serial","type":"object"}},"required":["mqtt"],"type":"object"},"coordinator":{"ieee_address":"0x00212effff04fc2c","meta":{"maintrel":0,"majorrel":38,"minorrel":88,"product":0,"revision":"0x26580700","transportrev":0},"type":"ConBee2/RaspBee2"},"log_level":"debug","network":{"channel":11,"extended_pan_id":"0xdddddddddddddddd","pan_id":6754},"permit_join":false,"restart_required":false,"version":"2.0.0","zigbee_herdsman":{"version":"3.2.1"},"zigbee_herdsman_converters":{"version":"21.12.0"}}'
[2025-01-19 22:58:11] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/bridge/devices' with data '[{"disabled":false,"endpoints":{"1":{"bindings":[],"clusters":{"input":["genBasic","genOnOff","genTime","genOta","ssIasAce"],"output":["genPowerCfg","genPollCtrl","ssIasZone","ssIasWd"]},"configured_reportings":[],"scenes":[]},"242":{"bindings":[],"clusters":{"input":[],"output":["greenPower"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"Coordinator","ieee_address":"0x00212effff04fc2c","interview_completed":true,"interviewing":false,"network_address":0,"supported":true,"type":"Coordinator"},{"date_code":"201801031853590","definition":{"description":"Smart+ switch mini","exposes":[{"access":1,"category":"diagnostic","description":"Remaining battery in %, can take up to 24 hours before reported","label":"Battery","name":"battery","property":"battery","type":"numeric","unit":"%","value_max":100,"value_min":0},{"access":1,"category":"diagnostic","description":"Triggered action (e.g. a button click)","label":"Action","name":"action","property":"action","type":"enum","values":["on","brightness_move_up","brightness_move_down","brightness_stop","color_temperature_move","hue_move","hue_stop","move_to_saturation","off","brightness_move_to_level"]},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"AC0251100NJ/AC0251600NJ/AC0251700NJ","options":[{"access":2,"description":"Simulate a brightness value. If this device provides a brightness_move_up or brightness_move_down action it is possible to specify the update interval and delta. The action_brightness_delta indicates the delta for each interval.","features":[{"access":2,"description":"Delta per interval, 20 by default","label":"Delta","name":"delta","property":"delta","type":"numeric","value_min":0},{"access":2,"description":"Interval duration","label":"Interval","name":"interval","property":"interval","type":"numeric","unit":"ms","value_min":0}],"label":"Simulated brightness","name":"simulated_brightness","property":"simulated_brightness","type":"composite"}],"supports_ota":true,"vendor":"OSRAM"},"disabled":false,"endpoints":{"1":{"bindings":[{"cluster":"genPollCtrl","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genOnOff","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genLevelCtrl","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genPowerCfg","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}}],"clusters":{"input":["genBasic","genPowerCfg","genPollCtrl","touchlink","64768"],"output":["genIdentify","genGroups","genScenes","genOnOff","genLevelCtrl","genOta","lightingColorCtrl","touchlink"]},"configured_reportings":[{"attribute":"batteryVoltage","cluster":"genPowerCfg","maximum_report_interval":65000,"minimum_report_interval":3600,"reportable_change":0}],"scenes":[]},"2":{"bindings":[{"cluster":"genOnOff","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genLevelCtrl","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}}],"clusters":{"input":["genBasic","touchlink","64768"],"output":["genIdentify","genGroups","genScenes","genOnOff","genLevelCtrl","lightingColorCtrl","touchlink"]},"configured_reportings":[],"scenes":[]},"3":{"bindings":[{"cluster":"genLevelCtrl","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"lightingColorCtrl","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}}],"clusters":{"input":["genBasic","touchlink","64768"],"output":["genIdentify","genGroups","genScenes","genOnOff","genLevelCtrl","lightingColorCtrl","touchlink"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"Fernbedienung","ieee_address":"0x000d6f00109eb214","interview_completed":true,"interviewing":false,"manufacturer":"OSRAM","model_id":"Lightify Switch Mini","network_address":40099,"power_source":"Battery","software_build_id":"e.1.11.0M","supported":true,"type":"EndDevice"},{"date_code":"20240523","definition":{"description":"SMART+ lamp E27 RGBW","exposes":[{"features":[{"access":7,"description":"On/off state of this light","label":"State","name":"state","property":"state","type":"binary","value_off":"OFF","value_on":"ON","value_toggle":"TOGGLE"},{"access":7,"description":"Brightness of this light","label":"Brightness","name":"brightness","property":"brightness","type":"numeric","value_max":254,"value_min":0},{"access":7,"description":"Color temperature of this light","label":"Color temp","name":"color_temp","presets":[{"description":"Coolest temperature supported","name":"coolest","value":153},{"description":"Cool temperature (250 mireds / 4000 Kelvin)","name":"cool","value":250},{"description":"Neutral temperature (370 mireds / 2700 Kelvin)","name":"neutral","value":370},{"description":"Warmest temperature supported","name":"warmest","value":370}],"property":"color_temp","type":"numeric","unit":"mired","value_max":370,"value_min":153},{"access":7,"description":"Color of this light in the CIE 1931 color space (x/y)","features":[{"access":7,"label":"X","name":"x","property":"x","type":"numeric"},{"access":7,"label":"Y","name":"y","property":"y","type":"numeric"}],"label":"Color (X/Y)","name":"color_xy","property":"color","type":"composite"},{"access":7,"description":"Color of this light expressed as hue/saturation","features":[{"access":7,"label":"Hue","name":"hue","property":"hue","type":"numeric"},{"access":7,"label":"Saturation","name":"saturation","property":"saturation","type":"numeric"}],"label":"Color (HS)","name":"color_hs","property":"color","type":"composite"}],"type":"light"},{"access":2,"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)","label":"Effect","name":"effect","property":"effect","type":"enum","values":["blink","breathe","okay","channel_change","finish_effect","stop_effect","colorloop","stop_colorloop"]},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"4058075208391","options":[{"access":2,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition).","label":"Transition","name":"transition","property":"transition","type":"numeric","value_min":0},{"access":2,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true).","label":"Color sync","name":"color_sync","property":"color_sync","type":"binary","value_off":false,"value_on":true},{"access":2,"description":"State actions will also be published as 'action' when true (default false).","label":"State action","name":"state_action","property":"state_action","type":"binary","value_off":false,"value_on":true}],"supports_ota":true,"vendor":"LEDVANCE"},"disabled":false,"endpoints":{"1":{"bindings":[],"clusters":{"input":["genBasic","genIdentify","genGroups","genScenes","genOnOff","genLevelCtrl","lightingColorCtrl","haDiagnostic","touchlink"],"output":["genOta"]},"configured_reportings":[],"scenes":[]},"242":{"bindings":[],"clusters":{"input":[],"output":["greenPower"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2","interview_completed":true,"interviewing":false,"manufacturer":"LEDVANCE","model_id":"A60S RGBW","network_address":30689,"power_source":"Mains (single phase)","software_build_id":"03197310","supported":true,"type":"Router"},{"definition":{"description":"Temperature & humidity sensor","exposes":[{"access":1,"category":"diagnostic","description":"Remaining battery in %, can take up to 24 hours before reported","label":"Battery","name":"battery","property":"battery","type":"numeric","unit":"%","value_max":100,"value_min":0},{"access":1,"description":"Measured temperature value","label":"Temperature","name":"temperature","property":"temperature","type":"numeric","unit":"°C"},{"access":1,"description":"Measured relative humidity","label":"Humidity","name":"humidity","property":"humidity","type":"numeric","unit":"%"},{"access":1,"category":"diagnostic","description":"Voltage of the battery in millivolts","label":"Voltage","name":"voltage","property":"voltage","type":"numeric","unit":"mV"},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"RSH-HS06_1","options":[{"access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device.","label":"Temperature calibration","name":"temperature_calibration","property":"temperature_calibration","type":"numeric"},{"access":2,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device. This option can only decrease the precision, not increase it.","label":"Temperature precision","name":"temperature_precision","property":"temperature_precision","type":"numeric","value_max":3,"value_min":0},{"access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device.","label":"Humidity calibration","name":"humidity_calibration","property":"humidity_calibration","type":"numeric"},{"access":2,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device. This option can only decrease the precision, not increase it.","label":"Humidity precision","name":"humidity_precision","property":"humidity_precision","type":"numeric","value_max":3,"value_min":0}],"supports_ota":false,"vendor":"Tuya"},"disabled":false,"endpoints":{"1":{"bindings":[],"clusters":{"input":["genBasic","genPowerCfg","genIdentify","msTemperatureMeasurement","msRelativeHumidity"],"output":["genOta"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"0xa4c138570b1956d9","ieee_address":"0xa4c138570b1956d9","interview_completed":true,"interviewing":false,"manufacturer":"_TZ3000_zl1kmjqx","model_id":"","network_address":39357,"power_source":"Battery","supported":true,"type":"EndDevice"},{"definition":{"description":"Temperature & humidity sensor","exposes":[{"access":1,"category":"diagnostic","description":"Remaining battery in %, can take up to 24 hours before reported","label":"Battery","name":"battery","property":"battery","type":"numeric","unit":"%","value_max":100,"value_min":0},{"access":1,"description":"Measured temperature value","label":"Temperature","name":"temperature","property":"temperature","type":"numeric","unit":"°C"},{"access":1,"description":"Measured relative humidity","label":"Humidity","name":"humidity","property":"humidity","type":"numeric","unit":"%"},{"access":1,"category":"diagnostic","description":"Voltage of the battery in millivolts","label":"Voltage","name":"voltage","property":"voltage","type":"numeric","unit":"mV"},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"RSH-HS06_1","options":[{"access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device.","label":"Temperature calibration","name":"temperature_calibration","property":"temperature_calibration","type":"numeric"},{"access":2,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device. This option can only decrease the precision, not increase it.","label":"Temperature precision","name":"temperature_precision","property":"temperature_precision","type":"numeric","value_max":3,"value_min":0},{"access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device.","label":"Humidity calibration","name":"humidity_calibration","property":"humidity_calibration","type":"numeric"},{"access":2,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device. This option can only decrease the precision, not increase it.","label":"Humidity precision","name":"humidity_precision","property":"humidity_precision","type":"numeric","value_max":3,"value_min":0}],"supports_ota":false,"vendor":"Tuya"},"disabled":false,"endpoints":{"1":{"bindings":[],"clusters":{"input":["genBasic","genPowerCfg","genIdentify","msTemperatureMeasurement","msRelativeHumidity"],"output":["genOta"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"0xa4c1383ec7aa7d95","ieee_address":"0xa4c1383ec7aa7d95","interview_completed":true,"interviewing":false,"manufacturer":"_TZ3000_zl1kmjqx","model_id":"","network_address":38696,"power_source":"Battery","supported":true,"type":"EndDevice"},{"definition":{"description":"Temperature & humidity sensor with display","exposes":[{"access":1,"category":"diagnostic","description":"Remaining battery in %, can take up to 24 hours before reported","label":"Battery","name":"battery","property":"battery","type":"numeric","unit":"%","value_max":100,"value_min":0},{"access":1,"description":"Measured temperature value","label":"Temperature","name":"temperature","property":"temperature","type":"numeric","unit":"°C"},{"access":1,"description":"Measured relative humidity","label":"Humidity","name":"humidity","property":"humidity","type":"numeric","unit":"%"},{"access":1,"category":"diagnostic","description":"Voltage of the battery in millivolts","label":"Voltage","name":"voltage","property":"voltage","type":"numeric","unit":"mV"},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"TS0201","options":[{"access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device.","label":"Temperature calibration","name":"temperature_calibration","property":"temperature_calibration","type":"numeric"},{"access":2,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device. This option can only decrease the precision, not increase it.","label":"Temperature precision","name":"temperature_precision","property":"temperature_precision","type":"numeric","value_max":3,"value_min":0},{"access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device.","label":"Humidity calibration","name":"humidity_calibration","property":"humidity_calibration","type":"numeric"},{"access":2,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device. This option can only decrease the precision, not increase it.","label":"Humidity precision","name":"humidity_precision","property":"humidity_precision","type":"numeric","value_max":3,"value_min":0}],"supports_ota":true,"vendor":"Tuya"},"disabled":false,"endpoints":{"1":{"bindings":[],"clusters":{"input":["genBasic","genPowerCfg","genIdentify","msTemperatureMeasurement","msRelativeHumidity"],"output":["genOta"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"0xa4c1383db5531833","ieee_address":"0xa4c1383db5531833","interview_completed":true,"interviewing":false,"manufacturer":"_TZ3000_bjawzodf","model_id":"TY0201","network_address":19795,"power_source":"Battery","supported":true,"type":"EndDevice"},{"date_code":"20220617\u0000","definition":{"description":"Automatically generated definition","exposes":[{"features":[{"access":7,"description":"On/off state of this light","label":"State","name":"state","property":"state","type":"binary","value_off":"OFF","value_on":"ON","value_toggle":"TOGGLE"},{"access":7,"description":"Brightness of this light","label":"Brightness","name":"brightness","property":"brightness","type":"numeric","value_max":254,"value_min":0},{"access":7,"description":"Color temperature of this light","label":"Color temp","name":"color_temp","presets":[{"description":"Coolest temperature supported","name":"coolest","value":153},{"description":"Cool temperature (250 mireds / 4000 Kelvin)","name":"cool","value":250},{"description":"Neutral temperature (370 mireds / 2700 Kelvin)","name":"neutral","value":370},{"description":"Warm temperature (454 mireds / 2200 Kelvin)","name":"warm","value":454},{"description":"Warmest temperature supported","name":"warmest","value":500}],"property":"color_temp","type":"numeric","unit":"mired","value_max":500,"value_min":153},{"access":7,"description":"Color temperature after cold power on of this light","label":"Color temp startup","name":"color_temp_startup","presets":[{"description":"Coolest temperature supported","name":"coolest","value":153},{"description":"Cool temperature (250 mireds / 4000 Kelvin)","name":"cool","value":250},{"description":"Neutral temperature (370 mireds / 2700 Kelvin)","name":"neutral","value":370},{"description":"Warm temperature (454 mireds / 2200 Kelvin)","name":"warm","value":454},{"description":"Warmest temperature supported","name":"warmest","value":500},{"description":"Restore previous color_temp on cold power on","name":"previous","value":65535}],"property":"color_temp_startup","type":"numeric","unit":"mired","value_max":500,"value_min":153},{"access":7,"description":"Color of this light in the CIE 1931 color space (x/y)","features":[{"access":7,"label":"X","name":"x","property":"x","type":"numeric"},{"access":7,"label":"Y","name":"y","property":"y","type":"numeric"}],"label":"Color (X/Y)","name":"color_xy","property":"color","type":"composite"},{"access":7,"description":"Color of this light expressed as hue/saturation","features":[{"access":7,"label":"Hue","name":"hue","property":"hue","type":"numeric"},{"access":7,"label":"Saturation","name":"saturation","property":"saturation","type":"numeric"}],"label":"Color (HS)","name":"color_hs","property":"color","type":"composite"}],"type":"light"},{"access":2,"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)","label":"Effect","name":"effect","property":"effect","type":"enum","values":["blink","breathe","okay","channel_change","finish_effect","stop_effect","colorloop","stop_colorloop"]},{"access":7,"category":"config","description":"Controls the behavior when the device is powered on after power loss","label":"Power-on behavior","name":"power_on_behavior","property":"power_on_behavior","type":"enum","values":["off","on","toggle","previous"]},{"features":[{"access":7,"description":"On/off state of this light","label":"State","name":"state","property":"state","type":"binary","value_off":"OFF","value_on":"ON","value_toggle":"TOGGLE"},{"access":7,"description":"Brightness of this light","label":"Brightness","name":"brightness","property":"brightness","type":"numeric","value_max":254,"value_min":0}],"type":"light"},{"access":2,"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)","label":"Effect","name":"effect","property":"effect","type":"enum","values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"]},{"access":7,"category":"config","description":"Controls the behavior when the device is powered on after power loss","label":"Power-on behavior","name":"power_on_behavior","property":"power_on_behavior","type":"enum","values":["off","on","toggle","previous"]},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"FLS-PP3 White\u0000","options":[{"access":2,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition).","label":"Transition","name":"transition","property":"transition","type":"numeric","value_min":0},{"access":2,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true).","label":"Color sync","name":"color_sync","property":"color_sync","type":"binary","value_off":false,"value_on":true},{"access":2,"description":"State actions will also be published as 'action' when true (default false).","label":"State action","name":"state_action","property":"state_action","type":"binary","value_off":false,"value_on":true}],"supports_ota":false,"vendor":"dresden elektronik\u0000"},"disabled":false,"endpoints":{"10":{"bindings":[],"clusters":{"input":["genBasic","touchlink","genGroups","genIdentify","genScenes","genOnOff","genLevelCtrl","lightingColorCtrl","64718"],"output":["genOta"]},"configured_reportings":[],"scenes":[]},"11":{"bindings":[],"clusters":{"input":["genBasic","touchlink","genGroups","genIdentify","genScenes","genOnOff","genLevelCtrl"],"output":[]},"configured_reportings":[],"scenes":[]}},"friendly_name":"Lichtschlauch","ieee_address":"0x00212effff0cb8b6","interview_completed":true,"interviewing":false,"manufacturer":"dresden elektronik\u0000","model_id":"FLS-PP3 White\u0000","network_address":32127,"power_source":"Mains (single phase)","software_build_id":"0214.201000F6\u0000","supported":false,"type":"Router"},{"date_code":"","definition":{"description":"Repeater","exposes":[{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"TS0207_repeater","options":[],"supports_ota":false,"vendor":"Tuya"},"disabled":false,"endpoints":{"1":{"bindings":[],"clusters":{"input":["genBasic","genTime","genIdentify"],"output":["genOta"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"0x0ceff6fffebf4739","ieee_address":"0x0ceff6fffebf4739","interview_completed":true,"interviewing":false,"manufacturer":"_TZ3000_nkkl7uzv","model_id":"TS0207","network_address":58894,"power_source":"Mains (single phase)","supported":true,"type":"Router"},{"definition":{"description":"LED white","exposes":[{"features":[{"access":7,"description":"On/off state of this light","label":"State","name":"state","property":"state","type":"binary","value_off":"OFF","value_on":"ON","value_toggle":"TOGGLE"},{"access":7,"description":"Brightness of this light","label":"Brightness","name":"brightness","property":"brightness","type":"numeric","value_max":254,"value_min":0}],"type":"light"},{"access":2,"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)","label":"Effect","name":"effect","property":"effect","type":"enum","values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"]},{"access":7,"category":"config","description":"Controls the behavior when the device is powered on after power loss","label":"Power-on behavior","name":"power_on_behavior","property":"power_on_behavior","type":"enum","values":["off","on","toggle","previous"]},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"33951/33948","options":[{"access":2,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition).","label":"Transition","name":"transition","property":"transition","type":"numeric","value_min":0},{"access":2,"description":"State actions will also be published as 'action' when true (default false).","label":"State action","name":"state_action","property":"state_action","type":"binary","value_off":false,"value_on":true}],"supports_ota":false,"vendor":"AwoX"},"disabled":false,"endpoints":{"1":{"bindings":[],"clusters":{"input":["genBasic","genIdentify","genGroups","genScenes","genOnOff","genLevelCtrl","lightingColorCtrl","touchlink","manuSpecificAmazonWWAH"],"output":["genOnOff"]},"configured_reportings":[],"scenes":[]},"242":{"bindings":[],"clusters":{"input":[],"output":["greenPower"]},"configured_reportings":[],"scenes":[]},"3":{"bindings":[],"clusters":{"input":["65360","65361"],"output":["65360","65361"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"Flur","ieee_address":"0xa4c138541ec8ddd2","interview_completed":true,"interviewing":false,"manufacturer":"AwoX","model_id":"TLSR82xx","network_address":9855,"power_source":"Mains (single phase)","software_build_id":"0122052017","supported":true,"type":"Router"},{"definition":{"description":"Water leak sensor","exposes":[{"access":1,"description":"Indicates whether the device detected a water leak","label":"Water leak","name":"water_leak","property":"water_leak","type":"binary","value_off":false,"value_on":true},{"access":1,"category":"diagnostic","description":"Indicates if the battery of this device is almost empty","label":"Battery low","name":"battery_low","property":"battery_low","type":"binary","value_off":false,"value_on":true},{"access":1,"category":"diagnostic","description":"Remaining battery in %, can take up to 24 hours before reported","label":"Battery","name":"battery","property":"battery","type":"numeric","unit":"%","value_max":100,"value_min":0},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"IH-K665","options":[],"supports_ota":false,"vendor":"Aubess"},"disabled":false,"endpoints":{"1":{"bindings":[{"cluster":"genPowerCfg","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}}],"clusters":{"input":["genBasic","genIdentify","ssIasZone","genPowerCfg"],"output":["genTime"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"Wasser Sensor Spüle","ieee_address":"0xa4c1384187f0960d","interview_completed":true,"interviewing":false,"manufacturer":"_TZ3000_k4ej3ww2","model_id":"TS0207","network_address":15382,"power_source":"Battery","supported":true,"type":"EndDevice"},{"date_code":"20211210","definition":{"description":"Hue Devere M white ambiance white & dimmer","exposes":[{"features":[{"access":7,"description":"On/off state of this light","label":"State","name":"state","property":"state","type":"binary","value_off":"OFF","value_on":"ON","value_toggle":"TOGGLE"},{"access":7,"description":"Brightness of this light","label":"Brightness","name":"brightness","property":"brightness","type":"numeric","value_max":254,"value_min":0},{"access":7,"description":"Color temperature of this light","label":"Color temp","name":"color_temp","presets":[{"description":"Coolest temperature supported","name":"coolest","value":153},{"description":"Cool temperature (250 mireds / 4000 Kelvin)","name":"cool","value":250},{"description":"Neutral temperature (370 mireds / 2700 Kelvin)","name":"neutral","value":370},{"description":"Warm temperature (454 mireds / 2200 Kelvin)","name":"warm","value":454},{"description":"Warmest temperature supported","name":"warmest","value":454}],"property":"color_temp","type":"numeric","unit":"mired","value_max":454,"value_min":153},{"access":7,"description":"Color temperature after cold power on of this light","label":"Color temp startup","name":"color_temp_startup","presets":[{"description":"Coolest temperature supported","name":"coolest","value":153},{"description":"Cool temperature (250 mireds / 4000 Kelvin)","name":"cool","value":250},{"description":"Neutral temperature (370 mireds / 2700 Kelvin)","name":"neutral","value":370},{"description":"Warm temperature (454 mireds / 2200 Kelvin)","name":"warm","value":454},{"description":"Warmest temperature supported","name":"warmest","value":454},{"description":"Restore previous color_temp on cold power on","name":"previous","value":65535}],"property":"color_temp_startup","type":"numeric","unit":"mired","value_max":454,"value_min":153}],"type":"light"},{"access":7,"category":"config","description":"Controls the behavior when the device is powered on after power loss","label":"Power-on behavior","name":"power_on_behavior","property":"power_on_behavior","type":"enum","values":["off","on","toggle","previous"]},{"access":2,"label":"Effect","name":"effect","property":"effect","type":"enum","values":["blink","breathe","okay","channel_change","candle","finish_effect","stop_effect","stop_hue_effect"]},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"915005997601","options":[{"access":2,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition).","label":"Transition","name":"transition","property":"transition","type":"numeric","value_min":0},{"access":2,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true).","label":"Color sync","name":"color_sync","property":"color_sync","type":"binary","value_off":false,"value_on":true},{"access":2,"description":"State actions will also be published as 'action' when true (default false).","label":"State action","name":"state_action","property":"state_action","type":"binary","value_off":false,"value_on":true}],"supports_ota":true,"vendor":"Philips"},"disabled":false,"endpoints":{"11":{"bindings":[{"cluster":"genOnOff","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genLevelCtrl","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}}],"clusters":{"input":["genBasic","genIdentify","genGroups","genScenes","genOnOff","genLevelCtrl","touchlink","lightingColorCtrl"],"output":["genOta"]},"configured_reportings":[{"attribute":"onOff","cluster":"genOnOff","maximum_report_interval":3600,"minimum_report_interval":0,"reportable_change":0},{"attribute":"currentLevel","cluster":"genLevelCtrl","maximum_report_interval":3600,"minimum_report_interval":5,"reportable_change":1}],"scenes":[]},"242":{"bindings":[],"clusters":{"input":[],"output":["greenPower"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"Badlampe","ieee_address":"0x001788010d1c884e","interview_completed":true,"interviewing":false,"manufacturer":"Signify Netherlands B.V.","model_id":"915005997601","network_address":451,"power_source":"Mains (single phase)","software_build_id":"1.93.7","supported":true,"type":"Router"},{"date_code":"20210729","definition":{"description":"Hue dimmer switch","exposes":[{"access":1,"category":"diagnostic","description":"Remaining battery in %, can take up to 24 hours before reported","label":"Battery","name":"battery","property":"battery","type":"numeric","unit":"%","value_max":100,"value_min":0},{"access":1,"category":"diagnostic","description":"Triggered action (e.g. a button click)","label":"Action","name":"action","property":"action","type":"enum","values":["on_press","on_hold","on_press_release","on_hold_release","off_press","off_hold","off_press_release","off_hold_release","up_press","up_hold","up_press_release","up_hold_release","down_press","down_hold","down_press_release","down_hold_release","recall_0","recall_1"]},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"929002398602","options":[{"access":2,"description":"Simulate a brightness value. If this device provides a brightness_move_up or brightness_move_down action it is possible to specify the update interval and delta. The action_brightness_delta indicates the delta for each interval.","features":[{"access":2,"description":"Delta per interval, 20 by default","label":"Delta","name":"delta","property":"delta","type":"numeric","value_min":0},{"access":2,"description":"Interval duration","label":"Interval","name":"interval","property":"interval","type":"numeric","unit":"ms","value_min":0}],"label":"Simulated brightness","name":"simulated_brightness","property":"simulated_brightness","type":"composite"}],"supports_ota":true,"vendor":"Philips"},"disabled":false,"endpoints":{"1":{"bindings":[{"cluster":"genOnOff","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genLevelCtrl","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"manuSpecificPhilips","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genPowerCfg","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genScenes","target":{"endpoint":11,"ieee_address":"0x001788010d1c884e","type":"endpoint"}},{"cluster":"genOnOff","target":{"endpoint":11,"ieee_address":"0x001788010d1c884e","type":"endpoint"}},{"cluster":"genLevelCtrl","target":{"endpoint":11,"ieee_address":"0x001788010d1c884e","type":"endpoint"}},{"cluster":"genBasic","target":{"endpoint":11,"ieee_address":"0x001788010d1c884e","type":"endpoint"}},{"cluster":"genGroups","target":{"endpoint":11,"ieee_address":"0x001788010d1c884e","type":"endpoint"}},{"cluster":"genIdentify","target":{"endpoint":11,"ieee_address":"0x001788010d1c884e","type":"endpoint"}},{"cluster":"touchlink","target":{"endpoint":11,"ieee_address":"0x001788010d1c884e","type":"endpoint"}},{"cluster":"genOta","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genIdentify","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}}],"clusters":{"input":["genBasic","genPowerCfg","genIdentify","manuSpecificPhilips","touchlink"],"output":["genOta","genBasic","genIdentify","genGroups","genOnOff","genLevelCtrl","genScenes","touchlink"]},"configured_reportings":[{"attribute":"batteryPercentageRemaining","cluster":"genPowerCfg","maximum_report_interval":65000,"minimum_report_interval":3600,"reportable_change":0}],"scenes":[]}},"friendly_name":"Fernbedienung Bad","ieee_address":"0x001788010e8a8be7","interview_completed":true,"interviewing":false,"manufacturer":"Signify Netherlands B.V.","model_id":"RWL022","network_address":51589,"power_source":"Battery","software_build_id":"2.45.2_hF4400CA","supported":true,"type":"EndDevice"},{"date_code":"20200710","definition":{"description":"SmartHome led spot","exposes":[{"features":[{"access":7,"description":"On/off state of this light","label":"State","name":"state","property":"state","type":"binary","value_off":"OFF","value_on":"ON","value_toggle":"TOGGLE"},{"access":7,"description":"Brightness of this light","label":"Brightness","name":"brightness","property":"brightness","type":"numeric","value_max":254,"value_min":0},{"access":7,"description":"Color temperature of this light","label":"Color temp","name":"color_temp","presets":[{"description":"Coolest temperature supported","name":"coolest","value":150},{"description":"Cool temperature (250 mireds / 4000 Kelvin)","name":"cool","value":250},{"description":"Neutral temperature (370 mireds / 2700 Kelvin)","name":"neutral","value":370},{"description":"Warm temperature (454 mireds / 2200 Kelvin)","name":"warm","value":454},{"description":"Warmest temperature supported","name":"warmest","value":500}],"property":"color_temp","type":"numeric","unit":"mired","value_max":500,"value_min":150},{"access":7,"description":"Color temperature after cold power on of this light","label":"Color temp startup","name":"color_temp_startup","presets":[{"description":"Coolest temperature supported","name":"coolest","value":150},{"description":"Cool temperature (250 mireds / 4000 Kelvin)","name":"cool","value":250},{"description":"Neutral temperature (370 mireds / 2700 Kelvin)","name":"neutral","value":370},{"description":"Warm temperature (454 mireds / 2200 Kelvin)","name":"warm","value":454},{"description":"Warmest temperature supported","name":"warmest","value":500},{"description":"Restore previous color_temp on cold power on","name":"previous","value":65535}],"property":"color_temp_startup","type":"numeric","unit":"mired","value_max":500,"value_min":150}],"type":"light"},{"access":2,"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)","label":"Effect","name":"effect","property":"effect","type":"enum","values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"]},{"access":7,"category":"config","description":"Controls the behavior when the device is powered on after power loss","label":"Power-on behavior","name":"power_on_behavior","property":"power_on_behavior","type":"enum","values":["off","on","toggle","previous"]},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"50064","options":[{"access":2,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition).","label":"Transition","name":"transition","property":"transition","type":"numeric","value_min":0},{"access":2,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true).","label":"Color sync","name":"color_sync","property":"color_sync","type":"binary","value_off":false,"value_on":true},{"access":2,"description":"State actions will also be published as 'action' when true (default false).","label":"State action","name":"state_action","property":"state_action","type":"binary","value_off":false,"value_on":true}],"supports_ota":false,"vendor":"Paulmann"},"disabled":false,"endpoints":{"1":{"bindings":[],"clusters":{"input":["genBasic","genGroups","genIdentify","genOnOff","genLevelCtrl","genScenes","lightingColorCtrl","65535","65535","touchlink","4111"],"output":["genOta","4111"]},"configured_reportings":[],"scenes":[]},"242":{"bindings":[],"clusters":{"input":["greenPower"],"output":["greenPower"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"0x00158d00053a1aab","ieee_address":"0x00158d00053a1aab","interview_completed":true,"interviewing":false,"manufacturer":"Paulmann lamp","model_id":"CCT Light","network_address":22068,"power_source":"Mains (single phase)","software_build_id":"00.00.01","supported":true,"type":"Router"},{"date_code":"20200710","definition":{"description":"SmartHome led spot","exposes":[{"features":[{"access":7,"description":"On/off state of this light","label":"State","name":"state","property":"state","type":"binary","value_off":"OFF","value_on":"ON","value_toggle":"TOGGLE"},{"access":7,"description":"Brightness of this light","label":"Brightness","name":"brightness","property":"brightness","type":"numeric","value_max":254,"value_min":0},{"access":7,"description":"Color temperature of this light","label":"Color temp","name":"color_temp","presets":[{"description":"Coolest temperature supported","name":"coolest","value":150},{"description":"Cool temperature (250 mireds / 4000 Kelvin)","name":"cool","value":250},{"description":"Neutral temperature (370 mireds / 2700 Kelvin)","name":"neutral","value":370},{"description":"Warm temperature (454 mireds / 2200 Kelvin)","name":"warm","value":454},{"description":"Warmest temperature supported","name":"warmest","value":500}],"property":"color_temp","type":"numeric","unit":"mired","value_max":500,"value_min":150},{"access":7,"description":"Color temperature after cold power on of this light","label":"Color temp startup","name":"color_temp_startup","presets":[{"description":"Coolest temperature supported","name":"coolest","value":150},{"description":"Cool temperature (250 mireds / 4000 Kelvin)","name":"cool","value":250},{"description":"Neutral temperature (370 mireds / 2700 Kelvin)","name":"neutral","value":370},{"description":"Warm temperature (454 mireds / 2200 Kelvin)","name":"warm","value":454},{"description":"Warmest temperature supported","name":"warmest","value":500},{"description":"Restore previous color_temp on cold power on","name":"previous","value":65535}],"property":"color_temp_startup","type":"numeric","unit":"mired","value_max":500,"value_min":150}],"type":"light"},{"access":2,"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)","label":"Effect","name":"effect","property":"effect","type":"enum","values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"]},{"access":7,"category":"config","description":"Controls the behavior when the device is powered on after power loss","label":"Power-on behavior","name":"power_on_behavior","property":"power_on_behavior","type":"enum","values":["off","on","toggle","previous"]},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"50064","options":[{"access":2,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition).","label":"Transition","name":"transition","property":"transition","type":"numeric","value_min":0},{"access":2,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true).","label":"Color sync","name":"color_sync","property":"color_sync","type":"binary","value_off":false,"value_on":true},{"access":2,"description":"State actions will also be published as 'action' when true (default false).","label":"State action","name":"state_action","property":"state_action","type":"binary","value_off":false,"value_on":true}],"supports_ota":false,"vendor":"Paulmann"},"disabled":false,"endpoints":{"1":{"bindings":[],"clusters":{"input":["genBasic","genGroups","genIdentify","genOnOff","genLevelCtrl","genScenes","lightingColorCtrl","65535","65535","touchlink","4111"],"output":["genOta","4111"]},"configured_reportings":[],"scenes":[]},"242":{"bindings":[],"clusters":{"input":["greenPower"],"output":["greenPower"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"0x00158d00053c6311","ieee_address":"0x00158d00053c6311","interview_completed":true,"interviewing":false,"manufacturer":"Paulmann lamp","model_id":"CCT Light","network_address":49663,"power_source":"Mains (single phase)","software_build_id":"00.00.01","supported":true,"type":"Router"},{"date_code":"","definition":{"description":"Motion sensor","exposes":[{"access":1,"description":"Indicates whether the device detected occupancy","label":"Occupancy","name":"occupancy","property":"occupancy","type":"binary","value_off":false,"value_on":true},{"access":1,"category":"diagnostic","description":"Indicates if the battery of this device is almost empty","label":"Battery low","name":"battery_low","property":"battery_low","type":"binary","value_off":false,"value_on":true},{"access":1,"category":"diagnostic","description":"Remaining battery in %, can take up to 24 hours before reported","label":"Battery","name":"battery","property":"battery","type":"numeric","unit":"%","value_max":100,"value_min":0},{"access":1,"category":"diagnostic","description":"Voltage of the battery in millivolts","label":"Voltage","name":"voltage","property":"voltage","type":"numeric","unit":"mV"},{"access":1,"description":"Indicates whether the device is tampered","label":"Tamper","name":"tamper","property":"tamper","type":"binary","value_off":false,"value_on":true},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"809WZT","options":[],"supports_ota":false,"vendor":"Tuya"},"disabled":false,"endpoints":{"1":{"bindings":[{"cluster":"genPowerCfg","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}}],"clusters":{"input":["genPowerCfg","genIdentify","genGroups","ssIasZone","genBasic"],"output":["genGroups","genOnOff","touchlink","genOta","genTime"]},"configured_reportings":[{"attribute":"batteryPercentageRemaining","cluster":"genPowerCfg","maximum_report_interval":65000,"minimum_report_interval":3600,"reportable_change":0},{"attribute":"batteryVoltage","cluster":"genPowerCfg","maximum_report_interval":65000,"minimum_report_interval":3600,"reportable_change":0}],"scenes":[]}},"friendly_name":"Bewegungsmelder 1","ieee_address":"0xa4c13864e6c8c400","interview_completed":true,"interviewing":false,"manufacturer":"_TZ3040_bb6xaihh","model_id":"TS0202","network_address":33906,"power_source":"Battery","supported":true,"type":"EndDevice"},{"date_code":"","definition":{"description":"Door sensor","exposes":[{"access":1,"description":"Indicates if the contact is closed (= true) or open (= false)","label":"Contact","name":"contact","property":"contact","type":"binary","value_off":true,"value_on":false},{"access":1,"category":"diagnostic","description":"Remaining battery in %, can take up to 24 hours before reported","label":"Battery","name":"battery","property":"battery","type":"numeric","unit":"%","value_max":100,"value_min":0},{"access":1,"category":"diagnostic","description":"Voltage of the battery in millivolts","label":"Voltage","name":"voltage","property":"voltage","type":"numeric","unit":"mV"},{"access":1,"description":"Indicates whether the device is tampered","label":"Tamper","name":"tamper","property":"tamper","type":"binary","value_off":false,"value_on":true},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"TS0203","options":[],"supports_ota":false,"vendor":"Tuya"},"disabled":false,"endpoints":{"1":{"bindings":[{"cluster":"genPowerCfg","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}}],"clusters":{"input":["genPowerCfg","genIdentify","ssIasZone","genBasic"],"output":["genIdentify","genGroups","genScenes","genOnOff","genLevelCtrl","touchlink","genOta","genTime"]},"configured_reportings":[{"attribute":"batteryPercentageRemaining","cluster":"genPowerCfg","maximum_report_interval":65000,"minimum_report_interval":3600,"reportable_change":0},{"attribute":"batteryVoltage","cluster":"genPowerCfg","maximum_report_interval":65000,"minimum_report_interval":3600,"reportable_change":0}],"scenes":[]}},"friendly_name":"Sensor Terassentür","ieee_address":"0xa4c138ef60e2fdbe","interview_completed":true,"interviewing":false,"manufacturer":"_TZ3000_26fmupbb","model_id":"TS0203","network_address":45092,"power_source":"Battery","supported":true,"type":"EndDevice"},{"date_code":"Sep 29 2021\u0000\u0000\u0000\u0000\u0000","definition":{"description":"SMART+ Candle E14 Dimmable White","exposes":[{"features":[{"access":7,"description":"On/off state of this light","label":"State","name":"state","property":"state","type":"binary","value_off":"OFF","value_on":"ON","value_toggle":"TOGGLE"},{"access":7,"description":"Brightness of this light","label":"Brightness","name":"brightness","property":"brightness","type":"numeric","value_max":254,"value_min":0}],"type":"light"},{"access":2,"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)","label":"Effect","name":"effect","property":"effect","type":"enum","values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"]},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"AC08562","options":[{"access":2,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition).","label":"Transition","name":"transition","property":"transition","type":"numeric","value_min":0},{"access":2,"description":"State actions will also be published as 'action' when true (default false).","label":"State action","name":"state_action","property":"state_action","type":"binary","value_off":false,"value_on":true}],"supports_ota":true,"vendor":"OSRAM"},"disabled":false,"endpoints":{"1":{"bindings":[],"clusters":{"input":["genBasic","genIdentify","genGroups","genScenes","genOnOff","genLevelCtrl","haDiagnostic","touchlink","manuSpecificOsram"],"output":["genOta"]},"configured_reportings":[],"scenes":[]},"242":{"bindings":[],"clusters":{"input":[],"output":["greenPower"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0","interview_completed":true,"interviewing":false,"manufacturer":"LEDVANCE","model_id":"B40 DIM Z3","network_address":47599,"power_source":"Mains (single phase)","software_build_id":"01056400","supported":true,"type":"Router"},{"date_code":"20140331CNEF****","definition":{"description":"LIGHTIFY LED Classic A60 clear","exposes":[{"features":[{"access":7,"description":"On/off state of this light","label":"State","name":"state","property":"state","type":"binary","value_off":"OFF","value_on":"ON","value_toggle":"TOGGLE"},{"access":7,"description":"Brightness of this light","label":"Brightness","name":"brightness","property":"brightness","type":"numeric","value_max":254,"value_min":0}],"type":"light"},{"access":2,"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)","label":"Effect","name":"effect","property":"effect","type":"enum","values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"]},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"AC03641","options":[{"access":2,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition).","label":"Transition","name":"transition","property":"transition","type":"numeric","value_min":0},{"access":2,"description":"State actions will also be published as 'action' when true (default false).","label":"State action","name":"state_action","property":"state_action","type":"binary","value_off":false,"value_on":true}],"supports_ota":true,"vendor":"OSRAM"},"disabled":false,"endpoints":{"3":{"bindings":[],"clusters":{"input":["touchlink","genBasic","genIdentify","genGroups","genScenes","genOnOff","genLevelCtrl","manuSpecificOsram"],"output":["genOta"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"Küchentisch","ieee_address":"0x7cb03eaa0a0176bd","interview_completed":true,"interviewing":false,"manufacturer":"OSRAM","model_id":"Classic A60 W clear - LIGHTIFY","network_address":59143,"power_source":"Mains (single phase)","software_build_id":"V1.05.10","supported":true,"type":"Router"},{"date_code":"201904180638010","definition":{"description":"Smart+ switch mini","exposes":[{"access":1,"category":"diagnostic","description":"Remaining battery in %, can take up to 24 hours before reported","label":"Battery","name":"battery","property":"battery","type":"numeric","unit":"%","value_max":100,"value_min":0},{"access":1,"category":"diagnostic","description":"Triggered action (e.g. a button click)","label":"Action","name":"action","property":"action","type":"enum","values":["on","brightness_move_up","brightness_move_down","brightness_stop","color_temperature_move","hue_move","hue_stop","move_to_saturation","off","brightness_move_to_level"]},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"AC0251100NJ/AC0251600NJ/AC0251700NJ","options":[{"access":2,"description":"Simulate a brightness value. If this device provides a brightness_move_up or brightness_move_down action it is possible to specify the update interval and delta. The action_brightness_delta indicates the delta for each interval.","features":[{"access":2,"description":"Delta per interval, 20 by default","label":"Delta","name":"delta","property":"delta","type":"numeric","value_min":0},{"access":2,"description":"Interval duration","label":"Interval","name":"interval","property":"interval","type":"numeric","unit":"ms","value_min":0}],"label":"Simulated brightness","name":"simulated_brightness","property":"simulated_brightness","type":"composite"}],"supports_ota":true,"vendor":"OSRAM"},"disabled":false,"endpoints":{"1":{"bindings":[{"cluster":"genPollCtrl","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genOnOff","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genLevelCtrl","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genPowerCfg","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}}],"clusters":{"input":["genBasic","genPowerCfg","genPollCtrl","touchlink","64768"],"output":["genIdentify","genGroups","genScenes","genOnOff","genLevelCtrl","genOta","lightingColorCtrl","touchlink"]},"configured_reportings":[{"attribute":"batteryVoltage","cluster":"genPowerCfg","maximum_report_interval":65000,"minimum_report_interval":3600,"reportable_change":0}],"scenes":[]},"2":{"bindings":[{"cluster":"genOnOff","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genLevelCtrl","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}}],"clusters":{"input":["genBasic","touchlink","64768"],"output":["genIdentify","genGroups","genScenes","genOnOff","genLevelCtrl","lightingColorCtrl","touchlink"]},"configured_reportings":[],"scenes":[]},"3":{"bindings":[{"cluster":"genLevelCtrl","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"lightingColorCtrl","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}}],"clusters":{"input":["genBasic","touchlink","64768"],"output":["genIdentify","genGroups","genScenes","genOnOff","genLevelCtrl","lightingColorCtrl","touchlink"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"Fernbedienung 2","ieee_address":"0x000d6f001417c142","interview_completed":true,"interviewing":false,"manufacturer":"OSRAM","model_id":"Lightify Switch Mini","network_address":31488,"power_source":"Battery","software_build_id":"e.1.11.0M","supported":true,"type":"EndDevice"},{"definition":{"description":"Zigbee water sensor","exposes":[{"access":5,"category":"diagnostic","description":"Remaining battery in %","label":"Battery","name":"battery","property":"battery","type":"numeric","unit":"%","value_max":100,"value_min":0},{"access":1,"description":"Indicates whether the device detected a water leak","label":"Water leak","name":"water_leak","property":"water_leak","type":"binary","value_off":false,"value_on":true},{"access":1,"category":"diagnostic","description":"Indicates whether the battery of the device is almost empty","label":"Battery low","name":"battery_low","property":"battery_low","type":"binary","value_off":false,"value_on":true},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"SNZB-05","options":[],"supports_ota":false,"vendor":"eWeLink"},"disabled":false,"endpoints":{"1":{"bindings":[{"cluster":"genPollCtrl","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}},{"cluster":"genPowerCfg","target":{"endpoint":1,"ieee_address":"0x00212effff04fc2c","type":"endpoint"}}],"clusters":{"input":["genBasic","genIdentify","genPowerCfg","ssIasZone","genPollCtrl"],"output":["genOta"]},"configured_reportings":[{"attribute":"batteryPercentageRemaining","cluster":"genPowerCfg","maximum_report_interval":65000,"minimum_report_interval":3600,"reportable_change":10}],"scenes":[]}},"friendly_name":"Wassersensor Keller","ieee_address":"0xa4c138e68023f4c6","interview_completed":true,"interviewing":false,"manufacturer":"_TZ3000_upgcbody","model_id":"SNZB-05","network_address":60500,"power_source":"Battery","software_build_id":"0122052017","supported":true,"type":"EndDevice"},{"definition":{"description":"Temperature and humidity sensor","exposes":[{"access":1,"description":"Measured temperature value","label":"Temperature","name":"temperature","property":"temperature","type":"numeric","unit":"°C"},{"access":1,"description":"Measured relative humidity","label":"Humidity","name":"humidity","property":"humidity","type":"numeric","unit":"%"},{"access":3,"description":"Temperature unit","label":"Temperature unit","name":"temperature_unit","property":"temperature_unit","type":"enum","values":["celsius","fahrenheit"]},{"access":3,"description":"Temperature calibration","label":"Temperature calibration","name":"temperature_calibration","property":"temperature_calibration","type":"numeric","unit":"°C","value_max":2,"value_min":-2,"value_step":0.1},{"access":3,"description":"Humidity calibration","label":"Humidity calibration","name":"humidity_calibration","property":"humidity_calibration","type":"numeric","unit":"%","value_max":30,"value_min":-30,"value_step":1},{"access":1,"category":"diagnostic","description":"Remaining battery in %, can take up to 24 hours before reported","label":"Battery","name":"battery","property":"battery","type":"numeric","unit":"%","value_max":100,"value_min":0},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"ZG-227Z","options":[{"access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device.","label":"Temperature calibration","name":"temperature_calibration","property":"temperature_calibration","type":"numeric"},{"access":2,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device. This option can only decrease the precision, not increase it.","label":"Temperature precision","name":"temperature_precision","property":"temperature_precision","type":"numeric","value_max":3,"value_min":0},{"access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device.","label":"Humidity calibration","name":"humidity_calibration","property":"humidity_calibration","type":"numeric"},{"access":2,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device. This option can only decrease the precision, not increase it.","label":"Humidity precision","name":"humidity_precision","property":"humidity_precision","type":"numeric","value_max":3,"value_min":0}],"supports_ota":false,"vendor":"Tuya"},"disabled":false,"endpoints":{"1":{"bindings":[],"clusters":{"input":["genBasic","genIdentify","msTemperatureMeasurement","msRelativeHumidity","genPowerCfg"],"output":["genIdentify"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"Medienschrank Wohnzimmer","ieee_address":"0xa4c13838ba59a1b2","interview_completed":true,"interviewing":false,"manufacturer":"_TZE200_a8sdabtg","model_id":"TS0601","network_address":63741,"power_source":"Battery","supported":true,"type":"EndDevice"},{"definition":{"description":"Temperature and humidity sensor","exposes":[{"access":1,"description":"Measured temperature value","label":"Temperature","name":"temperature","property":"temperature","type":"numeric","unit":"°C"},{"access":1,"description":"Measured relative humidity","label":"Humidity","name":"humidity","property":"humidity","type":"numeric","unit":"%"},{"access":3,"description":"Temperature unit","label":"Temperature unit","name":"temperature_unit","property":"temperature_unit","type":"enum","values":["celsius","fahrenheit"]},{"access":3,"description":"Temperature calibration","label":"Temperature calibration","name":"temperature_calibration","property":"temperature_calibration","type":"numeric","unit":"°C","value_max":2,"value_min":-2,"value_step":0.1},{"access":3,"description":"Humidity calibration","label":"Humidity calibration","name":"humidity_calibration","property":"humidity_calibration","type":"numeric","unit":"%","value_max":30,"value_min":-30,"value_step":1},{"access":1,"category":"diagnostic","description":"Remaining battery in %, can take up to 24 hours before reported","label":"Battery","name":"battery","property":"battery","type":"numeric","unit":"%","value_max":100,"value_min":0},{"access":1,"category":"diagnostic","description":"Link quality (signal strength)","label":"Linkquality","name":"linkquality","property":"linkquality","type":"numeric","unit":"lqi","value_max":255,"value_min":0}],"model":"ZG-227Z","options":[{"access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device.","label":"Temperature calibration","name":"temperature_calibration","property":"temperature_calibration","type":"numeric"},{"access":2,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device. This option can only decrease the precision, not increase it.","label":"Temperature precision","name":"temperature_precision","property":"temperature_precision","type":"numeric","value_max":3,"value_min":0},{"access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device.","label":"Humidity calibration","name":"humidity_calibration","property":"humidity_calibration","type":"numeric"},{"access":2,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device. This option can only decrease the precision, not increase it.","label":"Humidity precision","name":"humidity_precision","property":"humidity_precision","type":"numeric","value_max":3,"value_min":0}],"supports_ota":false,"vendor":"Tuya"},"disabled":false,"endpoints":{"1":{"bindings":[],"clusters":{"input":["genBasic","genIdentify","msTemperatureMeasurement","msRelativeHumidity","genPowerCfg"],"output":["genIdentify"]},"configured_reportings":[],"scenes":[]}},"friendly_name":"Temperatur Keller","ieee_address":"0xa4c1389d42e94844","interview_completed":true,"interviewing":false,"manufacturer":"_TZE200_a8sdabtg","model_id":"TS0601","network_address":4843,"power_source":"Battery","software_build_id":"0122052017","supported":true,"type":"EndDevice"}]'
[2025-01-19 22:58:11] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/bridge/groups' with data '[]'
[2025-01-19 22:58:11] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/bridge/definitions' with data '{"clusters":{"barrierControl":{"ID":259,"attributes":{"barrierPosition":{"ID":10,"type":32},"capabilities":{"ID":3,"type":24},"closeEvents":{"ID":5,"type":33},"closePeriod":{"ID":9,"type":33},"commandCloseEvents":{"ID":7,"type":33},"commandOpenEvents":{"ID":6,"type":33},"movingState":{"ID":1,"type":48},"openEvents":{"ID":4,"type":33},"openPeriod":{"ID":8,"type":33},"safetyStatus":{"ID":2,"type":25}},"commands":{"goToPercent":{"ID":0,"parameters":[{"name":"percentOpen","type":32}]},"stop":{"ID":1,"parameters":[]}},"commandsResponse":{}},"closuresDoorLock":{"ID":257,"attributes":{"actuatorEnabled":{"ID":2,"type":16},"alarmMask":{"ID":64,"type":25},"autoRelockTime":{"ID":35,"type":35},"defaultConfigurationRegister":{"ID":39,"type":25},"doorClosedEvents":{"ID":5,"type":35},"doorOpenEvents":{"ID":4,"type":35},"doorState":{"ID":3,"type":48},"enableInsideStatusLed":{"ID":42,"type":16},"enableLocalProgramming":{"ID":40,"type":16},"enableLogging":{"ID":32,"type":16},"enableOneTouchLocking":{"ID":41,"type":16},"enablePrivacyModeButton":{"ID":43,"type":16},"keypadOperationEventMask":{"ID":65,"type":25},"keypadProgrammingEventMask":{"ID":69,"type":25},"language":{"ID":33,"type":66},"ledSettings":{"ID":34,"type":32},"lockState":{"ID":0,"type":48},"lockType":{"ID":38,"type":25},"manualOperationEventMask":{"ID":67,"type":25},"maxPinLen":{"ID":23,"type":32},"maxRfidLen":{"ID":25,"type":32},"minPinLen":{"ID":24,"type":32},"minRfidLen":{"ID":26,"type":32},"numOfHolidayScheduledsSupported":{"ID":22,"type":32},"numOfLockRecordsSupported":{"ID":16,"type":33},"numOfPinUsersSupported":{"ID":18,"type":33},"numOfRfidUsersSupported":{"ID":19,"type":33},"numOfTotalUsersSupported":{"ID":17,"type":33},"numOfWeekDaySchedulesSupportedPerUser":{"ID":20,"type":32},"numOfYearDaySchedulesSupportedPerUser":{"ID":21,"type":32},"openPeriod":{"ID":6,"type":33},"operatingMode":{"ID":37,"type":35},"requirePinForRfOperation":{"ID":51,"type":16},"rfOperationEventMask":{"ID":66,"type":25},"rfProgrammingEventMask":{"ID":70,"type":25},"rfidOperationEventMask":{"ID":68,"type":25},"rfidProgrammingEventMask":{"ID":71,"type":25},"sendPinOta":{"ID":50,"type":16},"soundVolume":{"ID":36,"type":32},"userCodeTemporaryDisableTime":{"ID":49,"type":32},"wrongCodeEntryLimit":{"ID":48,"type":32},"zigbeeSecurityLevel":{"ID":52,"type":32}},"commands":{"clearAllPinCodes":{"ID":8,"parameters":[],"response":8},"clearAllRfidCodes":{"ID":25,"parameters":[],"response":25},"clearHolidaySchedule":{"ID":19,"parameters":[{"name":"holidayscheduleid","type":32}],"response":19},"clearPinCode":{"ID":7,"parameters":[{"name":"userid","type":33}],"response":7},"clearRfidCode":{"ID":24,"parameters":[{"name":"userid","type":33}],"response":24},"clearWeekDaySchedule":{"ID":13,"parameters":[{"name":"scheduleid","type":32},{"name":"userid","type":33}],"response":13},"clearYearDaySchedule":{"ID":16,"parameters":[{"name":"scheduleid","type":32},{"name":"userid","type":33}],"response":16},"getHolidaySchedule":{"ID":18,"parameters":[{"name":"holidayscheduleid","type":32}],"response":18},"getLogRecord":{"ID":4,"parameters":[{"name":"logindex","type":33}],"response":4},"getPinCode":{"ID":6,"parameters":[{"name":"userid","type":33}],"response":6},"getRfidCode":{"ID":23,"parameters":[{"name":"userid","type":33}],"response":23},"getUserStatus":{"ID":10,"parameters":[{"name":"userid","type":33}],"response":10},"getUserType":{"ID":21,"parameters":[{"name":"userid","type":33}],"response":21},"getWeekDaySchedule":{"ID":12,"parameters":[{"name":"scheduleid","type":32},{"name":"userid","type":33}],"response":12},"getYearDaySchedule":{"ID":15,"parameters":[{"name":"scheduleid","type":32},{"name":"userid","type":33}],"response":15},"lockDoor":{"ID":0,"parameters":[{"name":"pincodevalue","type":66}],"response":0},"setHolidaySchedule":{"ID":17,"parameters":[{"name":"holidayscheduleid","type":32},{"name":"zigbeelocalstarttime","type":35},{"name":"zigbeelocalendtime","type":35},{"name":"opermodelduringholiday","type":32}],"response":17},"setPinCode":{"ID":5,"parameters":[{"name":"userid","type":33},{"name":"userstatus","type":32},{"name":"usertype","type":32},{"name":"pincodevalue","type":66}],"response":5},"setRfidCode":{"ID":22,"parameters":[{"name":"userid","type":33},{"name":"userstatus","type":32},{"name":"usertype","type":32},{"name":"pincodevalue","type":66}],"response":22},"setUserStatus":{"ID":9,"parameters":[{"name":"userid","type":33},{"name":"userstatus","type":32}],"response":9},"setUserType":{"ID":20,"parameters":[{"name":"userid","type":33},{"name":"usertype","type":32}],"response":20},"setWeekDaySchedule":{"ID":11,"parameters":[{"name":"scheduleid","type":32},{"name":"userid","type":33},{"name":"daysmask","type":32},{"name":"starthour","type":32},{"name":"startminute","type":32},{"name":"endhour","type":32},{"name":"endminute","type":32}],"response":11},"setYearDaySchedule":{"ID":14,"parameters":[{"name":"scheduleid","type":32},{"name":"userid","type":33},{"name":"zigbeelocalstarttime","type":35},{"name":"zigbeelocalendtime","type":35}],"response":14},"toggleDoor":{"ID":2,"parameters":[{"name":"pincodevalue","type":66}],"response":2},"unlockDoor":{"ID":1,"parameters":[{"name":"pincodevalue","type":66}],"response":1},"unlockWithTimeout":{"ID":3,"parameters":[{"name":"timeout","type":33},{"name":"pincodevalue","type":66}],"response":3}},"commandsResponse":{"clearAllPinCodesRsp":{"ID":8,"parameters":[{"name":"status","type":32}]},"clearAllRfidCodesRsp":{"ID":25,"parameters":[{"name":"status","type":32}]},"clearHolidayScheduleRsp":{"ID":19,"parameters":[{"name":"status","type":32}]},"clearPinCodeRsp":{"ID":7,"parameters":[{"name":"status","type":32}]},"clearRfidCodeRsp":{"ID":24,"parameters":[{"name":"status","type":32}]},"clearWeekDayScheduleRsp":{"ID":13,"parameters":[{"name":"status","type":32}]},"clearYearDayScheduleRsp":{"ID":16,"parameters":[{"name":"status","type":32}]},"getHolidayScheduleRsp":{"ID":18,"parameters":[{"name":"holidayscheduleid","type":32},{"name":"status","type":32},{"name":"zigbeelocalstarttime","type":35},{"name":"zigbeelocalendtime","type":35},{"name":"opermodelduringholiday","type":32}]},"getLogRecordRsp":{"ID":4,"parameters":[{"name":"logentryid","type":33},{"name":"timestamp","type":35},{"name":"eventtype","type":32},{"name":"source","type":32},{"name":"eventidalarmcode","type":32},{"name":"userid","type":33},{"name":"pincodevalue","type":66}]},"getPinCodeRsp":{"ID":6,"parameters":[{"name":"userid","type":33},{"name":"userstatus","type":32},{"name":"usertype","type":32},{"name":"pincodevalue","type":66}]},"getRfidCodeRsp":{"ID":23,"parameters":[{"name":"userid","type":33},{"name":"userstatus","type":32},{"name":"usertype","type":32},{"name":"pincodevalue","type":66}]},"getUserStatusRsp":{"ID":10,"parameters":[{"name":"userid","type":33},{"name":"userstatus","type":32}]},"getUserTypeRsp":{"ID":21,"parameters":[{"name":"userid","type":33},{"name":"usertype","type":32}]},"getWeekDayScheduleRsp":{"ID":12,"parameters":[{"name":"scheduleid","type":32},{"name":"userid","type":33},{"name":"status","type":32},{"name":"daysmask","type":32},{"name":"starthour","type":32},{"name":"startminute","type":32},{"name":"endhour","type":32},{"name":"endminute","type":32}]},"getYearDayScheduleRsp":{"ID":15,"parameters":[{"name":"scheduleid","type":32},{"name":"userid","type":33},{"name":"status","type":32},{"name":"zigbeelocalstarttime","type":35},{"name":"zigbeelocalendtime","type":35}]},"lockDoorRsp":{"ID":0,"parameters":[{"name":"status","type":32}]},"operationEventNotification":{"ID":32,"parameters":[{"name":"opereventsrc","type":32},{"name":"opereventcode","type":32},{"name":"userid","type":33},{"name":"pin","type":65},{"name":"zigbeelocaltime","type":35},{"name":"data","type":32}]},"programmingEventNotification":{"ID":33,"parameters":[{"name":"programeventsrc","type":32},{"name":"programeventcode","type":32},{"name":"userid","type":33},{"name":"pin","type":65},{"name":"usertype","type":32},{"name":"userstatus","type":32},{"name":"zigbeelocaltime","type":35},{"name":"data","type":32}]},"setHolidayScheduleRsp":{"ID":17,"parameters":[{"name":"status","type":32}]},"setPinCodeRsp":{"ID":5,"parameters":[{"name":"status","type":32}]},"setRfidCodeRsp":{"ID":22,"parameters":[{"name":"status","type":32}]},"setUserStatusRsp":{"ID":9,"parameters":[{"name":"status","type":32}]},"setUserTypeRsp":{"ID":20,"parameters":[{"name":"status","type":32}]},"setWeekDayScheduleRsp":{"ID":11,"parameters":[{"name":"status","type":32}]},"setYearDayScheduleRsp":{"ID":14,"parameters":[{"name":"status","type":32}]},"toggleDoorRsp":{"ID":2,"parameters":[{"name":"status","type":32}]},"unlockDoorRsp":{"ID":1,"parameters":[{"name":"status","type":32}]},"unlockWithTimeoutRsp":{"ID":3,"parameters":[{"name":"status","type":32}]}}},"closuresShadeCfg":{"ID":256,"attributes":{"losedLimit":{"ID":16,"type":33},"mode":{"ID":18,"type":48},"motorStepSize":{"ID":1,"type":32},"physicalClosedLimit":{"ID":0,"type":33},"status":{"ID":2,"type":24}},"commands":{},"commandsResponse":{}},"closuresWindowCovering":{"ID":258,"attributes":{"accelerationTimeLift":{"ID":21,"type":33},"calibrationMode":{"ID":61442,"manufacturerCode":4129,"type":48},"configStatus":{"ID":7,"type":24},"currentPositionLiftCm":{"ID":3,"type":33},"currentPositionLiftPercentage":{"ID":8,"type":32},"currentPositionTiltDdegree":{"ID":4,"type":33},"currentPositionTiltPercentage":{"ID":9,"type":32},"decelerationTimeLift":{"ID":22,"type":33},"elkoDriveCloseDuration":{"ID":57344,"manufacturerCode":4727,"type":33},"elkoLiftDriveDownTime":{"ID":57365,"manufacturerCode":4727,"type":33},"elkoLiftDriveUpTime":{"ID":57364,"manufacturerCode":4727,"type":33},"elkoProtectionSensor":{"ID":57363,"manufacturerCode":4727,"type":24},"elkoProtectionStatus":{"ID":57360,"manufacturerCode":4727,"type":24},"elkoSunProtectionIlluminanceThreshold":{"ID":57362,"manufacturerCode":4727,"type":33},"elkoTiltOpenCloseAndStepTime":{"ID":57366,"manufacturerCode":4727,"type":33},"elkoTiltPositionPercentageAfterMoveToLevel":{"ID":57367,"manufacturerCode":4727,"type":32},"installedClosedLimitLiftCm":{"ID":17,"type":33},"installedClosedLimitTiltDdegree":{"ID":19,"type":33},"installedOpenLimitLiftCm":{"ID":16,"type":33},"installedOpenLimitTiltDdegree":{"ID":18,"type":33},"intermediateSetpointsLift":{"ID":24,"type":65},"intermediateSetpointsTilt":{"ID":25,"type":65},"moesCalibrationTime":{"ID":61443,"type":33},"nikoCalibrationTimeDown":{"ID":64706,"manufacturerCode":4703,"type":33},"nikoCalibrationTimeUp":{"ID":64705,"manufacturerCode":4703,"type":33},"numOfActuationsLift":{"ID":5,"type":33},"numOfActuationsTilt":{"ID":6,"type":33},"operationalStatus":{"ID":10,"type":24},"physicalClosedLimitLiftCm":{"ID":1,"type":33},"physicalClosedLimitTiltDdegree":{"ID":2,"type":33},"stepPositionLift":{"ID":61441,"manufacturerCode":4129,"type":48},"stepPositionTilt":{"ID":61444,"manufacturerCode":4129,"type":48},"targetPositionTiltPercentage":{"ID":61443,"manufacturerCode":4129,"type":48},"tuyaCalibration":{"ID":61441,"type":48},"tuyaMotorReversal":{"ID":61442,"type":48},"tuyaMovingState":{"ID":61440,"type":48},"velocityLift":{"ID":20,"type":33},"windowCoveringMode":{"ID":23,"type":24},"windowCoveringType":{"ID":0,"type":48}},"commands":{"downClose":{"ID":1,"parameters":[]},"elkoStopOrStepLiftPercentage":{"ID":128,"parameters":[{"name":"direction","type":33},{"name":"stepvalue","type":33}]},"goToLiftPercentage":{"ID":5,"parameters":[{"name":"percentageliftvalue","type":32}]},"goToLiftValue":{"ID":4,"parameters":[{"name":"liftvalue","type":33}]},"goToTiltPercentage":{"ID":8,"parameters":[{"name":"percentagetiltvalue","type":32}]},"goToTiltValue":{"ID":7,"parameters":[{"name":"tiltvalue","type":33}]},"stop":{"ID":2,"parameters":[]},"upOpen":{"ID":0,"parameters":[]}},"commandsResponse":{}},"elkoOccupancySettingClusterServer":{"ID":65305,"attributes":{"AmbienceLightThreshold":{"ID":0,"type":33},"OccupancyActions":{"ID":1,"type":48},"UnoccupiedLevel":{"ID":3,"type":32},"UnoccupiedLevelDflt":{"ID":2,"type":32}},"commands":{},"commandsResponse":{},"manufacturerCode":4727},"elkoSwitchConfigurationClusterServer":{"ID":65303,"attributes":{"DownGroupID":{"ID":33,"type":33},"DownSceneID":{"ID":32,"type":32},"SwitchActions":{"ID":1,"type":48},"SwitchIndication":{"ID":0,"type":48},"UpGroupID":{"ID":17,"type":33},"UpSceneID":{"ID":16,"type":32}},"commands":{},"commandsResponse":{},"manufacturerCode":4727},"genAlarms":{"ID":9,"attributes":{"alarmCount":{"ID":0,"type":33}},"commands":{"getAlarm":{"ID":2,"parameters":[]},"publishEventLog":{"ID":4,"parameters":[]},"reset":{"ID":0,"parameters":[{"name":"alarmcode","type":32},{"name":"clusterid","type":33}]},"resetAll":{"ID":1,"parameters":[]},"resetLog":{"ID":3,"parameters":[]}},"commandsResponse":{"alarm":{"ID":0,"parameters":[{"name":"alarmcode","type":32},{"name":"clusterid","type":33}]},"getEventLog":{"ID":2,"parameters":[]},"getRsp":{"ID":1,"parameters":[{"name":"status","type":32},{"name":"alarmcode","type":32},{"name":"clusterid","type":33},{"name":"timestamp","type":35}]}}},"genAnalogInput":{"ID":12,"attributes":{"applicationType":{"ID":256,"type":35},"description":{"ID":28,"type":66},"engineeringUnits":{"ID":117,"type":49},"maxPresentValue":{"ID":65,"type":57},"minPresentValue":{"ID":69,"type":57},"outOfService":{"ID":81,"type":16},"presentValue":{"ID":85,"type":57},"reliability":{"ID":103,"type":48},"resolution":{"ID":106,"type":57},"statusFlags":{"ID":111,"type":24}},"commands":{},"commandsResponse":{}},"genAnalogOutput":{"ID":13,"attributes":{"applicationType":{"ID":256,"type":35},"description":{"ID":28,"type":66},"engineeringUnits":{"ID":117,"type":49},"maxPresentValue":{"ID":65,"type":57},"minPresentValue":{"ID":69,"type":57},"outOfService":{"ID":81,"type":16},"presentValue":{"ID":85,"type":57},"priorityArray":{"ID":87,"type":72},"reliability":{"ID":103,"type":48},"relinquishDefault":{"ID":104,"type":57},"resolution":{"ID":106,"type":57},"statusFlags":{"ID":111,"type":24}},"commands":{},"commandsResponse":{}},"genAnalogValue":{"ID":14,"attributes":{"applicationType":{"ID":256,"type":35},"description":{"ID":28,"type":66},"engineeringUnits":{"ID":117,"type":49},"outOfService":{"ID":81,"type":16},"presentValue":{"ID":85,"type":57},"priorityArray":{"ID":87,"type":72},"reliability":{"ID":103,"type":48},"relinquishDefault":{"ID":104,"type":57},"statusFlags":{"ID":111,"type":24}},"commands":{},"commandsResponse":{}},"genBasic":{"ID":0,"attributes":{"alarmMask":{"ID":19,"type":24},"appProfileVersion":{"ID":8,"type":48},"appVersion":{"ID":1,"type":32},"dateCode":{"ID":6,"type":66},"deviceEnabled":{"ID":18,"type":16},"disableLocalConfig":{"ID":20,"type":24},"genericDeviceType":{"ID":9,"type":48},"hwVersion":{"ID":3,"type":32},"locationDesc":{"ID":16,"type":66},"manufacturerName":{"ID":4,"type":66},"manufacturerVersionDetails":{"ID":12,"type":66},"modelId":{"ID":5,"type":66},"physicalEnv":{"ID":17,"type":48},"powerSource":{"ID":7,"type":48},"productCode":{"ID":10,"type":65},"productLabel":{"ID":14,"type":66},"productUrl":{"ID":11,"type":66},"schneiderMeterRadioPower":{"ID":57856,"manufacturerCode":4190,"type":40},"serialNumber":{"ID":13,"type":66},"stackVersion":{"ID":2,"type":32},"swBuildId":{"ID":16384,"type":66},"zclVersion":{"ID":0,"type":32}},"commands":{"resetFactDefault":{"ID":0,"parameters":[]},"tuyaSetup":{"ID":240,"parameters":[]}},"commandsResponse":{}},"genBinaryInput":{"ID":15,"attributes":{"activeText":{"ID":4,"type":66},"applicationType":{"ID":256,"type":35},"description":{"ID":28,"type":66},"inactiveText":{"ID":46,"type":66},"outOfService":{"ID":81,"type":16},"polarity":{"ID":84,"type":48},"presentValue":{"ID":85,"type":16},"reliability":{"ID":103,"type":48},"statusFlags":{"ID":111,"type":24}},"commands":{},"commandsResponse":{}},"genBinaryOutput":{"ID":16,"attributes":{"activeText":{"ID":4,"type":66},"applicationType":{"ID":256,"type":35},"description":{"ID":28,"type":66},"inactiveText":{"ID":46,"type":66},"minimumOffTime":{"ID":66,"type":35},"minimumOnTime":{"ID":67,"type":35},"outOfService":{"ID":81,"type":16},"polarity":{"ID":84,"type":48},"presentValue":{"ID":85,"type":16},"priorityArray":{"ID":87,"type":72},"reliability":{"ID":103,"type":48},"relinquishDefault":{"ID":104,"type":16},"statusFlags":{"ID":111,"type":24}},"commands":{},"commandsResponse":{}},"genBinaryValue":{"ID":17,"attributes":{"activeText":{"ID":4,"type":66},"applicationType":{"ID":256,"type":35},"description":{"ID":28,"type":66},"inactiveText":{"ID":46,"type":66},"minimumOffTime":{"ID":66,"type":35},"minimumOnTime":{"ID":67,"type":35},"outOfService":{"ID":81,"type":16},"presentValue":{"ID":85,"type":16},"priorityArray":{"ID":87,"type":72},"reliability":{"ID":103,"type":48},"relinquishDefault":{"ID":104,"type":16},"statusFlags":{"ID":111,"type":24}},"commands":{},"commandsResponse":{}},"genCommissioning":{"ID":21,"attributes":{"channelmask":{"ID":3,"type":27},"concentratorDiscoveryTime":{"ID":66,"type":32},"concentratorFlag":{"ID":64,"type":16},"concentratorRus":{"ID":65,"type":32},"extendedPANId":{"ID":1,"type":240},"indirectPollRate":{"ID":48,"type":33},"maxRejoinInterval":{"ID":35,"type":33},"networkKey":{"ID":18,"type":241},"networkKeySeqNum":{"ID":21,"type":32},"networkKeyType":{"ID":22,"type":48},"networkManagerress":{"ID":23,"type":33},"panId":{"ID":2,"type":33},"parentRetryThreshold":{"ID":49,"type":32},"preconfiguredLinkKey":{"ID":20,"type":241},"protocolVersion":{"ID":4,"type":32},"rejoinInterval":{"ID":34,"type":33},"scanAttempts":{"ID":32,"type":32},"shortress":{"ID":0,"type":33},"stackProfile":{"ID":5,"type":32},"startupControl":{"ID":6,"type":48},"timeBetweenScans":{"ID":33,"type":33},"trustCenterMasterKey":{"ID":17,"type":241},"trustCenterress":{"ID":16,"type":240},"useInsecureJoin":{"ID":19,"type":16}},"commands":{"resetStartupParams":{"ID":3,"parameters":[{"name":"options","type":32},{"name":"index","type":32}]},"restartDevice":{"ID":0,"parameters":[{"name":"options","type":32},{"name":"delay","type":32},{"name":"jitter","type":32}]},"restoreStartupParams":{"ID":2,"parameters":[{"name":"options","type":32},{"name":"index","type":32}]},"saveStartupParams":{"ID":1,"parameters":[{"name":"options","type":32},{"name":"index","type":32}]}},"commandsResponse":{"resetStartupParamsRsp":{"ID":3,"parameters":[{"name":"status","type":32}]},"restartDeviceRsp":{"ID":0,"parameters":[{"name":"status","type":32}]},"restoreStartupParamsRsp":{"ID":2,"parameters":[{"name":"status","type":32}]},"saveStartupParamsRsp":{"ID":1,"parameters":[{"name":"status","type":32}]}}},"genDeviceTempCfg":{"ID":2,"attributes":{"currentTemperature":{"ID":0,"type":41},"devTempAlarmMask":{"ID":16,"type":24},"highTempDwellTripPoint":{"ID":20,"type":34},"highTempThres":{"ID":18,"type":41},"lowTempDwellTripPoint":{"ID":19,"type":34},"lowTempThres":{"ID":17,"type":41},"maxTempExperienced":{"ID":2,"type":41},"minTempExperienced":{"ID":1,"type":41},"overTempTotalDwell":{"ID":3,"type":33}},"commands":{},"commandsResponse":{}},"genGroups":{"ID":4,"attributes":{"nameSupport":{"ID":0,"type":24}},"commands":{"add":{"ID":0,"parameters":[{"name":"groupid","type":33},{"name":"groupname","type":66}],"response":0},"addIfIdentifying":{"ID":5,"parameters":[{"name":"groupid","type":33},{"name":"groupname","type":66}]},"getMembership":{"ID":2,"parameters":[{"name":"groupcount","type":32},{"name":"grouplist","type":1002}],"response":2},"miboxerSetZones":{"ID":240,"parameters":[{"name":"zones","type":1012}]},"remove":{"ID":3,"parameters":[{"name":"groupid","type":33}],"response":3},"removeAll":{"ID":4,"parameters":[]},"view":{"ID":1,"parameters":[{"name":"groupid","type":33}],"response":1}},"commandsResponse":{"addRsp":{"ID":0,"parameters":[{"name":"status","type":32},{"name":"groupid","type":33}]},"getMembershipRsp":{"ID":2,"parameters":[{"name":"capacity","type":32},{"name":"groupcount","type":32},{"name":"grouplist","type":1002}]},"removeRsp":{"ID":3,"parameters":[{"name":"status","type":32},{"name":"groupid","type":33}]},"viewRsp":{"ID":1,"parameters":[{"name":"status","type":32},{"name":"groupid","type":33},{"name":"groupname","type":66}]}}},"genIdentify":{"ID":3,"attributes":{"identifyCommissionState":{"ID":1,"type":255},"identifyTime":{"ID":0,"type":33}},"commands":{"ezmodeInvoke":{"ID":2,"parameters":[{"name":"action","type":32}]},"identify":{"ID":0,"parameters":[{"name":"identifytime","type":33}]},"identifyQuery":{"ID":1,"parameters":[]},"triggerEffect":{"ID":64,"parameters":[{"name":"effectid","type":32},{"name":"effectvariant","type":32}]},"updateCommissionState":{"ID":3,"parameters":[{"name":"action","type":32},{"name":"commstatemask","type":32}]}},"commandsResponse":{"identifyQueryRsp":{"ID":0,"parameters":[{"name":"timeout","type":33}]}}},"genLevelCtrl":{"ID":8,"attributes":{"currentLevel":{"ID":0,"type":32},"defaultMoveRate":{"ID":20,"type":33},"elkoStartUpCurrentLevel":{"ID":16384,"manufacturerCode":4727,"type":32},"maxLevel":{"ID":3,"type":32},"minLevel":{"ID":2,"type":32},"offTransitionTime":{"ID":19,"type":33},"onLevel":{"ID":17,"type":32},"onOffTransitionTime":{"ID":16,"type":33},"onTransitionTime":{"ID":18,"type":33},"options":{"ID":15,"type":24},"remainingTime":{"ID":1,"type":33},"startUpCurrentLevel":{"ID":16384,"type":32}},"commands":{"move":{"ID":1,"parameters":[{"name":"movemode","type":32},{"name":"rate","type":32}]},"moveToLevel":{"ID":0,"parameters":[{"name":"level","type":32},{"name":"transtime","type":33}]},"moveToLevelTuya":{"ID":240,"parameters":[{"name":"level","type":33},{"name":"transtime","type":33}]},"moveToLevelWithOnOff":{"ID":4,"parameters":[{"name":"level","type":32},{"name":"transtime","type":33}]},"moveWithOnOff":{"ID":5,"parameters":[{"name":"movemode","type":32},{"name":"rate","type":32}]},"step":{"ID":2,"parameters":[{"name":"stepmode","type":32},{"name":"stepsize","type":32},{"name":"transtime","type":33}]},"stepWithOnOff":{"ID":6,"parameters":[{"name":"stepmode","type":32},{"name":"stepsize","type":32},{"name":"transtime","type":33}]},"stop":{"ID":3,"parameters":[]},"stopWithOnOff":{"ID":7,"parameters":[]}},"commandsResponse":{}},"genMultistateInput":{"ID":18,"attributes":{"applicationType":{"ID":256,"type":35},"description":{"ID":28,"type":66},"numberOfStates":{"ID":74,"type":33},"outOfService":{"ID":81,"type":16},"presentValue":{"ID":85,"type":33},"reliability":{"ID":103,"type":48},"stateText":{"ID":14,"type":72},"statusFlags":{"ID":111,"type":24}},"commands":{},"commandsResponse":{}},"genMultistateOutput":{"ID":19,"attributes":{"applicationType":{"ID":256,"type":35},"description":{"ID":28,"type":66},"numberOfStates":{"ID":74,"type":33},"outOfService":{"ID":81,"type":16},"presentValue":{"ID":85,"type":33},"priorityArray":{"ID":87,"type":72},"reliability":{"ID":103,"type":48},"relinquishDefault":{"ID":104,"type":33},"stateText":{"ID":14,"type":72},"statusFlags":{"ID":111,"type":24}},"commands":{},"commandsResponse":{}},"genMultistateValue":{"ID":20,"attributes":{"applicationType":{"ID":256,"type":35},"description":{"ID":28,"type":66},"numberOfStates":{"ID":74,"type":33},"outOfService":{"ID":81,"type":16},"presentValue":{"ID":85,"type":33},"priorityArray":{"ID":87,"type":72},"reliability":{"ID":103,"type":48},"relinquishDefault":{"ID":104,"type":33},"stateText":{"ID":14,"type":72},"statusFlags":{"ID":111,"type":24}},"commands":{},"commandsResponse":{}},"genOnOff":{"ID":6,"attributes":{"elkoOnTimeReload":{"ID":57345,"manufacturerCode":4727,"type":35},"elkoOnTimeReloadOptions":{"ID":57346,"manufacturerCode":4727,"type":24},"elkoPreWarningTime":{"ID":57344,"manufacturerCode":4727,"type":33},"globalSceneCtrl":{"ID":16384,"type":16},"moesStartUpOnOff":{"ID":32770,"type":48},"nodonTransitionTime":{"ID":1,"manufacturerCode":4747,"type":33},"offWaitTime":{"ID":16386,"type":33},"onOff":{"ID":0,"type":16},"onTime":{"ID":16385,"type":33},"startUpOnOff":{"ID":16387,"type":48},"tuyaBacklightMode":{"ID":32769,"type":48},"tuyaBacklightSwitch":{"ID":20480,"type":48},"tuyaOperationMode":{"ID":32772,"type":48}},"commands":{"off":{"ID":0,"parameters":[]},"offWithEffect":{"ID":64,"parameters":[{"name":"effectid","type":32},{"name":"effectvariant","type":32}]},"on":{"ID":1,"parameters":[]},"onWithRecallGlobalScene":{"ID":65,"parameters":[]},"onWithTimedOff":{"ID":66,"parameters":[{"name":"ctrlbits","type":32},{"name":"ontime","type":33},{"name":"offwaittime","type":33}]},"toggle":{"ID":2,"parameters":[]},"tuyaAction":{"ID":253,"parameters":[{"name":"value","type":32},{"name":"data","type":1008}]},"tuyaAction2":{"ID":252,"parameters":[{"name":"value","type":32}]}},"commandsResponse":{}},"genOnOffSwitchCfg":{"ID":7,"attributes":{"switchActions":{"ID":16,"type":48},"switchMultiFunction":{"ID":2,"type":255},"switchType":{"ID":0,"type":48}},"commands":{},"commandsResponse":{}},"genOta":{"ID":25,"attributes":{"currentFileVersion":{"ID":2,"type":35},"currentZigbeeStackVersion":{"ID":3,"type":33},"downloadedFileVersion":{"ID":4,"type":35},"downloadedZigbeeStackVersion":{"ID":5,"type":33},"fileOffset":{"ID":1,"type":35},"imageStamp":{"ID":10,"type":35},"imageTypeId":{"ID":8,"type":33},"imageUpgradeStatus":{"ID":6,"type":48},"manufacturerId":{"ID":7,"type":33},"minimumBlockReqDelay":{"ID":9,"type":33},"upgradeServerId":{"ID":0,"type":240}},"commands":{"imageBlockRequest":{"ID":3,"parameters":[{"name":"fieldControl","type":32},{"name":"manufacturerCode","type":33},{"name":"imageType","type":33},{"name":"fileVersion","type":35},{"name":"fileOffset","type":35},{"name":"maximumDataSize","type":32}],"response":5},"imagePageRequest":{"ID":4,"parameters":[{"name":"fieldControl","type":32},{"name":"manufacturerCode","type":33},{"name":"imageType","type":33},{"name":"fileVersion","type":35},{"name":"fileOffset","type":35},{"name":"maximumDataSize","type":32},{"name":"pageSize","type":33},{"name":"responseSpacing","type":33}],"response":5},"queryNextImageRequest":{"ID":1,"parameters":[{"name":"fieldControl","type":32},{"name":"manufacturerCode","type":33},{"name":"imageType","type":33},{"name":"fileVersion","type":35}],"response":2},"upgradeEndRequest":{"ID":6,"parameters":[{"name":"status","type":32},{"name":"manufacturerCode","type":33},{"name":"imageType","type":33},{"name":"fileVersion","type":35}],"response":7}},"commandsResponse":{"imageBlockResponse":{"ID":5,"parameters":[{"name":"status","type":32},{"name":"manufacturerCode","type":33},{"name":"imageType","type":33},{"name":"fileVersion","type":35},{"name":"fileOffset","type":35},{"name":"dataSize","type":32},{"name":"data","type":1008}]},"imageNotify":{"ID":0,"parameters":[{"name":"payloadType","type":32},{"name":"queryJitter","type":32}]},"queryNextImageResponse":{"ID":2,"parameters":[{"name":"status","type":32},{"conditions":[{"type":"statusEquals","value":0}],"name":"manufacturerCode","type":33},{"conditions":[{"type":"statusEquals","value":0}],"name":"imageType","type":33},{"conditions":[{"type":"statusEquals","value":0}],"name":"fileVersion","type":35},{"conditions":[{"type":"statusEquals","value":0}],"name":"imageSize","type":35}]},"upgradeEndResponse":{"ID":7,"parameters":[{"name":"manufacturerCode","type":33},{"name":"imageType","type":33},{"name":"fileVersion","type":35},{"name":"currentTime","type":35},{"name":"upgradeTime","type":35}]}}},"genPollCtrl":{"ID":32,"attributes":{"checkinInterval":{"ID":0,"type":35},"checkinIntervalMin":{"ID":4,"type":35},"fastPollTimeout":{"ID":3,"type":33},"fastPollTimeoutMax":{"ID":6,"type":33},"longPollInterval":{"ID":1,"type":35},"longPollIntervalMin":{"ID":5,"type":35},"shortPollInterval":{"ID":2,"type":33}},"commands":{"checkinRsp":{"ID":0,"parameters":[{"name":"startFastPolling","type":16},{"name":"fastPollTimeout","type":33}]},"fastPollStop":{"ID":1,"parameters":[]},"setLongPollInterval":{"ID":2,"parameters":[{"name":"newLongPollInterval","type":35}]},"setShortPollInterval":{"ID":3,"parameters":[{"name":"newShortPollInterval","type":33}]}},"commandsResponse":{"checkin":{"ID":0,"parameters":[]}}},"genPowerCfg":{"ID":1,"attributes":{"batteryAHrRating":{"ID":50,"type":33},"batteryAlarmMask":{"ID":53,"type":24},"batteryAlarmState":{"ID":62,"type":27},"batteryManufacturer":{"ID":48,"type":66},"batteryPercentMinThres":{"ID":58,"type":32},"batteryPercentThres1":{"ID":59,"type":32},"batteryPercentThres2":{"ID":60,"type":32},"batteryPercentThres3":{"ID":61,"type":32},"batteryPercentageRemaining":{"ID":33,"type":32},"batteryQuantity":{"ID":51,"type":32},"batteryRatedVoltage":{"ID":52,"type":32},"batterySize":{"ID":49,"type":48},"batteryVoltMinThres":{"ID":54,"type":32},"batteryVoltThres1":{"ID":55,"type":32},"batteryVoltThres2":{"ID":56,"type":32},"batteryVoltThres3":{"ID":57,"type":32},"batteryVoltage":{"ID":32,"type":32},"mainsAlarmMask":{"ID":16,"type":24},"mainsFrequency":{"ID":1,"type":32},"mainsVoltMaxThres":{"ID":18,"type":33},"mainsVoltMinThres":{"ID":17,"type":33},"mainsVoltage":{"ID":0,"type":33},"mainsVoltageDwellTripPoint":{"ID":19,"type":33}},"commands":{},"commandsResponse":{}},"genRssiLocation":{"ID":11,"attributes":{"age":{"ID":2,"type":33},"calcPeriod":{"ID":22,"type":33},"coordinate1":{"ID":16,"type":41},"coordinate2":{"ID":17,"type":41},"coordinate3":{"ID":18,"type":41},"method":{"ID":1,"type":48},"numOfDevices":{"ID":4,"type":32},"numRSSIMeasurements":{"ID":23,"type":33},"pathLossExponent":{"ID":20,"type":33},"power":{"ID":19,"type":41},"qualityMeasure":{"ID":3,"type":32},"reportingPeriod":{"ID":21,"type":33},"type":{"ID":0,"type":8}},"commands":{"getData":{"ID":3,"parameters":[{"name":"getdatainfo","type":32},{"name":"numrsp","type":32},{"name":"targetaddr","type":240}]},"getDevCfg":{"ID":2,"parameters":[{"name":"targetaddr","type":240}]},"setAbsolute":{"ID":0,"parameters":[{"name":"coord1","type":41},{"name":"coord2","type":41},{"name":"coord3","type":41},{"name":"power","type":41},{"name":"pathlossexponent","type":33}]},"setDevCfg":{"ID":1,"parameters":[{"name":"power","type":41},{"name":"pathlossexponent","type":33},{"name":"calperiod","type":33},{"name":"numrssimeasurements","type":32},{"name":"reportingperiod","type":33}]}},"commandsResponse":{"compactDataNotif":{"ID":3,"parameters":[{"name":"locationtype","type":32},{"name":"coord1","type":41},{"name":"coord2","type":41},{"name":"coord3","type":41},{"name":"qualitymeasure","type":32},{"name":"locationage","type":33}]},"dataNotif":{"ID":2,"parameters":[{"name":"locationtype","type":32},{"name":"coord1","type":41},{"name":"coord2","type":41},{"name":"coord3","type":41},{"name":"power","type":41},{"name":"pathlossexp","type":33},{"name":"locationmethod","type":32},{"name":"qualitymeasure","type":32},{"name":"locationage","type":33}]},"dataRsp":{"ID":1,"parameters":[{"name":"status","type":32},{"name":"locationtype","type":32},{"name":"coord1","type":41},{"name":"coord2","type":41},{"name":"coord3","type":41},{"name":"power","type":41},{"name":"pathlossexp","type":33},{"name":"locationmethod","type":32},{"name":"qualitymeasure","type":32},{"name":"locationage","type":33}]},"devCfgRsp":{"ID":0,"parameters":[{"name":"status","type":32},{"name":"power","type":41},{"name":"pathlossexp","type":33},{"name":"calperiod","type":33},{"name":"numrssimeasurements","type":32},{"name":"reportingperiod","type":33}]},"rssiPing":{"ID":4,"parameters":[{"name":"locationtype","type":32}]}}},"genScenes":{"ID":5,"attributes":{"count":{"ID":0,"type":32},"currentGroup":{"ID":2,"type":33},"currentScene":{"ID":1,"type":32},"lastCfgBy":{"ID":5,"type":240},"nameSupport":{"ID":4,"type":24},"sceneValid":{"ID":3,"type":16}},"commands":{"add":{"ID":0,"parameters":[{"name":"groupid","type":33},{"name":"sceneid","type":32},{"name":"transtime","type":33},{"name":"scenename","type":66},{"name":"extensionfieldsets","type":1006}],"response":0},"copy":{"ID":66,"parameters":[{"name":"mode","type":32},{"name":"groupidfrom","type":33},{"name":"sceneidfrom","type":32},{"name":"groupidto","type":33},{"name":"sceneidto","type":32}],"response":66},"enhancedAdd":{"ID":64,"parameters":[{"name":"groupid","type":33},{"name":"sceneid","type":32},{"name":"transtime","type":33},{"name":"scenename","type":66},{"name":"extensionfieldsets","type":1006}],"response":64},"enhancedView":{"ID":65,"parameters":[{"name":"groupid","type":33},{"name":"sceneid","type":32}],"response":65},"getSceneMembership":{"ID":6,"parameters":[{"name":"groupid","type":33}],"response":6},"recall":{"ID":5,"parameters":[{"name":"groupid","type":33},{"name":"sceneid","type":32}]},"remove":{"ID":2,"parameters":[{"name":"groupid","type":33},{"name":"sceneid","type":32}],"response":2},"removeAll":{"ID":3,"parameters":[{"name":"groupid","type":33}],"response":3},"store":{"ID":4,"parameters":[{"name":"groupid","type":33},{"name":"sceneid","type":32}],"response":4},"tradfriArrowHold":{"ID":8,"parameters":[{"name":"value","type":33}]},"tradfriArrowRelease":{"ID":9,"parameters":[{"name":"value","type":33}]},"tradfriArrowSingle":{"ID":7,"parameters":[{"name":"value","type":33},{"name":"value2","type":33}]},"view":{"ID":1,"parameters":[{"name":"groupid","type":33},{"name":"sceneid","type":32}],"response":1}},"commandsResponse":{"addRsp":{"ID":0,"parameters":[{"name":"status","type":32},{"name":"groupId","type":33},{"name":"sceneId","type":32}]},"copyRsp":{"ID":66,"parameters":[{"name":"status","type":32},{"name":"groupidfrom","type":33},{"name":"sceneidfrom","type":32}]},"enhancedAddRsp":{"ID":64,"parameters":[{"name":"status","type":32},{"name":"groupId","type":33},{"name":"sceneId","type":32}]},"enhancedViewRsp":{"ID":65,"parameters":[{"name":"status","type":32},{"name":"groupid","type":33},{"name":"sceneid","type":32},{"conditions":[{"type":"statusEquals","value":0}],"name":"transtime","type":33},{"conditions":[{"type":"statusEquals","value":0}],"name":"scenename","type":66},{"conditions":[{"type":"statusEquals","value":0}],"name":"extensionfieldsets","type":1006}]},"getSceneMembershipRsp":{"ID":6,"parameters":[{"name":"status","type":32},{"name":"capacity","type":32},{"name":"groupid","type":33},{"conditions":[{"type":"statusEquals","value":0}],"name":"scenecount","type":32},{"conditions":[{"type":"statusEquals","value":0}],"name":"scenelist","type":1001}]},"removeAllRsp":{"ID":3,"parameters":[{"name":"status","type":32},{"name":"groupid","type":33}]},"removeRsp":{"ID":2,"parameters":[{"name":"status","type":32},{"name":"groupid","type":33},{"name":"sceneid","type":32}]},"storeRsp":{"ID":4,"parameters":[{"name":"status","type":32},{"name":"groupid","type":33},{"name":"sceneid","type":32}]},"viewRsp":{"ID":1,"parameters":[{"name":"status","type":32},{"name":"groupid","type":33},{"name":"sceneid","type":32},{"conditions":[{"type":"statusEquals","value":0}],"name":"transtime","type":33},{"conditions":[{"type":"statusEquals","value":0}],"name":"scenename","type":66},{"conditions":[{"type":"statusEquals","value":0}],"name":"extensionfieldsets","type":1006}]}}},"genTime":{"ID":10,"attributes":{"dstEnd":{"ID":4,"type":35},"dstShift":{"ID":5,"type":43},"dstStart":{"ID":3,"type":35},"lastSetTime":{"ID":8,"type":226},"localTime":{"ID":7,"type":35},"standardTime":{"ID":6,"type":35},"time":{"ID":0,"type":226},"timeStatus":{"ID":1,"type":24},"timeZone":{"ID":2,"type":43},"validUntilTime":{"ID":9,"type":226}},"commands":{},"commandsResponse":{}},"greenPower":{"ID":33,"attributes":{},"commands":{"commissioningNotification":{"ID":4,"parameters":[{"name":"options","type":33},{"conditions":[{"offset":0,"param":"options","size":3,"type":"bitFieldEnum","value":0}],"name":"srcID","type":35},{"conditions":[{"offset":0,"param":"options","size":3,"type":"bitFieldEnum","value":2}],"name":"gpdIEEEAddr","type":240},{"conditions":[{"offset":0,"param":"options","size":3,"type":"bitFieldEnum","value":2}],"name":"gpdEndpoint","type":32},{"name":"frameCounter","type":35},{"name":"commandID","type":32},{"name":"payloadSize","type":32},{"name":"commandFrame","type":1009},{"conditions":[{"mask":2048,"param":"options","type":"bitMaskSet"}],"name":"gppNwkAddr","type":33},{"conditions":[{"mask":2048,"param":"options","type":"bitMaskSet"}],"name":"gppGddLink","type":32}]},"notification":{"ID":0,"parameters":[{"name":"options","type":33},{"conditions":[{"offset":0,"param":"options","size":3,"type":"bitFieldEnum","value":0}],"name":"srcID","type":35},{"conditions":[{"offset":0,"param":"options","size":3,"type":"bitFieldEnum","value":2}],"name":"gpdIEEEAddr","type":240},{"conditions":[{"offset":0,"param":"options","size":3,"type":"bitFieldEnum","value":2}],"name":"gpdEndpoint","type":32},{"name":"frameCounter","type":35},{"name":"commandID","type":32},{"name":"payloadSize","type":32},{"name":"commandFrame","type":1009},{"conditions":[{"mask":16384,"param":"options","type":"bitMaskSet"}],"name":"gppNwkAddr","type":33},{"conditions":[{"mask":16384,"param":"options","type":"bitMaskSet"}],"name":"gppGddLink","type":32}]}},"commandsResponse":{"commisioningMode":{"ID":2,"parameters":[{"name":"options","type":32},{"name":"commisioningWindow","type":33}]},"pairing":{"ID":1,"parameters":[{"name":"options","type":34},{"conditions":[{"offset":0,"param":"options","size":3,"type":"bitFieldEnum","value":0}],"name":"srcID","type":35},{"conditions":[{"offset":0,"param":"options","size":3,"type":"bitFieldEnum","value":2}],"name":"gpdIEEEAddr","type":240},{"conditions":[{"offset":0,"param":"options","size":3,"type":"bitFieldEnum","value":2}],"name":"gpdEndpoint","type":32},{"conditions":[{"offset":4,"param":"options","size":3,"type":"bitFieldEnum","value":6}],"name":"sinkIEEEAddr","type":240},{"conditions":[{"offset":4,"param":"options","size":3,"type":"bitFieldEnum","value":0}],"name":"sinkIEEEAddr","type":240},{"conditions":[{"offset":4,"param":"options","size":3,"type":"bitFieldEnum","value":6}],"name":"sinkNwkAddr","type":33},{"conditions":[{"offset":4,"param":"options","size":3,"type":"bitFieldEnum","value":0}],"name":"sinkNwkAddr","type":33},{"conditions":[{"offset":4,"param":"options","size":3,"type":"bitFieldEnum","value":4}],"name":"sinkGroupID","type":33},{"conditions":[{"offset":4,"param":"options","size":3,"type":"bitFieldEnum","value":2}],"name":"sinkGroupID","type":33},{"conditions":[{"mask":8,"param":"options","type":"bitMaskSet"}],"name":"deviceID","type":32},{"conditions":[{"mask":16384,"param":"options","type":"bitMaskSet"}],"name":"frameCounter","type":35},{"conditions":[{"mask":32768,"param":"options","type":"bitMaskSet"}],"name":"gpdKey","type":241}]},"response":{"ID":6,"parameters":[{"name":"options","type":32},{"name":"tempMaster","type":33},{"name":"tempMasterTx","type":32},{"conditions":[{"offset":0,"param":"options","size":3,"type":"bitFieldEnum","value":0}],"name":"srcID","type":35},{"conditions":[{"offset":0,"param":"options","size":3,"type":"bitFieldEnum","value":2}],"name":"gpdIEEEAddr","type":240},{"conditions":[{"offset":0,"param":"options","size":3,"type":"bitFieldEnum","value":2}],"name":"gpdEndpoint","type":32},{"name":"gpdCmd","type":32},{"name":"gpdPayload","type":1009}]}}},"haApplianceEventsAlerts":{"ID":2818,"attributes":{},"commands":{"getAlerts":{"ID":0,"parameters":[]}},"commandsResponse":{"alertsNotification":{"ID":1,"parameters":[{"name":"alertscount","type":32},{"name":"aalert","type":1003}]},"eventNotification":{"ID":2,"parameters":[{"name":"eventheader","type":32},{"name":"eventid","type":32}]},"getAlertsRsp":{"ID":0,"parameters":[{"name":"alertscount","type":32},{"name":"aalert","type":1003}]}}},"haApplianceIdentification":{"ID":2816,"attributes":{"basicIdentification":{"ID":0,"type":38},"brandId":{"ID":19,"type":33},"brandName":{"ID":18,"type":66},"cecedSpecificationVersion":{"ID":26,"type":32},"companyId":{"ID":17,"type":33},"companyName":{"ID":16,"type":66},"model":{"ID":20,"type":65},"partNumber":{"ID":21,"type":65},"productRevision":{"ID":22,"type":65},"productTypeId":{"ID":25,"type":33},"productTypeName":{"ID":24,"type":65},"softwareRevision":{"ID":23,"type":65}},"commands":{},"commandsResponse":{}},"haApplianceStatistics":{"ID":2819,"attributes":{"logMaxSize":{"ID":0,"type":35},"logQueueMaxSize":{"ID":1,"type":32}},"commands":{"log":{"ID":0,"parameters":[{"name":"logid","type":35}]},"logQueue":{"ID":1,"parameters":[]}},"commandsResponse":{"logNotification":{"ID":0,"parameters":[{"name":"timestamp","type":35},{"name":"logid","type":35},{"name":"loglength","type":35},{"name":"logpayload","type":1001}]},"logQueueRsp":{"ID":2,"parameters":[{"name":"logqueuesize","type":32},{"name":"logid","type":1004}]},"logRsp":{"ID":1,"parameters":[{"name":"timestamp","type":35},{"name":"logid","type":35},{"name":"loglength","type":35},{"name":"logpayload","type":1001}]},"statisticsAvailable":{"ID":3,"parameters":[{"name":"logqueuesize","type":32},{"name":"logid","type":1004}]}}},"haDiagnostic":{"ID":2821,"attributes":{"aPSRxBcast":{"ID":262,"type":33},"aPSRxUcast":{"ID":264,"type":33},"aPSTxBcast":{"ID":263,"type":33},"aPSTxUcastFail":{"ID":267,"type":33},"aPSTxUcastRetry":{"ID":266,"type":33},"aPSTxUcastSuccess":{"ID":265,"type":33},"apsDecryptFailures":{"ID":278,"type":33},"apsFcFailure":{"ID":275,"type":33},"apsUnauthorizedKey":{"ID":276,"type":33},"averageMacRetryPerApsMessageSent":{"ID":283,"type":33},"childMoved":{"ID":273,"type":33},"danfossMultimasterRole":{"ID":16897,"manufacturerCode":4678,"type":48},"danfossSystemStatusCode":{"ID":16384,"manufacturerCode":4678,"type":25},"danfossSystemStatusWater":{"ID":16896,"manufacturerCode":4678,"type":48},"joinIndication":{"ID":272,"type":33},"lastMessageLqi":{"ID":284,"type":32},"lastMessageRssi":{"ID":285,"type":40},"macRxBcast":{"ID":256,"type":35},"macRxUcast":{"ID":258,"type":35},"macTxBcast":{"ID":257,"type":35},"macTxUcast":{"ID":259,"type":35},"macTxUcastFail":{"ID":261,"type":33},"macTxUcastRetry":{"ID":260,"type":33},"neighborAdded":{"ID":269,"type":33},"neighborRemoved":{"ID":270,"type":33},"neighborStale":{"ID":271,"type":33},"numberOfResets":{"ID":0,"type":33},"nwkDecryptFailures":{"ID":277,"type":33},"nwkFcFailure":{"ID":274,"type":33},"packetBufferAllocateFailures":{"ID":279,"type":33},"packetValidateDropCount":{"ID":282,"type":33},"persistentMemoryWrites":{"ID":1,"type":33},"phyToMacQueueLimitReached":{"ID":281,"type":33},"relayedUcast":{"ID":280,"type":33},"routeDiscInitiated":{"ID":268,"type":33},"schneiderCommunicationQuality":{"ID":16384,"manufacturerCode":4190,"type":32},"schneiderDiagnosticRegister1":{"ID":65282,"manufacturerCode":4190,"type":35},"schneiderMeterStatus":{"ID":65281,"manufacturerCode":4190,"type":35}},"commands":{},"commandsResponse":{}},"haElectricalMeasurement":{"ID":2820,"attributes":{"acActivePowerOverload":{"ID":2051,"type":41},"acAlarmsMask":{"ID":2048,"type":25},"acCurrentDivisor":{"ID":1539,"type":33},"acCurrentMultiplier":{"ID":1538,"type":33},"acCurrentOverload":{"ID":2050,"type":41},"acFrequency":{"ID":768,"type":33},"acFrequencyDivisor":{"ID":1025,"type":33},"acFrequencyMax":{"ID":770,"type":33},"acFrequencyMin":{"ID":769,"type":33},"acFrequencyMultiplier":{"ID":1024,"type":33},"acPowerDivisor":{"ID":1541,"type":33},"acPowerMultiplier":{"ID":1540,"type":33},"acReactivePowerOverload":{"ID":2052,"type":41},"acVoltageDivisor":{"ID":1537,"type":33},"acVoltageMultiplier":{"ID":1536,"type":33},"acVoltageOverload":{"ID":2049,"type":41},"activeCurrentPhB":{"ID":2306,"type":41},"activeCurrentPhC":{"ID":2562,"type":41},"activePower":{"ID":1291,"type":41},"activePowerMax":{"ID":1293,"type":41},"activePowerMaxPhB":{"ID":2317,"type":41},"activePowerMaxPhC":{"ID":2573,"type":41},"activePowerMin":{"ID":1292,"type":41},"activePowerMinPhB":{"ID":2316,"type":41},"activePowerMinPhC":{"ID":2572,"type":41},"activePowerPhB":{"ID":2315,"type":41},"activePowerPhC":{"ID":2571,"type":41},"apparentPower":{"ID":1295,"type":33},"apparentPowerPhB":{"ID":2319,"type":33},"apparentPowerPhC":{"ID":2575,"type":33},"averageRmsOverVoltage":{"ID":2053,"type":41},"averageRmsOverVoltageCounter":{"ID":1298,"type":33},"averageRmsOverVoltageCounterPhB":{"ID":2322,"type":33},"averageRmsOverVoltageCounterPhC":{"ID":2578,"type":33},"averageRmsUnderVoltage":{"ID":2054,"type":41},"averageRmsUnderVoltageCounter":{"ID":1299,"type":33},"averageRmsVoltageMeasPeriod":{"ID":1297,"type":33},"averageRmsVoltageMeasPeriodPhC":{"ID":2577,"type":33},"averageRmsVoltageMeasurePeriodPhB":{"ID":2321,"type":33},"averageUnderVoltageCounterPhB":{"ID":2323,"type":33},"averageUnderVoltageCounterPhC":{"ID":2579,"type":33},"dcCurrent":{"ID":259,"type":41},"dcCurrentDivisor":{"ID":515,"type":33},"dcCurrentMax":{"ID":261,"type":41},"dcCurrentMin":{"ID":260,"type":41},"dcCurrentMultiplier":{"ID":514,"type":33},"dcCurrentOverload":{"ID":1794,"type":41},"dcOverloadAlarmsMask":{"ID":1792,"type":24},"dcPower":{"ID":262,"type":41},"dcPowerDivisor":{"ID":517,"type":33},"dcPowerMax":{"ID":264,"type":41},"dcPowerMin":{"ID":263,"type":41},"dcPowerMultiplier":{"ID":516,"type":33},"dcVoltage":{"ID":256,"type":41},"dcVoltageDivisor":{"ID":513,"type":33},"dcVoltageMin":{"ID":257,"type":41},"dcVoltageMultiplier":{"ID":512,"type":33},"dcVoltageOverload":{"ID":1793,"type":41},"dcvoltagemax":{"ID":258,"type":41},"harmonicCurrentMultiplier":{"ID":1028,"type":40},"instantaneousActiveCurrent":{"ID":1282,"type":41},"instantaneousLineCurrent":{"ID":1281,"type":33},"instantaneousPower":{"ID":1284,"type":41},"instantaneousReactiveCurrent":{"ID":1283,"type":41},"instantaneousVoltage":{"ID":1280,"type":41},"lineCurrentPhB":{"ID":2305,"type":33},"lineCurrentPhC":{"ID":2561,"type":33},"meas11thHarmonicCurrent":{"ID":780,"type":41},"meas1stHarmonicCurrent":{"ID":775,"type":41},"meas3rdHarmonicCurrent":{"ID":776,"type":41},"meas5thHarmonicCurrent":{"ID":777,"type":41},"meas7thHarmonicCurrent":{"ID":778,"type":41},"meas9thHarmonicCurrent":{"ID":779,"type":41},"measPhase11thHarmonicCurrent":{"ID":786,"type":41},"measPhase1stHarmonicCurrent":{"ID":781,"type":41},"measPhase3rdHarmonicCurrent":{"ID":782,"type":41},"measPhase5thHarmonicCurrent":{"ID":783,"type":41},"measPhase7thHarmonicCurrent":{"ID":784,"type":41},"measPhase9thHarmonicCurrent":{"ID":785,"type":41},"measurementType":{"ID":0,"type":27},"neutralCurrent":{"ID":771,"type":33},"phaseHarmonicCurrentMultiplier":{"ID":1029,"type":40},"powerDivisor":{"ID":1027,"type":35},"powerFactor":{"ID":1296,"type":40},"powerFactorPhB":{"ID":2320,"type":40},"powerFactorPhC":{"ID":2576,"type":40},"powerMultiplier":{"ID":1026,"type":35},"reactiveCurrentPhB":{"ID":2307,"type":41},"reactiveCurrentPhC":{"ID":2563,"type":41},"reactivePower":{"ID":1294,"type":41},"reactivePowerPhB":{"ID":2318,"type":41},"reactivePowerPhC":{"ID":2574,"type":41},"rmsCurrent":{"ID":1288,"type":33},"rmsCurrentMax":{"ID":1290,"type":33},"rmsCurrentMaxPhB":{"ID":2314,"type":33},"rmsCurrentMaxPhC":{"ID":2570,"type":33},"rmsCurrentMin":{"ID":1289,"type":33},"rmsCurrentMinPhB":{"ID":2313,"type":33},"rmsCurrentMinPhC":{"ID":2569,"type":33},"rmsCurrentPhB":{"ID":2312,"type":33},"rmsCurrentPhC":{"ID":2568,"type":33},"rmsExtremeOverVoltage":{"ID":2055,"type":41},"rmsExtremeOverVoltagePeriod":{"ID":1300,"type":33},"rmsExtremeOverVoltagePeriodPhB":{"ID":2324,"type":33},"rmsExtremeOverVoltagePeriodPhC":{"ID":2580,"type":33},"rmsExtremeUnderVoltage":{"ID":2056,"type":41},"rmsExtremeUnderVoltagePeriod":{"ID":1301,"type":33},"rmsExtremeUnderVoltagePeriodPhB":{"ID":2325,"type":33},"rmsExtremeUnderVoltagePeriodPhC":{"ID":2581,"type":33},"rmsVoltage":{"ID":1285,"type":33},"rmsVoltageMax":{"ID":1287,"type":33},"rmsVoltageMaxPhB":{"ID":2311,"type":33},"rmsVoltageMaxPhC":{"ID":2567,"type":33},"rmsVoltageMin":{"ID":1286,"type":33},"rmsVoltageMinPhB":{"ID":2310,"type":33},"rmsVoltageMinPhC":{"ID":2566,"type":33},"rmsVoltagePhB":{"ID":2309,"type":33},"rmsVoltagePhC":{"ID":2565,"type":33},"rmsVoltageSag":{"ID":2057,"type":41},"rmsVoltageSagPeriod":{"ID":1302,"type":33},"rmsVoltageSagPeriodPhB":{"ID":2326,"type":33},"rmsVoltageSagPeriodPhC":{"ID":2582,"type":33},"rmsVoltageSwell":{"ID":2058,"type":41},"rmsVoltageSwellPeriod":{"ID":1303,"type":33},"rmsVoltageSwellPeriodPhB":{"ID":2327,"type":33},"rmsVoltageSwellPeriodPhC":{"ID":2583,"type":33},"schneiderActivePowerDemandPhase1":{"ID":17673,"manufacturerCode":4190,"type":43},"schneiderActivePowerDemandPhase2":{"ID":18697,"manufacturerCode":4190,"type":43},"schneiderActivePowerDemandPhase3":{"ID":18953,"manufacturerCode":4190,"type":43},"schneiderActivePowerDemandTotal":{"ID":17152,"manufacturerCode":4190,"type":43},"schneiderApparentPowerDemandPhase1":{"ID":17675,"manufacturerCode":4190,"type":43},"schneiderApparentPowerDemandPhase2":{"ID":18699,"manufacturerCode":4190,"type":43},"schneiderApparentPowerDemandPhase3":{"ID":18955,"manufacturerCode":4190,"type":43},"schneiderApparentPowerDemandTotal":{"ID":17176,"manufacturerCode":4190,"type":43},"schneiderCurrentSensorMultiplier":{"ID":19968,"manufacturerCode":4190,"type":32},"schneiderDemandDateTime":{"ID":17184,"manufacturerCode":4190,"type":226},"schneiderDemandIntervalDuration":{"ID":17177,"manufacturerCode":4190,"type":34},"schneiderDemandIntervalMaximalCurrentI1":{"ID":17683,"manufacturerCode":4190,"type":33},"schneiderDemandIntervalMaximalCurrentI2":{"ID":18707,"manufacturerCode":4190,"type":33},"schneiderDemandIntervalMaximalCurrentI3":{"ID":18963,"manufacturerCode":4190,"type":33},"schneiderDemandIntervalMinimalVoltageL1":{"ID":17680,"manufacturerCode":4190,"type":33},"schneiderDemandIntervalMinimalVoltageL2":{"ID":18704,"manufacturerCode":4190,"type":33},"schneiderDemandIntervalMinimalVoltageL3":{"ID":18960,"manufacturerCode":4190,"type":33},"schneiderReactivePowerDemandPhase1":{"ID":17674,"manufacturerCode":4190,"type":43},"schneiderReactivePowerDemandPhase2":{"ID":18698,"manufacturerCode":4190,"type":43},"schneiderReactivePowerDemandPhase3":{"ID":18954,"manufacturerCode":4190,"type":43},"schneiderReactivePowerDemandTotal":{"ID":17155,"manufacturerCode":4190,"type":43},"totalActivePower":{"ID":772,"type":43},"totalApparentPower":{"ID":774,"type":35},"totalReactivePower":{"ID":773,"type":43}},"commands":{"getMeasurementProfile":{"ID":1,"parameters":[{"name":"attrId","type":33},{"name":"starttime","type":35},{"name":"numofuntervals","type":32}]},"getProfileInfo":{"ID":0,"parameters":[]}},"commandsResponse":{"getMeasurementProfileRsp":{"ID":1,"parameters":[{"name":"starttime","type":35},{"name":"status","type":32},{"name":"profileintervalperiod","type":32},{"name":"numofintervalsdeliv","type":32},{"name":"attrId","type":33},{"name":"intervals","type":1001}]},"getProfileInfoRsp":{"ID":0,"parameters":[{"name":"profilecount","type":32},{"name":"profileintervalperiod","type":32},{"name":"maxnumofintervals","type":32},{"name":"numofattrs","type":32},{"name":"listofattr","type":1002}]}}},"haMeterIdentification":{"ID":2817,"attributes":{"availablePower":{"ID":13,"type":42},"companyName":{"ID":0,"type":66},"customerName":{"ID":5,"type":66},"dataQualityId":{"ID":4,"type":33},"meterTypeId":{"ID":1,"type":33},"model":{"ID":6,"type":66},"partNumber":{"ID":7,"type":66},"pod":{"ID":12,"type":66},"powerThreshold":{"ID":14,"type":42},"productRevision":{"ID":8,"type":66},"softwareRevision":{"ID":10,"type":66},"utilityName":{"ID":11,"type":66}},"commands":{},"commandsResponse":{}},"heimanSpecificAirQuality":{"ID":64641,"attributes":{"alarmEnable":{"ID":61450,"type":33},"aqiMeasuredValue":{"ID":61445,"type":33},"batteryState":{"ID":61442,"type":32},"humidityMeasuredMax":{"ID":61448,"type":33},"humidityMeasuredMin":{"ID":61449,"type":33},"language":{"ID":61440,"type":32},"pm10measuredValue":{"ID":61443,"type":33},"temperatureMeasuredMax":{"ID":61446,"type":41},"temperatureMeasuredMin":{"ID":61447,"type":41},"tvocMeasuredValue":{"ID":61444,"type":33},"unitOfMeasure":{"ID":61441,"type":32}},"commands":{"getTime":{"ID":285,"parameters":[]},"setLanguage":{"ID":283,"parameters":[{"name":"languageCode","type":32}]},"setUnitOfTemperature":{"ID":284,"parameters":[{"name":"unitsCode","type":32}]}},"commandsResponse":{},"manufacturerCode":4619},"heimanSpecificInfraRedRemote":{"ID":64642,"attributes":{},"commands":{"createId":{"ID":244,"parameters":[{"name":"modelType","type":32}]},"deleteKey":{"ID":243,"parameters":[{"name":"id","type":32},{"name":"keyCode","type":32}]},"getIdAndKeyCodeList":{"ID":246,"parameters":[]},"sendKey":{"ID":240,"parameters":[{"name":"id","type":32},{"name":"keyCode","type":32}]},"studyKey":{"ID":241,"parameters":[{"name":"id","type":32},{"name":"keyCode","type":32}]}},"commandsResponse":{"createIdRsp":{"ID":245,"parameters":[{"name":"id","type":32},{"name":"modelType","type":32}]},"getIdAndKeyCodeListRsp":{"ID":247,"parameters":[{"name":"packetsTotal","type":32},{"name":"packetNumber","type":32},{"name":"packetLength","type":32},{"name":"learnedDevicesList","type":1001}]},"studyKeyRsp":{"ID":242,"parameters":[{"name":"id","type":32},{"name":"keyCode","type":32},{"name":"result","type":32}]}},"manufacturerCode":4619},"heimanSpecificScenes":{"ID":64640,"attributes":{},"commands":{"atHome":{"ID":241,"parameters":[]},"cinema":{"ID":240,"parameters":[]},"goOut":{"ID":243,"parameters":[]},"repast":{"ID":244,"parameters":[]},"sleep":{"ID":242,"parameters":[]}},"commandsResponse":{},"manufacturerCode":4619},"hvacDehumidificationCtrl":{"ID":515,"attributes":{"dehumidCooling":{"ID":1,"type":32},"dehumidHysteresis":{"ID":19,"type":32},"dehumidLockout":{"ID":18,"type":48},"dehumidMaxCool":{"ID":20,"type":32},"relativeHumidDisplay":{"ID":21,"type":48},"relativeHumidity":{"ID":0,"type":32},"relativeHumidityMode":{"ID":17,"type":48},"rhDehumidSetpoint":{"ID":16,"type":32}},"commands":{},"commandsResponse":{}},"hvacFanCtrl":{"ID":514,"attributes":{"fanMode":{"ID":0,"type":48},"fanModeSequence":{"ID":1,"type":48}},"commands":{},"commandsResponse":{}},"hvacPumpCfgCtrl":{"ID":512,"attributes":{"alarmMask":{"ID":34,"type":25},"capacity":{"ID":19,"type":41},"controlMode":{"ID":33,"type":48},"effectiveControlMode":{"ID":18,"type":48},"effectiveOperationMode":{"ID":17,"type":48},"lifetimeEnergyConsumed":{"ID":23,"type":35},"lifetimeRunningHours":{"ID":21,"type":34},"maxCompPressure":{"ID":6,"type":41},"maxConstFlow":{"ID":10,"type":33},"maxConstPressure":{"ID":4,"type":41},"maxConstSpeed":{"ID":8,"type":33},"maxConstTemp":{"ID":12,"type":41},"maxFlow":{"ID":2,"type":33},"maxPressure":{"ID":0,"type":41},"maxSpeed":{"ID":1,"type":33},"minCompPressure":{"ID":5,"type":41},"minConstFlow":{"ID":9,"type":33},"minConstPressure":{"ID":3,"type":41},"minConstSpeed":{"ID":7,"type":33},"minConstTemp":{"ID":11,"type":41},"operationMode":{"ID":32,"type":48},"power":{"ID":22,"type":34},"pumpStatus":{"ID":16,"type":25},"speed":{"ID":20,"type":33}},"commands":{},"commandsResponse":{}},"hvacThermostat":{"ID":513,"attributes":{"SinopeAuxCycleOutput":{"ID":1028,"manufacturerCode":4508,"type":33},"SinopeBacklight":{"ID":1026,"manufacturerCode":4508,"type":48},"SinopeMainCycleOutput":{"ID":1025,"manufacturerCode":4508,"type":33},"SinopeOccupancy":{"ID":1024,"manufacturerCode":4508,"type":48},"StelproOutdoorTemp":{"ID":16385,"type":41},"StelproSystemMode":{"ID":16412,"type":48},"absMaxCoolSetpointLimit":{"ID":6,"type":41},"absMaxHeatSetpointLimit":{"ID":4,"type":41},"absMinCoolSetpointLimit":{"ID":5,"type":41},"absMinHeatSetpointLimit":{"ID":3,"type":41},"acCapacity":{"ID":65,"type":33},"acCapacityFormat":{"ID":71,"type":48},"acCollTemp":{"ID":70,"type":41},"acConpressorType":{"ID":67,"type":48},"acErrorCode":{"ID":68,"type":27},"acLouverPosition":{"ID":69,"type":48},"acRefrigerantType":{"ID":66,"type":48},"acType":{"ID":64,"type":48},"alarmMask":{"ID":29,"type":24},"ctrlSeqeOfOper":{"ID":27,"type":48},"danfossAdaptionRunControl":{"ID":16460,"manufacturerCode":4678,"type":48},"danfossAdaptionRunSettings":{"ID":16462,"manufacturerCode":4678,"type":24},"danfossAdaptionRunStatus":{"ID":16461,"manufacturerCode":4678,"type":24},"danfossAlgorithmScaleFactor":{"ID":16416,"manufacturerCode":4678,"type":32},"danfossDayOfWeek":{"ID":16400,"manufacturerCode":4678,"type":48},"danfossExternalMeasuredRoomSensor":{"ID":16405,"manufacturerCode":4678,"type":41},"danfossFloorMaxSetpoint":{"ID":16674,"manufacturerCode":4678,"type":41},"danfossFloorMinSetpoint":{"ID":16673,"manufacturerCode":4678,"type":41},"danfossHeatAvailable":{"ID":16432,"manufacturerCode":4678,"type":16},"danfossHeatRequired":{"ID":16433,"manufacturerCode":4678,"type":16},"danfossLoadBalancingEnable":{"ID":16434,"manufacturerCode":4678,"type":16},"danfossLoadEstimate":{"ID":16458,"manufacturerCode":4678,"type":41},"danfossLoadRoomMean":{"ID":16448,"manufacturerCode":4678,"type":41},"danfossMountedModeActive":{"ID":16402,"manufacturerCode":4678,"type":16},"danfossMountedModeControl":{"ID":16403,"manufacturerCode":4678,"type":16},"danfossOutputStatus":{"ID":16656,"manufacturerCode":4678,"type":48},"danfossPreheatStatus":{"ID":16463,"manufacturerCode":4678,"type":16},"danfossPreheatTime":{"ID":16464,"manufacturerCode":4678,"type":35},"danfossRadiatorCovered":{"ID":16406,"manufacturerCode":4678,"type":16},"danfossRegulationSetpointOffset":{"ID":16459,"manufacturerCode":4678,"type":40},"danfossRoomFloorSensorMode":{"ID":16672,"manufacturerCode":4678,"type":48},"danfossRoomStatusCode":{"ID":16640,"manufacturerCode":4678,"type":25},"danfossThermostatOrientation":{"ID":16404,"manufacturerCode":4678,"type":16},"danfossTriggerTime":{"ID":16401,"manufacturerCode":4678,"type":33},"danfossWindowOpenExternal":{"ID":16387,"manufacturerCode":4678,"type":16},"danfossWindowOpenFeatureEnable":{"ID":16465,"manufacturerCode":4678,"type":16},"danfossWindowOpenInternal":{"ID":16384,"manufacturerCode":4678,"type":48},"elkoCalibration":{"ID":1047,"type":40},"elkoChildLock":{"ID":1043,"type":16},"elkoDateTime":{"ID":1031,"type":65},"elkoDisplayText":{"ID":1026,"type":66},"elkoExternalTemp":{"ID":1033,"type":41},"elkoFrostGuard":{"ID":1042,"type":16},"elkoLastMessageId":{"ID":1048,"type":32},"elkoLastMessageStatus":{"ID":1049,"type":32},"elkoLoad":{"ID":1025,"type":33},"elkoMaxFloorTemp":{"ID":1044,"type":32},"elkoMeanPower":{"ID":1032,"type":33},"elkoNightSwitching":{"ID":1041,"type":16},"elkoPowerStatus":{"ID":1030,"type":16},"elkoRegulatorMode":{"ID":1029,"type":16},"elkoRegulatorTime":{"ID":1028,"type":32},"elkoRelayState":{"ID":1045,"type":16},"elkoSensor":{"ID":1027,"type":48},"elkoVersion":{"ID":1046,"type":65},"fourNoksHysteresisHigh":{"ID":257,"manufacturerCode":4209,"type":33},"fourNoksHysteresisLow":{"ID":258,"manufacturerCode":4209,"type":33},"localTemp":{"ID":0,"type":41},"localTemperatureCalibration":{"ID":16,"type":40},"maxCoolSetpointLimit":{"ID":24,"type":41},"maxHeatSetpointLimit":{"ID":22,"type":41},"minCoolSetpointLimit":{"ID":23,"type":41},"minHeatSetpointLimit":{"ID":21,"type":41},"minSetpointDeadBand":{"ID":25,"type":40},"numberOfDailyTrans":{"ID":34,"type":32},"numberOfWeeklyTrans":{"ID":33,"type":32},"occupancy":{"ID":2,"type":24},"occupiedCoolingSetpoint":{"ID":17,"type":41},"occupiedHeatingSetpoint":{"ID":18,"type":41},"outdoorTemp":{"ID":1,"type":41},"pICoolingDemand":{"ID":7,"type":32},"pIHeatingDemand":{"ID":8,"type":32},"programingOperMode":{"ID":37,"type":24},"remoteSensing":{"ID":26,"type":24},"runningMode":{"ID":30,"type":48},"runningState":{"ID":41,"type":25},"schneiderWiserSpecific":{"ID":57616,"manufacturerCode":4190,"type":48},"setpointChangeAmount":{"ID":49,"type":41},"setpointChangeSource":{"ID":48,"type":48},"setpointChangeSourceTimeStamp":{"ID":50,"type":226},"startOfWeek":{"ID":32,"type":48},"systemMode":{"ID":28,"type":48},"systemTypeConfig":{"ID":9,"type":24},"tempSetpointHold":{"ID":35,"type":48},"tempSetpointHoldDuration":{"ID":36,"type":33},"unoccupiedCoolingSetpoint":{"ID":19,"type":41},"unoccupiedHeatingSetpoint":{"ID":20,"type":41},"viessmannAssemblyMode":{"ID":16402,"manufacturerCode":4641,"type":16},"viessmannWindowOpenForce":{"ID":16387,"manufacturerCode":4641,"type":16},"viessmannWindowOpenInternal":{"ID":16384,"manufacturerCode":4641,"type":48}},"commands":{"clearWeeklySchedule":{"ID":3,"parameters":[]},"danfossSetpointCommand":{"ID":64,"parameters":[{"name":"setpointType","type":48},{"name":"setpoint","type":41}]},"getRelayStatusLog":{"ID":4,"parameters":[]},"getWeeklySchedule":{"ID":2,"parameters":[{"name":"daystoreturn","type":32},{"name":"modetoreturn","type":32}]},"plugwiseCalibrateValve":{"ID":160,"parameters":[]},"schneiderWiserThermostatBoost":{"ID":128,"parameters":[{"name":"command","type":48},{"name":"enable","type":48},{"name":"temperature","type":33},{"name":"duration","type":33}]},"setWeeklySchedule":{"ID":1,"parameters":[{"name":"numoftrans","type":32},{"name":"dayofweek","type":32},{"name":"mode","type":32},{"name":"transitions","type":1007}]},"setpointRaiseLower":{"ID":0,"parameters":[{"name":"mode","type":32},{"name":"amount","type":40}]},"wiserSmartCalibrateValve":{"ID":226,"parameters":[]},"wiserSmartSetFipMode":{"ID":225,"parameters":[{"name":"zonemode","type":32},{"name":"fipmode","type":48},{"name":"reserved","type":32}]},"wiserSmartSetSetpoint":{"ID":224,"parameters":[{"name":"operatingmode","type":32},{"name":"zonemode","type":32},{"name":"setpoint","type":41},{"name":"reserved","type":32}]}},"commandsResponse":{"getRelayStatusLogRsp":{"ID":1,"parameters":[{"name":"timeofday","type":33},{"name":"relaystatus","type":33},{"name":"localtemp","type":33},{"name":"humidity","type":32},{"name":"setpoint","type":33},{"name":"unreadentries","type":33}]},"getWeeklyScheduleRsp":{"ID":0,"parameters":[{"name":"numoftrans","type":32},{"name":"dayofweek","type":32},{"name":"mode","type":32},{"name":"transitions","type":1007}]}}},"hvacUserInterfaceCfg":{"ID":516,"attributes":{"danfossViewingDirection":{"ID":16384,"manufacturerCode":4678,"type":48},"keypadLockout":{"ID":1,"type":48},"programmingVisibility":{"ID":2,"type":48},"tempDisplayMode":{"ID":0,"type":48}},"commands":{},"commandsResponse":{}},"liXeePrivate":{"ID":65382,"attributes":{"activeEnergyOutD01":{"ID":515,"type":35},"activeEnergyOutD02":{"ID":516,"type":35},"activeEnergyOutD03":{"ID":517,"type":35},"activeEnergyOutD04":{"ID":518,"type":35},"currentDate":{"ID":514,"type":66},"currentIndexTarif":{"ID":513,"type":32},"currentPrice":{"ID":512,"type":66},"currentTarif":{"ID":0,"type":66},"daysNumberCurrentCalendar":{"ID":549,"type":32},"daysNumberNextCalendar":{"ID":550,"type":32},"daysProfileCurrentCalendar":{"ID":551,"type":67},"daysProfileNextCalendar":{"ID":552,"type":67},"drawnVAMaxN1":{"ID":530,"type":41},"drawnVAMaxN1P2":{"ID":531,"type":41},"drawnVAMaxN1P3":{"ID":532,"type":41},"injectedActiveLoadN":{"ID":528,"type":41},"injectedActiveLoadN1":{"ID":529,"type":41},"injectedVA":{"ID":519,"type":33},"injectedVAMaxN":{"ID":520,"type":41},"injectedVAMaxN1":{"ID":521,"type":41},"linkyMode":{"ID":768,"type":32},"message1":{"ID":533,"type":66},"message2":{"ID":534,"type":66},"motDEtat":{"ID":9,"type":66},"presencePotential":{"ID":3,"type":32},"relais":{"ID":548,"type":33},"scheduleHPHC":{"ID":2,"type":32},"startMobilePoint1":{"ID":536,"type":32},"startMobilePoint2":{"ID":544,"type":32},"startMobilePoint3":{"ID":546,"type":32},"startNoticeEJP":{"ID":4,"type":32},"statusRegister":{"ID":535,"type":65},"stopMobilePoint1":{"ID":537,"type":32},"stopMobilePoint2":{"ID":545,"type":32},"stopMobilePoint3":{"ID":547,"type":32},"tomorrowColor":{"ID":1,"type":66},"warnDIR1":{"ID":6,"type":33},"warnDIR2":{"ID":7,"type":33},"warnDIR3":{"ID":8,"type":33},"warnDPS":{"ID":5,"type":33}},"commands":{},"commandsResponse":{},"manufacturerCode":4151},"lightingBallastCfg":{"ID":769,"attributes":{"ballastFactorAdjustment":{"ID":21,"type":32},"ballastStatus":{"ID":2,"type":24},"elkoControlMode":{"ID":57344,"manufacturerCode":4727,"type":48},"intrinsicBallastFactor":{"ID":20,"type":32},"lampAlarmMode":{"ID":52,"type":24},"lampBurnHours":{"ID":51,"type":34},"lampBurnHoursTripPoint":{"ID":53,"type":34},"lampManufacturer":{"ID":49,"type":66},"lampQuantity":{"ID":32,"type":32},"lampRatedHours":{"ID":50,"type":34},"lampType":{"ID":48,"type":66},"maxLevel":{"ID":17,"type":32},"minLevel":{"ID":16,"type":32},"physicalMaxLevel":{"ID":1,"type":32},"physicalMinLevel":{"ID":0,"type":32},"powerOnFadeTime":{"ID":19,"type":33},"powerOnLevel":{"ID":18,"type":32},"wiserControlMode":{"ID":57344,"manufacturerCode":4190,"type":48}},"commands":{},"commandsResponse":{}},"lightingColorCtrl":{"ID":768,"attributes":{"colorCapabilities":{"ID":16394,"type":33},"colorLoopActive":{"ID":16386,"type":32},"colorLoopDirection":{"ID":16387,"type":32},"colorLoopStartEnhancedHue":{"ID":16389,"type":33},"colorLoopStoredEnhancedHue":{"ID":16390,"type":33},"colorLoopTime":{"ID":16388,"type":33},"colorMode":{"ID":8,"type":48},"colorPointBIntensity":{"ID":60,"type":32},"colorPointBX":{"ID":58,"type":33},"colorPointBY":{"ID":59,"type":33},"colorPointGIntensity":{"ID":56,"type":32},"colorPointGX":{"ID":54,"type":33},"colorPointGY":{"ID":55,"type":33},"colorPointRIntensity":{"ID":52,"type":32},"colorPointRX":{"ID":50,"type":33},"colorPointRY":{"ID":51,"type":33},"colorTempPhysicalMax":{"ID":16396,"type":33},"colorTempPhysicalMin":{"ID":16395,"type":33},"colorTemperature":{"ID":7,"type":33},"compensationText":{"ID":6,"type":66},"coupleColorTempToLevelMin":{"ID":16397,"type":33},"currentHue":{"ID":0,"type":32},"currentSaturation":{"ID":1,"type":32},"currentX":{"ID":3,"type":33},"currentY":{"ID":4,"type":33},"driftCompensation":{"ID":5,"type":48},"enhancedColorMode":{"ID":16385,"type":48},"enhancedCurrentHue":{"ID":16384,"type":33},"numPrimaries":{"ID":16,"type":32},"options":{"ID":15,"type":24},"primary1Intensity":{"ID":19,"type":32},"primary1X":{"ID":17,"type":33},"primary1Y":{"ID":18,"type":33},"primary2Intensity":{"ID":23,"type":32},"primary2X":{"ID":21,"type":33},"primary2Y":{"ID":22,"type":33},"primary3Intensity":{"ID":27,"type":32},"primary3X":{"ID":25,"type":33},"primary3Y":{"ID":26,"type":33},"primary4Intensity":{"ID":34,"type":32},"primary4X":{"ID":32,"type":33},"primary4Y":{"ID":33,"type":33},"primary5Intensity":{"ID":38,"type":32},"primary5X":{"ID":36,"type":33},"primary5Y":{"ID":37,"type":33},"primary6Intensity":{"ID":42,"type":32},"primary6X":{"ID":40,"type":33},"primary6Y":{"ID":41,"type":33},"remainingTime":{"ID":2,"type":33},"startUpColorTemperature":{"ID":16400,"type":33},"tuyaBrightness":{"ID":61441,"type":32},"tuyaRgbMode":{"ID":61440,"type":32},"whitePointX":{"ID":48,"type":33},"whitePointY":{"ID":49,"type":33}},"commands":{"colorLoopSet":{"ID":68,"parameters":[{"name":"updateflags","type":32},{"name":"action","type":32},{"name":"direction","type":32},{"name":"time","type":33},{"name":"starthue","type":33}]},"enhancedMoveHue":{"ID":65,"parameters":[{"name":"movemode","type":32},{"name":"rate","type":33}]},"enhancedMoveToHue":{"ID":64,"parameters":[{"name":"enhancehue","type":33},{"name":"direction","type":32},{"name":"transtime","type":33}]},"enhancedMoveToHueAndSaturation":{"ID":67,"parameters":[{"name":"enhancehue","type":33},{"name":"saturation","type":32},{"name":"transtime","type":33}]},"enhancedStepHue":{"ID":66,"parameters":[{"name":"stepmode","type":32},{"name":"stepsize","type":33},{"name":"transtime","type":33}]},"moveColor":{"ID":8,"parameters":[{"name":"ratex","type":41},{"name":"ratey","type":41}]},"moveColorTemp":{"ID":75,"parameters":[{"name":"movemode","type":32},{"name":"rate","type":33},{"name":"minimum","type":33},{"name":"maximum","type":33}]},"moveHue":{"ID":1,"parameters":[{"name":"movemode","type":32},{"name":"rate","type":32}]},"moveSaturation":{"ID":4,"parameters":[{"name":"movemode","type":32},{"name":"rate","type":32}]},"moveToColor":{"ID":7,"parameters":[{"name":"colorx","type":33},{"name":"colory","type":33},{"name":"transtime","type":33}]},"moveToColorTemp":{"ID":10,"parameters":[{"name":"colortemp","type":33},{"name":"transtime","type":33}]},"moveToHue":{"ID":0,"parameters":[{"name":"hue","type":32},{"name":"direction","type":32},{"name":"transtime","type":33}]},"moveToHueAndSaturation":{"ID":6,"parameters":[{"name":"hue","type":32},{"name":"saturation","type":32},{"name":"transtime","type":33}]},"moveToSaturation":{"ID":3,"parameters":[{"name":"saturation","type":32},{"name":"transtime","type":33}]},"stepColor":{"ID":9,"parameters":[{"name":"stepx","type":41},{"name":"stepy","type":41},{"name":"transtime","type":33}]},"stepColorTemp":{"ID":76,"parameters":[{"name":"stepmode","type":32},{"name":"stepsize","type":33},{"name":"transtime","type":33},{"name":"minimum","type":33},{"name":"maximum","type":33}]},"stepHue":{"ID":2,"parameters":[{"name":"stepmode","type":32},{"name":"stepsize","type":32},{"name":"transtime","type":32}]},"stepSaturation":{"ID":5,"parameters":[{"name":"stepmode","type":32},{"name":"stepsize","type":32},{"name":"transtime","type":32}]},"stopMoveStep":{"ID":71,"parameters":[{"name":"bits","type":32},{"name":"bytee","type":32},{"name":"action","type":32},{"name":"direction","type":32},{"name":"time","type":33},{"name":"starthue","type":33}]},"tuyaDoNotDisturb":{"ID":250,"parameters":[{"name":"enable","type":32}]},"tuyaMoveToHueAndSaturationBrightness":{"ID":6,"parameters":[{"name":"hue","type":32},{"name":"saturation","type":32},{"name":"transtime","type":33},{"name":"brightness","type":32}]},"tuyaMoveToHueAndSaturationBrightness2":{"ID":225,"parameters":[{"name":"hue","type":33},{"name":"saturation","type":33},{"name":"brightness","type":33}]},"tuyaOnOffTransitionTime":{"ID":251,"parameters":[{"name":"unknown","type":32},{"name":"onTransitionTime","type":1013},{"name":"offTransitionTime","type":1013}]},"tuyaOnStartUp":{"ID":249,"parameters":[{"name":"mode","type":33},{"name":"data","type":1001}]},"tuyaRgbMode":{"ID":240,"parameters":[{"name":"enable","type":32}]},"tuyaSetMinimumBrightness":{"ID":224,"parameters":[{"name":"minimum","type":33}]}},"commandsResponse":{}},"manuSpecificAmazonWWAH":{"ID":64599,"attributes":{"clusterRevision":{"ID":65533,"type":33},"configurationModeEnabled":{"ID":13,"type":16},"currentDebugReportID":{"ID":14,"type":32},"disableOTADowngrades":{"ID":2,"type":16},"macPollFailureWaitTime":{"ID":12,"type":32},"macRetryCount":{"ID":5,"type":32},"mgmtLeaveWithoutRejoinEnabled":{"ID":3,"type":16},"nwkRetryCount":{"ID":4,"type":32},"otaMaxOfflineDuration":{"ID":19,"type":33},"pendingNetworkUpdateChannel":{"ID":17,"type":32},"pendingNetworkUpdatePANID":{"ID":18,"type":33},"routerCheckInEnabled":{"ID":6,"type":16},"tcSecurityOnNwkKeyRotationEnabled":{"ID":15,"type":16},"touchlinkInterpanEnabled":{"ID":7,"type":16},"wwahAppEventRetryEnabled":{"ID":9,"type":16},"wwahAppEventRetryQueueSize":{"ID":10,"type":32},"wwahBadParentRecoveryEnabled":{"ID":16,"type":16},"wwahParentClassificationEnabled":{"ID":8,"type":16},"wwahRejoinEnabled":{"ID":11,"type":16}},"commands":{"clearBindingTable":{"ID":10,"parameters":[]}},"commandsResponse":{},"manufacturerCode":4631},"manuSpecificAssaDoorLock":{"ID":64512,"attributes":{"alarmMask":{"ID":80,"type":32},"allCodesLockout":{"ID":26,"type":16},"autoLockTime":{"ID":18,"type":32},"batteryLevel":{"ID":21,"type":32},"insideEscutcheonLED":{"ID":22,"type":32},"language":{"ID":25,"type":32},"lockMode":{"ID":24,"type":32},"numberLogRecordsSupported":{"ID":33,"type":33},"numberPinsSupported":{"ID":48,"type":32},"numberScheduleSlotsPerUser":{"ID":64,"type":32},"oneTouchLocking":{"ID":27,"type":16},"privacyButtonSetting":{"ID":28,"type":16},"shutdownTime":{"ID":20,"type":32},"volume":{"ID":23,"type":32},"wrongCodeAttempts":{"ID":19,"type":32}},"commands":{"clearAllUserCodes":{"ID":51,"parameters":[]},"configureReporting":{"ID":179,"parameters":[]},"getBasicClusterAttributes":{"ID":180,"parameters":[]},"getBatteryLevel":{"ID":18,"parameters":[]},"getHistory":{"ID":160,"parameters":[]},"getLastUserIdEntered":{"ID":54,"parameters":[]},"getLockStatus":{"ID":16,"parameters":[],"response":0},"getLogin":{"ID":161,"parameters":[]},"getMandatoryAttributes":{"ID":176,"parameters":[]},"getReflashLock":{"ID":144,"parameters":[]},"getScheduleSlot":{"ID":65,"parameters":[{"name":"payload","type":66}]},"getUser":{"ID":162,"parameters":[]},"getUserCodeStatus":{"ID":53,"parameters":[]},"getUsers":{"ID":163,"parameters":[]},"readAttribute":{"ID":177,"parameters":[]},"reflash":{"ID":96,"parameters":[{"name":"payload","type":66}],"response":1},"reflashData":{"ID":97,"parameters":[{"name":"payload","type":66}],"response":2},"reflashStatus":{"ID":98,"parameters":[{"name":"payload","type":66}],"response":3},"setRFLockoutTime":{"ID":19,"parameters":[]},"setScheduleSlot":{"ID":64,"parameters":[{"name":"payload","type":66}]},"setScheduleSlotStatus":{"ID":66,"parameters":[{"name":"payload","type":66}]},"setUserCodeStatus":{"ID":52,"parameters":[]},"userAdded":{"ID":55,"parameters":[]},"userCodeClear":{"ID":50,"parameters":[{"name":"payload","type":66}]},"userCodeGet":{"ID":49,"parameters":[{"name":"payload","type":66}]},"userCodeSet":{"ID":48,"parameters":[{"name":"payload","type":66}]},"userDeleted":{"ID":56,"parameters":[]},"writeAttribute":{"ID":178,"parameters":[]}},"commandsResponse":{"getLockStatusRsp":{"ID":0,"parameters":[{"name":"status","type":32}]},"reflashDataRsp":{"ID":2,"parameters":[{"name":"status","type":32}]},"reflashRsp":{"ID":1,"parameters":[{"name":"status","type":32}]},"reflashStatusRsp":{"ID":3,"parameters":[{"name":"status","type":32}]}}},"manuSpecificCentraliteHumidity":{"ID":64581,"attributes":{"measuredValue":{"ID":0,"type":33}},"commands":{},"commandsResponse":{},"manufacturerCode":4174},"manuSpecificClusterAduroSmart":{"ID":64716,"attributes":{},"commands":{"cmd0":{"ID":0,"parameters":[]}},"commandsResponse":{}},"manuSpecificDoorman":{"ID":60108,"attributes":{},"commands":{"armDisarm":{"ID":78,"parameters":[{"name":"payload","type":66}]},"getConfigurationParameter":{"ID":252,"parameters":[{"name":"payload","type":66}]},"integrationModeActivation":{"ID":37,"parameters":[{"name":"payload","type":66}]},"setConfigurationParameter":{"ID":253,"parameters":[{"name":"payload","type":66}]}},"commandsResponse":{}},"manuSpecificLegrandDevices":{"ID":64513,"attributes":{},"commands":{},"commandsResponse":{},"manufacturerCode":4129},"manuSpecificLegrandDevices2":{"ID":64576,"attributes":{},"commands":{"command0":{"ID":0,"parameters":[{"name":"data","type":1008}]}},"commandsResponse":{},"manufacturerCode":4129},"manuSpecificLegrandDevices3":{"ID":64577,"attributes":{},"commands":{"command0":{"ID":0,"parameters":[{"name":"data","type":1008}]}},"commandsResponse":{},"manufacturerCode":4129},"manuSpecificLumi":{"ID":64704,"attributes":{"airQuality":{"ID":297,"type":32},"curtainCalibrated":{"ID":1026,"type":16},"curtainHandOpen":{"ID":1025,"type":16},"curtainReverse":{"ID":1024,"type":16},"displayUnit":{"ID":276,"type":32},"illuminance":{"ID":274,"type":35},"mode":{"ID":9,"type":32}},"commands":{},"commandsResponse":{},"manufacturerCode":4447},"manuSpecificNiko1":{"ID":64512,"attributes":{"outletChildLock":{"ID":257,"type":32},"outletLedColor":{"ID":256,"type":34},"outletLedState":{"ID":260,"type":32},"switchOperationMode":{"ID":0,"type":48}},"commands":{},"commandsResponse":{},"manufacturerCode":4703},"manuSpecificNiko2":{"ID":64513,"attributes":{"switchAction":{"ID":2,"type":32}},"commands":{},"commandsResponse":{},"manufacturerCode":4703},"manuSpecificOsram":{"ID":64527,"attributes":{},"commands":{"resetStartupParams":{"ID":2,"parameters":[]},"saveStartupParams":{"ID":1,"parameters":[]}},"commandsResponse":{"saveStartupParamsRsp":{"ID":0,"parameters":[]}}},"manuSpecificPhilips":{"ID":64512,"attributes":{"config":{"ID":49,"type":25}},"commands":{},"commandsResponse":{"hueNotification":{"ID":0,"parameters":[{"name":"button","type":32},{"name":"unknown1","type":34},{"name":"type","type":32},{"name":"unknown2","type":32},{"name":"time","type":32},{"name":"unknown2","type":32}]}},"manufacturerCode":4107},"manuSpecificPhilips2":{"ID":64515,"attributes":{"state":{"ID":2,"type":65}},"commands":{"multiColor":{"ID":0,"parameters":[{"name":"data","type":1008}]}},"commandsResponse":{},"manufacturerCode":4107},"manuSpecificProfalux1":{"ID":64545,"attributes":{"motorCoverType":{"ID":0,"type":32}},"commands":{},"commandsResponse":{},"manufacturerCode":4368},"manuSpecificSamsungAccelerometer":{"ID":64514,"attributes":{"acceleration":{"ID":16,"type":24},"motion_threshold":{"ID":2,"type":33},"motion_threshold_multiplier":{"ID":0,"type":32},"x_axis":{"ID":18,"type":41},"y_axis":{"ID":19,"type":41},"z_axis":{"ID":20,"type":41}},"commands":{},"commandsResponse":{},"manufacturerCode":4362},"manuSpecificSchneiderFanSwitchConfiguration":{"ID":64516,"attributes":{"ledIndication":{"ID":2,"type":32},"ledOrientation":{"ID":96,"type":32}},"commands":{},"commandsResponse":{},"manufacturerCode":4190},"manuSpecificSchneiderLightSwitchConfiguration":{"ID":65303,"attributes":{"downGroupID":{"ID":33,"type":33},"downSceneID":{"ID":32,"type":32},"ledIndication":{"ID":0,"type":48},"switchActions":{"ID":1,"type":48},"upGroupID":{"ID":17,"type":33},"upSceneID":{"ID":16,"type":32}},"commands":{},"commandsResponse":{},"manufacturerCode":4190},"manuSpecificSiglisZigfred":{"ID":64578,"attributes":{"buttonEvent":{"ID":8,"type":35}},"commands":{"siglisZigfredButtonEvent":{"ID":2,"parameters":[{"name":"button","type":32},{"name":"type","type":32},{"name":"duration","type":33}]}},"commandsResponse":{},"manufacturerCode":4764},"manuSpecificSinope":{"ID":65281,"attributes":{"GFCiStatus":{"ID":277,"type":48},"actionReport":{"ID":84,"type":48},"ambiantMaxHeatSetpointLimit":{"ID":264,"type":41},"auxConnectedLoad":{"ID":280,"type":33},"auxOutputMode":{"ID":262,"type":48},"coldLoadPickupStatus":{"ID":643,"type":32},"connectedLoad":{"ID":281,"type":33},"connectedLoadRM":{"ID":96,"type":33},"currentLoad":{"ID":112,"type":24},"currentSetpoint":{"ID":299,"type":41},"currentTimeToDisplay":{"ID":32,"type":35},"dimmerTimmer":{"ID":160,"type":35},"drConfigWaterTempMin":{"ID":118,"type":32},"drConfigWaterTempTime":{"ID":119,"type":32},"drWTTimeOn":{"ID":120,"type":33},"ecoMode":{"ID":113,"type":40},"ecoMode1":{"ID":114,"type":32},"ecoMode2":{"ID":115,"type":32},"firmwareVersion":{"ID":4,"type":66},"floorControlMode":{"ID":261,"type":48},"floorLimitStatus":{"ID":268,"type":48},"floorMaxHeatSetpointLimit":{"ID":266,"type":41},"floorMinHeatSetpointLimit":{"ID":265,"type":41},"floorTemperature":{"ID":263,"type":41},"flowMeterConfig":{"ID":576,"type":72},"keypadLockout":{"ID":2,"type":48},"ledColorOff":{"ID":81,"type":34},"ledColorOn":{"ID":80,"type":34},"ledIntensityOff":{"ID":83,"type":32},"ledIntensityOn":{"ID":82,"type":32},"minimumBrightness":{"ID":85,"type":33},"offLedIntensity":{"ID":83,"type":32},"onLedIntensity":{"ID":82,"type":32},"outdoorTempToDisplay":{"ID":16,"type":41},"outdoorTempToDisplayTimeout":{"ID":17,"type":33},"pumpProtection":{"ID":296,"type":32},"reportLocalTemperature":{"ID":301,"type":41},"roomTemperature":{"ID":269,"type":41},"secondScreenBehavior":{"ID":18,"type":48},"temperatureSensor":{"ID":267,"type":48},"timeFormatToDisplay":{"ID":276,"type":48},"unknown":{"ID":117,"type":27},"unknown1":{"ID":128,"type":35},"unknown2":{"ID":256,"type":32},"unknown3":{"ID":298,"type":48}},"commands":{},"commandsResponse":{},"manufacturerCode":4508},"manuSpecificSmartThingsArrivalSensor":{"ID":64517,"attributes":{},"commands":{},"commandsResponse":{"arrivalSensorNotify":{"ID":1,"parameters":[]}},"manufacturerCode":4362},"manuSpecificTuya":{"ID":61184,"attributes":{},"commands":{"dataQuery":{"ID":3,"parameters":[]},"dataRequest":{"ID":0,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}]},"mcuGatewayConnectionStatus":{"ID":37,"parameters":[{"name":"payloadSize","type":33},{"name":"payload","type":32}]},"mcuOtaBlockDataResponse":{"ID":20,"parameters":[{"name":"seq","type":33},{"name":"status","type":32},{"name":"key_hi","type":35},{"name":"key_lo","type":35},{"name":"version","type":32},{"name":"offset","type":35},{"name":"imageData","type":1001}]},"mcuOtaNotify":{"ID":18,"parameters":[{"name":"seq","type":33},{"name":"key_hi","type":35},{"name":"key_lo","type":35},{"name":"version","type":32},{"name":"imageSize","type":35},{"name":"crc","type":35}]},"mcuSyncTime":{"ID":36,"parameters":[{"name":"payloadSize","type":33},{"name":"payload","type":1001}]},"mcuVersionRequest":{"ID":16,"parameters":[{"name":"seq","type":33}]},"sendData":{"ID":4,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}]}},"commandsResponse":{"activeStatusReport":{"ID":6,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}]},"activeStatusReportAlt":{"ID":5,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}]},"dataReport":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}]},"dataResponse":{"ID":1,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}]},"mcuGatewayConnectionStatus":{"ID":37,"parameters":[{"name":"payloadSize","type":33}]},"mcuOtaBlockDataRequest":{"ID":19,"parameters":[{"name":"seq","type":33},{"name":"key_hi","type":35},{"name":"key_lo","type":35},{"name":"version","type":32},{"name":"offset","type":35},{"name":"size","type":35}]},"mcuOtaResult":{"ID":21,"parameters":[{"name":"seq","type":33},{"name":"status","type":32},{"name":"key_hi","type":35},{"name":"key_lo","type":35},{"name":"version","type":32}]},"mcuSyncTime":{"ID":36,"parameters":[{"name":"payloadSize","type":33}]},"mcuVersionResponse":{"ID":17,"parameters":[{"name":"seq","type":33},{"name":"version","type":32}]}}},"manuSpecificTuya_2":{"ID":57346,"attributes":{"alarm_humidity":{"ID":53263,"type":48},"alarm_humidity_max":{"ID":53261,"type":41},"alarm_humidity_min":{"ID":53262,"type":41},"alarm_temperature":{"ID":53254,"type":48},"alarm_temperature_max":{"ID":53258,"type":41},"alarm_temperature_min":{"ID":53259,"type":41},"unknown":{"ID":53264,"type":32}},"commands":{},"commandsResponse":{}},"manuSpecificTuya_3":{"ID":57345,"attributes":{"powerOnBehavior":{"ID":53264,"type":48},"switchMode":{"ID":53280,"type":48},"switchType":{"ID":53296,"type":48}},"commands":{"setOptions1":{"ID":229,"parameters":[{"name":"data","type":1008}]},"setOptions2":{"ID":230,"parameters":[{"name":"data","type":1008}]},"setOptions3":{"ID":231,"parameters":[{"name":"data","type":1008}]}},"commandsResponse":{}},"mobileDeviceCfg":{"ID":34,"attributes":{"keepAliveTime":{"ID":0,"type":33},"rejoinTimeout":{"ID":1,"type":33}},"commands":{},"commandsResponse":{}},"msCO2":{"ID":1037,"attributes":{"maxMeasuredValue":{"ID":2,"type":57},"measuredValue":{"ID":0,"type":57},"minMeasuredValue":{"ID":1,"type":57},"sprutCO2AutoCalibration":{"ID":26113,"manufacturerCode":26214,"type":16},"sprutCO2Calibration":{"ID":26112,"manufacturerCode":26214,"type":16}},"commands":{},"commandsResponse":{}},"msFlowMeasurement":{"ID":1028,"attributes":{"maxMeasuredValue":{"ID":2,"type":33},"measuredValue":{"ID":0,"type":33},"minMeasuredValue":{"ID":1,"type":33},"tolerance":{"ID":3,"type":33}},"commands":{},"commandsResponse":{}},"msFormaldehyde":{"ID":1067,"attributes":{"maxMeasuredValue":{"ID":2,"type":57},"measuredTolerance":{"ID":3,"type":57},"measuredValue":{"ID":0,"type":57},"minMeasuredValue":{"ID":1,"type":57}},"commands":{},"commandsResponse":{}},"msIlluminanceLevelSensing":{"ID":1025,"attributes":{"illuminanceTargetLevel":{"ID":16,"type":33},"levelStatus":{"ID":0,"type":48},"lightSensorType":{"ID":1,"type":48}},"commands":{},"commandsResponse":{}},"msIlluminanceMeasurement":{"ID":1024,"attributes":{"lightSensorType":{"ID":4,"type":48},"maxMeasuredValue":{"ID":2,"type":33},"measuredValue":{"ID":0,"type":33},"minMeasuredValue":{"ID":1,"type":33},"tolerance":{"ID":3,"type":33}},"commands":{},"commandsResponse":{}},"msOccupancySensing":{"ID":1030,"attributes":{"contactOToUDelay":{"ID":48,"type":33},"contactUToODelay":{"ID":49,"type":33},"contactUToOThreshold":{"ID":50,"type":32},"elkoForceOffTimeout":{"ID":57346,"manufacturerCode":4727,"type":33},"elkoOccupancyDfltOperationMode":{"ID":57344,"manufacturerCode":4727,"type":48},"elkoOccupancyOperationMode":{"ID":57345,"manufacturerCode":4727,"type":48},"elkoOccupancySensitivity":{"ID":57347,"manufacturerCode":4727,"type":32},"occupancy":{"ID":0,"type":24},"occupancySensorType":{"ID":1,"type":48},"occupancySensorTypeBitmap":{"ID":2,"type":24},"pirOToUDelay":{"ID":16,"type":33},"pirUToODelay":{"ID":17,"type":33},"pirUToOThreshold":{"ID":18,"type":32},"sprutOccupancyLevel":{"ID":26112,"manufacturerCode":26214,"type":33},"sprutOccupancySensitivity":{"ID":26113,"manufacturerCode":26214,"type":33},"ultrasonicOToUDelay":{"ID":32,"type":33},"ultrasonicUToODelay":{"ID":33,"type":33},"ultrasonicUToOThreshold":{"ID":34,"type":32}},"commands":{},"commandsResponse":{}},"msPressureMeasurement":{"ID":1027,"attributes":{"maxMeasuredValue":{"ID":2,"type":41},"maxScaledValue":{"ID":18,"type":41},"measuredValue":{"ID":0,"type":41},"minMeasuredValue":{"ID":1,"type":41},"minScaledValue":{"ID":17,"type":41},"scale":{"ID":20,"type":40},"scaledTolerance":{"ID":19,"type":33},"scaledValue":{"ID":16,"type":41},"tolerance":{"ID":3,"type":33}},"commands":{},"commandsResponse":{}},"msRelativeHumidity":{"ID":1029,"attributes":{"maxMeasuredValue":{"ID":2,"type":33},"measuredValue":{"ID":0,"type":33},"minMeasuredValue":{"ID":1,"type":33},"sprutHeater":{"ID":26112,"manufacturerCode":26214,"type":16},"tolerance":{"ID":3,"type":33}},"commands":{},"commandsResponse":{}},"msSoilMoisture":{"ID":1032,"attributes":{"maxMeasuredValue":{"ID":2,"type":33},"measuredValue":{"ID":0,"type":33},"minMeasuredValue":{"ID":1,"type":33},"tolerance":{"ID":3,"type":33}},"commands":{},"commandsResponse":{}},"msTemperatureMeasurement":{"ID":1026,"attributes":{"maxMeasuredValue":{"ID":2,"type":41},"measuredValue":{"ID":0,"type":41},"minAbsoluteChange":{"ID":17,"type":255},"minMeasuredValue":{"ID":1,"type":41},"minPercentChange":{"ID":16,"type":255},"sprutTemperatureOffset":{"ID":26112,"manufacturerCode":26214,"type":41},"tolerance":{"ID":3,"type":33}},"commands":{},"commandsResponse":{}},"nearestGateway":{"ID":36,"attributes":{"nearestGateway":{"ID":0,"type":33},"newMobileNode":{"ID":1,"type":33}},"commands":{},"commandsResponse":{}},"neighborCleaning":{"ID":35,"attributes":{"neighborCleaningTimeout":{"ID":0,"type":33}},"commands":{},"commandsResponse":{}},"owonClearMetering":{"ID":65504,"attributes":{},"commands":{"owonClearMeasurementData":{"ID":0,"parameters":[]}},"commandsResponse":{},"manufacturerCode":4412},"pHMeasurement":{"ID":1033,"attributes":{"maxMeasuredValue":{"ID":2,"type":33},"measuredValue":{"ID":0,"type":33},"minMeasuredValue":{"ID":1,"type":33},"tolerance":{"ID":3,"type":33}},"commands":{},"commandsResponse":{}},"pi11073ProtocolTunnel":{"ID":1556,"attributes":{"connected":{"ID":3,"type":16},"deviceidList":{"ID":0,"type":72},"idleTimeout":{"ID":5,"type":33},"managerEndpoint":{"ID":2,"type":32},"managerTarget":{"ID":1,"type":240},"preemptible":{"ID":4,"type":16}},"commands":{"connectReq":{"ID":1,"parameters":[]},"connectStatusNoti":{"ID":3,"parameters":[]},"disconnectReq":{"ID":2,"parameters":[]},"transferApdu":{"ID":0,"parameters":[]}},"commandsResponse":{}},"piAnalogInputExt":{"ID":1539,"attributes":{"ackedTransitions":{"ID":0,"type":24},"deadband":{"ID":25,"type":57},"eventEnable":{"ID":35,"type":24},"eventState":{"ID":36,"type":48},"eventTimeStamps":{"ID":130,"type":72},"highLimit":{"ID":45,"type":57},"limitEnable":{"ID":52,"type":24},"lowLimit":{"ID":59,"type":57},"notificationClass":{"ID":17,"type":33},"notifyType":{"ID":72,"type":48},"timeDelay":{"ID":113,"type":32}},"commands":{"connectReq":{"ID":1,"parameters":[]},"connectStatusNoti":{"ID":3,"parameters":[]},"disconnectReq":{"ID":2,"parameters":[]},"transferApdu":{"ID":0,"parameters":[]}},"commandsResponse":{}},"piAnalogInputReg":{"ID":1538,"attributes":{"covIncrement":{"ID":22,"type":57},"deviceType":{"ID":31,"type":66},"objectId":{"ID":75,"type":234},"objectName":{"ID":77,"type":66},"objectType":{"ID":79,"type":49},"profileName":{"ID":168,"type":66},"updateInterval":{"ID":118,"type":32}},"commands":{},"commandsResponse":{}},"piAnalogOutputExt":{"ID":1541,"attributes":{"ackedTransitions":{"ID":0,"type":24},"deadband":{"ID":25,"type":57},"eventEnable":{"ID":35,"type":24},"eventState":{"ID":36,"type":48},"eventTimeStamps":{"ID":130,"type":72},"highLimit":{"ID":45,"type":57},"limitEnable":{"ID":52,"type":24},"lowLimit":{"ID":59,"type":57},"notificationClass":{"ID":17,"type":33},"notifyType":{"ID":72,"type":48},"timeDelay":{"ID":113,"type":32}},"commands":{},"commandsResponse":{}},"piAnalogOutputReg":{"ID":1540,"attributes":{"covIncrement":{"ID":22,"type":57},"deviceType":{"ID":31,"type":66},"objectId":{"ID":75,"type":234},"objectName":{"ID":77,"type":66},"objectType":{"ID":79,"type":49},"profileName":{"ID":168,"type":66},"updateInterval":{"ID":118,"type":32}},"commands":{},"commandsResponse":{}},"piAnalogValueExt":{"ID":1543,"attributes":{"ackedTransitions":{"ID":0,"type":24},"deadband":{"ID":25,"type":57},"eventEnable":{"ID":35,"type":24},"eventState":{"ID":36,"type":48},"eventTimeStamps":{"ID":130,"type":72},"highLimit":{"ID":45,"type":57},"limitEnable":{"ID":52,"type":24},"lowLimit":{"ID":59,"type":57},"notificationClass":{"ID":17,"type":33},"notifyType":{"ID":72,"type":48},"timeDelay":{"ID":113,"type":32}},"commands":{},"commandsResponse":{}},"piAnalogValueReg":{"ID":1542,"attributes":{"covIncrement":{"ID":22,"type":57},"objectId":{"ID":75,"type":234},"objectName":{"ID":77,"type":66},"objectType":{"ID":79,"type":49},"profileName":{"ID":168,"type":66}},"commands":{},"commandsResponse":{}},"piBacnetProtocolTunnel":{"ID":1537,"attributes":{},"commands":{"transferNpdu":{"ID":0,"parameters":[{"name":"npdu","type":32}]}},"commandsResponse":{}},"piBinaryInputExt":{"ID":1545,"attributes":{"ackedTransitions":{"ID":0,"type":24},"alarmValue":{"ID":6,"type":16},"eventEnable":{"ID":35,"type":24},"eventState":{"ID":36,"type":48},"eventTimeStamps":{"ID":130,"type":72},"notificationClass":{"ID":17,"type":33},"notifyType":{"ID":72,"type":48},"timeDelay":{"ID":113,"type":32}},"commands":{},"commandsResponse":{}},"piBinaryInputReg":{"ID":1544,"attributes":{"changeOfStateCount":{"ID":15,"type":35},"changeOfStateTime":{"ID":16,"type":76},"deviceType":{"ID":31,"type":66},"elapsedActiveTime":{"ID":33,"type":35},"objectIdentifier":{"ID":75,"type":234},"objectName":{"ID":77,"type":66},"objectType":{"ID":79,"type":49},"profileName":{"ID":168,"type":66},"timeOfATReset":{"ID":114,"type":76},"timeOfSCReset":{"ID":115,"type":76}},"commands":{},"commandsResponse":{}},"piBinaryOutputExt":{"ID":1547,"attributes":{"ackedTransitions":{"ID":0,"type":24},"eventEnable":{"ID":35,"type":24},"eventState":{"ID":36,"type":48},"eventTimeStamps":{"ID":130,"type":72},"notificationClass":{"ID":17,"type":33},"notifyType":{"ID":72,"type":48},"timeDelay":{"ID":113,"type":32}},"commands":{},"commandsResponse":{}},"piBinaryOutputReg":{"ID":1546,"attributes":{"changeOfStateCount":{"ID":15,"type":35},"changeOfStateTime":{"ID":16,"type":76},"deviceType":{"ID":31,"type":66},"elapsedActiveTime":{"ID":33,"type":35},"feedBackValue":{"ID":40,"type":48},"objectIdentifier":{"ID":75,"type":234},"objectName":{"ID":77,"type":66},"objectType":{"ID":79,"type":49},"profileName":{"ID":168,"type":66},"timeOfATReset":{"ID":114,"type":76},"timeOfSCReset":{"ID":115,"type":76}},"commands":{},"commandsResponse":{}},"piBinaryValueExt":{"ID":1549,"attributes":{"ackedTransitions":{"ID":0,"type":24},"alarmValue":{"ID":6,"type":16},"eventEnable":{"ID":35,"type":24},"eventState":{"ID":36,"type":48},"eventTimeStamps":{"ID":130,"type":72},"notificationClass":{"ID":17,"type":33},"notifyType":{"ID":72,"type":48},"timeDelay":{"ID":113,"type":32}},"commands":{},"commandsResponse":{}},"piBinaryValueReg":{"ID":1548,"attributes":{"changeOfStateCount":{"ID":15,"type":35},"changeOfStateTime":{"ID":16,"type":76},"elapsedActiveTime":{"ID":33,"type":35},"objectIdentifier":{"ID":75,"type":234},"objectName":{"ID":77,"type":66},"objectType":{"ID":79,"type":49},"profileName":{"ID":168,"type":66},"timeOfATReset":{"ID":114,"type":76},"timeOfSCReset":{"ID":115,"type":76}},"commands":{},"commandsResponse":{}},"piGenericTunnel":{"ID":1536,"attributes":{"maxIncomeTransSize":{"ID":1,"type":33},"maxOutgoTransSize":{"ID":2,"type":33},"protocolAddr":{"ID":3,"type":65}},"commands":{"matchProtocolAddr":{"ID":0,"parameters":[{"name":"protocoladdr","type":66}]}},"commandsResponse":{"advertiseProtocolAddr":{"ID":1,"parameters":[{"name":"protocoladdr","type":66}]},"matchProtocolAddrRsp":{"ID":0,"parameters":[{"name":"devieeeaddr","type":240},{"name":"protocoladdr","type":66}]}}},"piIso7818ProtocolTunnel":{"ID":1557,"attributes":{"status":{"ID":0,"type":32}},"commands":{},"commandsResponse":{}},"piMultistateInputExt":{"ID":1551,"attributes":{"ackedTransitions":{"ID":0,"type":24},"alarmValue":{"ID":6,"type":33},"eventEnable":{"ID":35,"type":24},"eventState":{"ID":36,"type":48},"eventTimeStamps":{"ID":130,"type":72},"faultValues":{"ID":37,"type":33},"notificationClass":{"ID":17,"type":33},"notifyType":{"ID":72,"type":48},"timeDelay":{"ID":113,"type":32}},"commands":{},"commandsResponse":{}},"piMultistateInputReg":{"ID":1550,"attributes":{"deviceType":{"ID":31,"type":66},"objectId":{"ID":75,"type":234},"objectName":{"ID":77,"type":66},"objectType":{"ID":79,"type":49},"profileName":{"ID":168,"type":66}},"commands":{},"commandsResponse":{}},"piMultistateOutputExt":{"ID":1553,"attributes":{"ackedTransitions":{"ID":0,"type":24},"eventEnable":{"ID":35,"type":24},"eventState":{"ID":36,"type":48},"eventTimeStamps":{"ID":130,"type":72},"notificationClass":{"ID":17,"type":33},"notifyType":{"ID":72,"type":48},"timeDelay":{"ID":113,"type":32}},"commands":{},"commandsResponse":{}},"piMultistateOutputReg":{"ID":1552,"attributes":{"deviceType":{"ID":31,"type":66},"feedBackValue":{"ID":40,"type":48},"objectId":{"ID":75,"type":234},"objectName":{"ID":77,"type":66},"objectType":{"ID":79,"type":49},"profileName":{"ID":168,"type":66}},"commands":{},"commandsResponse":{}},"piMultistateValueExt":{"ID":1555,"attributes":{"ackedTransitions":{"ID":0,"type":24},"alarmValue":{"ID":6,"type":33},"eventEnable":{"ID":35,"type":24},"eventState":{"ID":36,"type":48},"eventTimeStamps":{"ID":130,"type":72},"faultValues":{"ID":37,"type":33},"notificationClass":{"ID":17,"type":33},"notifyType":{"ID":72,"type":48},"timeDelay":{"ID":113,"type":32}},"commands":{},"commandsResponse":{}},"piMultistateValueReg":{"ID":1554,"attributes":{"objectId":{"ID":75,"type":234},"objectName":{"ID":77,"type":66},"objectType":{"ID":79,"type":49},"profileName":{"ID":168,"type":66}},"commands":{},"commandsResponse":{}},"piRetailTunnel":{"ID":1559,"attributes":{"manufacturerCode":{"ID":0,"type":33},"msProfile":{"ID":1,"type":33}},"commands":{},"commandsResponse":{}},"pm10Measurement":{"ID":1069,"attributes":{"measuredMaxValue":{"ID":2,"type":57},"measuredMinValue":{"ID":1,"type":57},"measuredTolerance":{"ID":3,"type":57},"measuredValue":{"ID":0,"type":57}},"commands":{},"commandsResponse":{}},"pm1Measurement":{"ID":1068,"attributes":{"measuredMaxValue":{"ID":2,"type":57},"measuredMinValue":{"ID":1,"type":57},"measuredTolerance":{"ID":3,"type":57},"measuredValue":{"ID":0,"type":57}},"commands":{},"commandsResponse":{}},"pm25Measurement":{"ID":1066,"attributes":{"measuredMaxValue":{"ID":2,"type":57},"measuredMinValue":{"ID":1,"type":57},"measuredTolerance":{"ID":3,"type":57},"measuredValue":{"ID":0,"type":57}},"commands":{},"commandsResponse":{}},"schneiderSpecificPilotMode":{"ID":65315,"attributes":{"pilotMode":{"ID":49,"type":48}},"commands":{},"commandsResponse":{},"manufacturerCode":4190},"seMetering":{"ID":1794,"attributes":{"DFTSummationReceived":{"ID":31,"type":37},"activeRegisterTierDelivered":{"ID":32,"type":48},"activeRegisterTierReceived":{"ID":33,"type":48},"billToDate":{"ID":2560,"type":35},"billToDateTimeStamp":{"ID":2561,"type":226},"controlTempreature":{"ID":25,"type":42},"curMonthMaxEnergyCarrDemand":{"ID":1043,"type":42},"curMonthMinEnergyCarrDemand":{"ID":1044,"type":42},"curPartProfileIntStartTimeDelivered":{"ID":1029,"type":226},"curPartProfileIntStartTimeReceived":{"ID":1030,"type":226},"curPartProfileIntValueDelivered":{"ID":1031,"type":34},"curPartProfileIntValueReceived":{"ID":1032,"type":34},"curYearMaxEnergyCarrDemand":{"ID":1045,"type":42},"curYearMinEnergyCarrDemand":{"ID":1046,"type":42},"currentBlock":{"ID":14,"type":48},"currentBlockPeriodConsumpDelivered":{"ID":12,"type":37},"currentBlockPeriodConsumpReceived":{"ID":29,"type":37},"currentBlockReceived":{"ID":30,"type":37},"currentDayMaxDemand":{"ID":1037,"type":42},"currentDayMaxPressure":{"ID":1033,"type":37},"currentDayMinPressure":{"ID":1034,"type":37},"currentDemandDelivered":{"ID":1536,"type":34},"currentInEnergyCarrierDemand":{"ID":26,"type":42},"currentInEnergyCarrierSumm":{"ID":21,"type":37},"currentMaxDemandDeliverdTime":{"ID":8,"type":226},"currentMaxDemandDelivered":{"ID":2,"type":37},"currentMaxDemandReceived":{"ID":3,"type":37},"currentMaxDemandReceivedTime":{"ID":9,"type":226},"currentMonthMaxDemand":{"ID":1039,"type":42},"currentOutEnergyCarrierDemand":{"ID":27,"type":42},"currentOutEnergyCarrierSumm":{"ID":22,"type":37},"currentSummDelivered":{"ID":0,"type":37},"currentSummReceived":{"ID":1,"type":37},"currentTier10SummDelivered":{"ID":274,"type":37},"currentTier10SummReceived":{"ID":275,"type":37},"currentTier11SummDelivered":{"ID":276,"type":37},"currentTier11SummReceived":{"ID":277,"type":37},"currentTier12SummDelivered":{"ID":278,"type":37},"currentTier12SummReceived":{"ID":279,"type":37},"currentTier13SummDelivered":{"ID":280,"type":37},"currentTier13SummReceived":{"ID":281,"type":37},"currentTier14SummDelivered":{"ID":282,"type":37},"currentTier14SummReceived":{"ID":283,"type":37},"currentTier15SummDelivered":{"ID":284,"type":37},"currentTier15SummReceived":{"ID":285,"type":37},"currentTier1SummDelivered":{"ID":256,"type":37},"currentTier1SummReceived":{"ID":257,"type":37},"currentTier2SummDelivered":{"ID":258,"type":37},"currentTier2SummReceived":{"ID":259,"type":37},"currentTier3SummDelivered":{"ID":260,"type":37},"currentTier3SummReceived":{"ID":261,"type":37},"currentTier4SummDelivered":{"ID":262,"type":37},"currentTier4SummReceived":{"ID":263,"type":37},"currentTier5SummDelivered":{"ID":264,"type":37},"currentTier5SummReceived":{"ID":265,"type":37},"currentTier6SummDelivered":{"ID":266,"type":37},"currentTier6SummReceived":{"ID":267,"type":37},"currentTier7SummDelivered":{"ID":268,"type":37},"currentTier7SummReceived":{"ID":269,"type":37},"currentTier8SummDelivered":{"ID":270,"type":37},"currentTier8SummReceived":{"ID":271,"type":37},"currentTier9SummDelivered":{"ID":272,"type":37},"currentTier9SummReceived":{"ID":273,"type":37},"currentYearMaxDemand":{"ID":1040,"type":42},"currentdayConsumpDelivered":{"ID":1025,"type":34},"currentdayConsumpReceived":{"ID":1026,"type":34},"currentdayMaxEnergyCarrDemand":{"ID":1041,"type":42},"dailyConsumpTarget":{"ID":13,"type":34},"dailyFreezeTime":{"ID":5,"type":33},"defaultUpdatePeriod":{"ID":10,"type":32},"demandFormatting":{"ID":772,"type":24},"demandIntegrationPeriod":{"ID":1538,"type":32},"demandLimit":{"ID":1537,"type":34},"demandLimitArmDuration":{"ID":1540,"type":33},"develcoCurrentSummation":{"ID":769,"manufacturerCode":4117,"type":37},"develcoInterfaceMode":{"ID":770,"manufacturerCode":4117,"type":49},"develcoPulseConfiguration":{"ID":768,"manufacturerCode":4117,"type":33},"dftSumm":{"ID":4,"type":37},"divisor":{"ID":770,"type":34},"electricityAlarmMask":{"ID":2049,"type":27},"energyCarrierDemandFormatting":{"ID":779,"type":24},"energyCarrierSummFormatting":{"ID":778,"type":24},"energyCarrierUnitOfMeas":{"ID":777,"type":48},"extendedGenericAlarmMask":{"ID":2054,"type":29},"extendedStatus":{"ID":516,"type":31},"fastPollUpdatePeriod":{"ID":11,"type":32},"flowRestriction":{"ID":19,"type":32},"gasSpecificAlarmMask":{"ID":2053,"type":25},"genFlowPressureAlarmMask":{"ID":2050,"type":25},"genericAlarmMask":{"ID":2048,"type":25},"heatCoolSpecificAlarmMASK":{"ID":2052,"type":25},"historicalConsumpFormatting":{"ID":773,"type":24},"hoursInFault":{"ID":515,"type":34},"hoursInOperation":{"ID":514,"type":34},"inletTempreature":{"ID":23,"type":42},"instantaneousDemand":{"ID":1024,"type":42},"intervalReadReportingPeriod":{"ID":16,"type":33},"manufactureAlarmMask":{"ID":2055,"type":25},"maxNumberOfPeriodsDelivered":{"ID":1280,"type":32},"meterSerialNumber":{"ID":776,"type":65},"meteringDeviceType":{"ID":774,"type":24},"moduleSerialNumber":{"ID":782,"type":65},"multiplier":{"ID":769,"type":34},"numberOfDemandSubintervals":{"ID":1539,"type":32},"operatingTariffLevel":{"ID":783,"type":65},"outletTempreature":{"ID":24,"type":42},"owonAccumulativeEnergyThreshold":{"ID":20486,"manufacturerCode":4412,"type":32},"owonCurrentSum":{"ID":12547,"manufacturerCode":4412,"type":34},"owonFrequency":{"ID":20485,"manufacturerCode":4412,"type":32},"owonL1Energy":{"ID":16384,"manufacturerCode":4412,"type":37},"owonL1PhaseCurrent":{"ID":12544,"manufacturerCode":4412,"type":34},"owonL1PhasePower":{"ID":8192,"manufacturerCode":4412,"type":42},"owonL1PhaseReactivePower":{"ID":8448,"manufacturerCode":4412,"type":42},"owonL1PhaseVoltage":{"ID":12288,"manufacturerCode":4412,"type":34},"owonL1PowerFactor":{"ID":16644,"manufacturerCode":4412,"type":40},"owonL1ReactiveEnergy":{"ID":16640,"manufacturerCode":4412,"type":37},"owonL2Energy":{"ID":16385,"manufacturerCode":4412,"type":37},"owonL2PhaseCurrent":{"ID":12545,"manufacturerCode":4412,"type":34},"owonL2PhasePower":{"ID":8193,"manufacturerCode":4412,"type":42},"owonL2PhaseReactivePower":{"ID":8449,"manufacturerCode":4412,"type":42},"owonL2PhaseVoltage":{"ID":12289,"manufacturerCode":4412,"type":34},"owonL2PowerFactor":{"ID":16645,"manufacturerCode":4412,"type":40},"owonL2ReactiveEnergy":{"ID":16641,"manufacturerCode":4412,"type":37},"owonL3Energy":{"ID":16386,"manufacturerCode":4412,"type":37},"owonL3PhaseCurrent":{"ID":12546,"manufacturerCode":4412,"type":34},"owonL3PhasePower":{"ID":8194,"manufacturerCode":4412,"type":42},"owonL3PhaseReactivePower":{"ID":8450,"manufacturerCode":4412,"type":42},"owonL3PhaseVoltage":{"ID":12290,"manufacturerCode":4412,"type":34},"owonL3PowerFactor":{"ID":16646,"manufacturerCode":4412,"type":40},"owonL3ReactiveEnergy":{"ID":16642,"manufacturerCode":4412,"type":37},"owonLastHistoricalRecordTime":{"ID":20480,"manufacturerCode":4412,"type":35},"owonLeakageCurrent":{"ID":12548,"manufacturerCode":4412,"type":34},"owonMaximumReportCycle":{"ID":20483,"manufacturerCode":4412,"type":35},"owonMinimumReportCycle":{"ID":20482,"manufacturerCode":4412,"type":35},"owonOldestHistoricalRecordTime":{"ID":20481,"manufacturerCode":4412,"type":35},"owonPercentChangeInPower":{"ID":20488,"manufacturerCode":4412,"type":32},"owonReactiveEnergySum":{"ID":16643,"manufacturerCode":4412,"type":37},"owonReactivePowerSum":{"ID":8451,"manufacturerCode":4412,"type":42},"owonReportMap":{"ID":4096,"manufacturerCode":4412,"type":24},"owonReportMode":{"ID":20487,"manufacturerCode":4412,"type":32},"owonSentHistoricalRecordState":{"ID":20484,"manufacturerCode":4412,"type":32},"powerFactor":{"ID":6,"type":40},"presetReadingTime":{"ID":17,"type":33},"previousDayMaxDemand":{"ID":1038,"type":42},"previousDayMaxPressure":{"ID":1035,"type":37},"previousDayMinPressure":{"ID":1036,"type":37},"previousdayConsumpDelivered":{"ID":1027,"type":34},"previousdayConsumpReceived":{"ID":1028,"type":34},"previousdayMaxEnergyCarrDemand":{"ID":1042,"type":42},"profileIntervalPeriod":{"ID":15,"type":48},"projectedBill":{"ID":2562,"type":35},"projectedBillTimeStamp":{"ID":2563,"type":226},"readingSnapshotTime":{"ID":7,"type":226},"remainingBattLife":{"ID":513,"type":32},"schneiderActiveEnergyDivisor":{"ID":17409,"manufacturerCode":4190,"type":34},"schneiderActiveEnergyL1Phase":{"ID":16643,"manufacturerCode":4190,"type":45},"schneiderActiveEnergyL2Phase":{"ID":16899,"manufacturerCode":4190,"type":45},"schneiderActiveEnergyL3Phase":{"ID":17155,"manufacturerCode":4190,"type":45},"schneiderActiveEnergyMultiplier":{"ID":17408,"manufacturerCode":4190,"type":34},"schneiderActiveEnergyTotal":{"ID":16400,"manufacturerCode":4190,"type":45},"schneiderApparentEnergyDivisor":{"ID":17413,"manufacturerCode":4190,"type":34},"schneiderApparentEnergyL1Phase":{"ID":16645,"manufacturerCode":4190,"type":45},"schneiderApparentEnergyL2Phase":{"ID":16901,"manufacturerCode":4190,"type":45},"schneiderApparentEnergyL3Phase":{"ID":17157,"manufacturerCode":4190,"type":45},"schneiderApparentEnergyMultiplier":{"ID":17412,"manufacturerCode":4190,"type":34},"schneiderApparentEnergyTotal":{"ID":16402,"manufacturerCode":4190,"type":45},"schneiderEnergyCountersReportingPeriod":{"ID":17920,"manufacturerCode":4190,"type":33},"schneiderEnergyResetDateTime":{"ID":17665,"manufacturerCode":4190,"type":226},"schneiderPartialActiveEnergyL1Phase":{"ID":16640,"manufacturerCode":4190,"type":45},"schneiderPartialActiveEnergyL2Phase":{"ID":16896,"manufacturerCode":4190,"type":45},"schneiderPartialActiveEnergyL3Phase":{"ID":17152,"manufacturerCode":4190,"type":45},"schneiderPartialActiveEnergyTotal":{"ID":16404,"manufacturerCode":4190,"type":45},"schneiderPartialApparentEnergyL1Phase":{"ID":16642,"manufacturerCode":4190,"type":45},"schneiderPartialApparentEnergyL2Phase":{"ID":16898,"manufacturerCode":4190,"type":45},"schneiderPartialApparentEnergyL3Phase":{"ID":17154,"manufacturerCode":4190,"type":45},"schneiderPartialApparentEnergyTotal":{"ID":16406,"manufacturerCode":4190,"type":45},"schneiderPartialReactiveEnergyL1Phase":{"ID":16641,"manufacturerCode":4190,"type":45},"schneiderPartialReactiveEnergyL2Phase":{"ID":16897,"manufacturerCode":4190,"type":45},"schneiderPartialReactiveEnergyL3Phase":{"ID":17153,"manufacturerCode":4190,"type":45},"schneiderPartialReactiveEnergyTotal":{"ID":16405,"manufacturerCode":4190,"type":45},"schneiderReactiveEnergyDivisor":{"ID":17411,"manufacturerCode":4190,"type":34},"schneiderReactiveEnergyL1Phase":{"ID":16644,"manufacturerCode":4190,"type":45},"schneiderReactiveEnergyL2Phase":{"ID":16900,"manufacturerCode":4190,"type":45},"schneiderReactiveEnergyL3Phase":{"ID":17156,"manufacturerCode":4190,"type":45},"schneiderReactiveEnergyMultiplier":{"ID":17410,"manufacturerCode":4190,"type":34},"schneiderReactiveEnergyTotal":{"ID":16401,"manufacturerCode":4190,"type":45},"siteId":{"ID":775,"type":65},"status":{"ID":512,"type":24},"summaFormatting":{"ID":771,"type":24},"supplyStatus":{"ID":20,"type":48},"temperatureFormatting":{"ID":781,"type":24},"temperatureUnitOfMeas":{"ID":780,"type":48},"unitOfMeasure":{"ID":768,"type":48},"volumePerReport":{"ID":18,"type":33},"waterSpecificAlarmMask":{"ID":2051,"type":25}},"commands":{"getProfile":{"ID":0,"parameters":[]},"getSnapshot":{"ID":4,"parameters":[]},"mirrorRem":{"ID":2,"parameters":[]},"mirrorReportAttrRsp":{"ID":6,"parameters":[]},"owonGetHistoryRecord":{"ID":32,"parameters":[]},"owonStopSendingHistoricalRecord":{"ID":33,"parameters":[]},"reqFastPollMode":{"ID":3,"parameters":[]},"reqMirror":{"ID":1,"parameters":[]},"takeSnapshot":{"ID":5,"parameters":[]}},"commandsResponse":{"getProfileRsp":{"ID":0,"parameters":[]},"getSnapshotRsp":{"ID":4,"parameters":[]},"mirrorRemRsp":{"ID":2,"parameters":[]},"owonGetHistoryRecordRsp":{"ID":32,"parameters":[]},"reqFastPollModeRsp":{"ID":3,"parameters":[]},"reqMirrorRsp":{"ID":1,"parameters":[]}}},"sprutDevice":{"ID":26112,"attributes":{"debug":{"ID":0,"type":16}},"commands":{},"commandsResponse":{},"manufacturerCode":26214},"sprutIrBlaster":{"ID":26115,"attributes":{},"commands":{"clearStore":{"ID":3,"parameters":[]},"learnRamStart":{"ID":5,"parameters":[]},"learnRamStop":{"ID":6,"parameters":[]},"learnStart":{"ID":1,"parameters":[{"name":"value","type":32}]},"learnStop":{"ID":2,"parameters":[{"name":"value","type":32}]},"playRam":{"ID":4,"parameters":[]},"playStore":{"ID":0,"parameters":[{"name":"param","type":32}]}},"commandsResponse":{},"manufacturerCode":26214},"sprutNoise":{"ID":26114,"attributes":{"noise":{"ID":26112,"type":57},"noiseAfterDetectDelay":{"ID":26115,"type":33},"noiseDetectLevel":{"ID":26114,"type":57},"noiseDetected":{"ID":26113,"type":24}},"commands":{},"commandsResponse":{},"manufacturerCode":26214},"sprutVoc":{"ID":26113,"attributes":{"voc":{"ID":26112,"type":33}},"commands":{},"commandsResponse":{},"manufacturerCode":26214},"ssIasAce":{"ID":1281,"attributes":{},"commands":{"arm":{"ID":0,"parameters":[{"name":"armmode","type":32},{"name":"code","type":66},{"name":"zoneid","type":32}],"response":0},"bypass":{"ID":1,"parameters":[{"name":"numofzones","type":32},{"name":"zoneidlist","type":1001}]},"emergency":{"ID":2,"parameters":[]},"fire":{"ID":3,"parameters":[]},"getBypassedZoneList":{"ID":8,"parameters":[]},"getPanelStatus":{"ID":7,"parameters":[],"response":5},"getZoneIDMap":{"ID":5,"parameters":[],"response":1},"getZoneInfo":{"ID":6,"parameters":[{"name":"zoneid","type":32}],"response":2},"getZoneStatus":{"ID":9,"parameters":[{"name":"startzoneid","type":32},{"name":"maxnumzoneid","type":32},{"name":"zonestatusmaskflag","type":32},{"name":"zonestatusmask","type":33}],"response":8},"panic":{"ID":4,"parameters":[]}},"commandsResponse":{"armRsp":{"ID":0,"parameters":[{"name":"armnotification","type":32}]},"bypassRsp":{"ID":7,"parameters":[{"name":"numofzones","type":32},{"name":"bypassresult","type":1001}]},"getPanelStatusRsp":{"ID":5,"parameters":[{"name":"panelstatus","type":32},{"name":"secondsremain","type":32},{"name":"audiblenotif","type":32},{"name":"alarmstatus","type":32}]},"getZoneIDMapRsp":{"ID":1,"parameters":[{"name":"zoneidmapsection0","type":33},{"name":"zoneidmapsection1","type":33},{"name":"zoneidmapsection2","type":33},{"name":"zoneidmapsection3","type":33},{"name":"zoneidmapsection4","type":33},{"name":"zoneidmapsection5","type":33},{"name":"zoneidmapsection6","type":33},{"name":"zoneidmapsection7","type":33},{"name":"zoneidmapsection8","type":33},{"name":"zoneidmapsection9","type":33},{"name":"zoneidmapsection10","type":33},{"name":"zoneidmapsection11","type":33},{"name":"zoneidmapsection12","type":33},{"name":"zoneidmapsection13","type":33},{"name":"zoneidmapsection14","type":33},{"name":"zoneidmapsection15","type":33}]},"getZoneInfoRsp":{"ID":2,"parameters":[{"name":"zoneid","type":32},{"name":"zonetype","type":33},{"name":"ieeeaddr","type":240},{"name":"zonelabel","type":66}]},"getZoneStatusRsp":{"ID":8,"parameters":[{"name":"zonestatuscomplete","type":32},{"name":"numofzones","type":32},{"name":"zoneinfo","type":1005}]},"panelStatusChanged":{"ID":4,"parameters":[{"name":"panelstatus","type":32},{"name":"secondsremain","type":32},{"name":"audiblenotif","type":32},{"name":"alarmstatus","type":32}]},"setBypassedZoneList":{"ID":6,"parameters":[{"name":"numofzones","type":32},{"name":"zoneid","type":1001}]},"zoneStatusChanged":{"ID":3,"parameters":[{"name":"zoneid","type":32},{"name":"zonestatus","type":33},{"name":"audiblenotif","type":32},{"name":"zonelabel","type":66}]}}},"ssIasWd":{"ID":1282,"attributes":{"maxDuration":{"ID":0,"type":33}},"commands":{"squawk":{"ID":1,"parameters":[{"name":"squawkinfo","type":32}]},"startWarning":{"ID":0,"parameters":[{"name":"startwarninginfo","type":32},{"name":"warningduration","type":33},{"name":"strobedutycycle","type":32},{"name":"strobelevel","type":32}]}},"commandsResponse":{}},"ssIasZone":{"ID":1280,"attributes":{"currentZoneSensitivityLevel":{"ID":19,"type":32},"develcoAlarmOffDelay":{"ID":32769,"manufacturerCode":4117,"type":33},"iasCieAddr":{"ID":16,"type":240},"numZoneSensitivityLevelsSupported":{"ID":18,"type":32},"zoneId":{"ID":17,"type":32},"zoneState":{"ID":0,"type":48},"zoneStatus":{"ID":2,"type":25},"zoneType":{"ID":1,"type":49}},"commands":{"enrollRsp":{"ID":0,"parameters":[{"name":"enrollrspcode","type":32},{"name":"zoneid","type":32}]},"initNormalOpMode":{"ID":1,"parameters":[]},"initTestMode":{"ID":2,"parameters":[]}},"commandsResponse":{"enrollReq":{"ID":1,"parameters":[{"name":"zonetype","type":33},{"name":"manucode","type":33}]},"statusChangeNotification":{"ID":0,"parameters":[{"name":"zonestatus","type":33},{"name":"extendedstatus","type":32}]}}},"telecommunicationsChatting":{"ID":2309,"attributes":{"cID":{"ID":16,"type":33},"enableAddChat":{"ID":18,"type":16},"name":{"ID":17,"type":66},"nickname":{"ID":1,"type":66},"uID":{"ID":0,"type":33}},"commands":{},"commandsResponse":{}},"telecommunicationsInformation":{"ID":2304,"attributes":{"contentRootID":{"ID":17,"type":33},"deliveryEnable":{"ID":1,"type":16},"enableSecureConfiguration":{"ID":3,"type":16},"nodeDescription":{"ID":0,"type":66},"numberOfContents":{"ID":16,"type":33},"pushInformationTimer":{"ID":2,"type":35}},"commands":{},"commandsResponse":{}},"telecommunicationsVoiceOverZigbee":{"ID":2308,"attributes":{"codecType":{"ID":0,"type":48},"codecTypeSub1":{"ID":4,"type":48},"codecTypeSub2":{"ID":5,"type":48},"codecTypeSub3":{"ID":6,"type":48},"codecrate":{"ID":2,"type":48},"compressionRate":{"ID":8,"type":48},"compressionType":{"ID":7,"type":48},"establishmentTimeout":{"ID":3,"type":32},"optionFlags":{"ID":9,"type":24},"samplingFrequency":{"ID":1,"type":48},"threshold":{"ID":10,"type":32}},"commands":{},"commandsResponse":{}},"touchlink":{"ID":4096,"attributes":{},"commands":{"identifyRequest":{"ID":6,"parameters":[{"name":"transactionID","type":35},{"name":"duration","type":33}]},"resetToFactoryNew":{"ID":7,"parameters":[{"name":"transactionID","type":35}]},"scanRequest":{"ID":0,"parameters":[{"name":"transactionID","type":35},{"name":"zigbeeInformation","type":24},{"name":"touchlinkInformation","type":24}],"response":1}},"commandsResponse":{"scanResponse":{"ID":1,"parameters":[{"name":"transactionID","type":35},{"name":"rssiCorrection","type":32},{"name":"zigbeeInformation","type":32},{"name":"touchlinkInformation","type":32},{"name":"keyBitmask","type":33},{"name":"responseID","type":35},{"name":"extendedPanID","type":240},{"name":"networkUpdateID","type":32},{"name":"logicalChannel","type":32},{"name":"panID","type":33},{"name":"networkAddress","type":33},{"name":"numberOfSubDevices","type":32},{"name":"totalGroupIdentifiers","type":32}]}}},"tradfriButton":{"ID":64640,"attributes":{},"commands":{"action1":{"ID":1,"parameters":[{"name":"data","type":32}]},"action2":{"ID":2,"parameters":[{"name":"data","type":32}]},"action3":{"ID":3,"parameters":[{"name":"data","type":32}]},"action4":{"ID":4,"parameters":[{"name":"data","type":32}]},"action6":{"ID":6,"parameters":[{"name":"data","type":32}]}},"commandsResponse":{},"manufacturerCode":4476},"tunneling":{"ID":1796,"attributes":{},"commands":{"transferData":{"ID":2,"parameters":[{"name":"tunnelID","type":33},{"name":"data","type":1008}]}},"commandsResponse":{"transferDataResp":{"ID":1,"parameters":[{"name":"tunnelID","type":33},{"name":"data","type":1008}]}}},"wiserDeviceInfo":{"ID":65027,"attributes":{"deviceInfo":{"ID":32,"type":66}},"commands":{},"commandsResponse":{}},"zosungIRControl":{"ID":57348,"attributes":{},"commands":{"zosungControlIRCommand00":{"ID":0,"parameters":[{"name":"data","type":1008}]}},"commandsResponse":{}},"zosungIRTransmit":{"ID":60672,"attributes":{},"commands":{"zosungSendIRCode00":{"ID":0,"parameters":[{"name":"seq","type":33},{"name":"length","type":35},{"name":"unk1","type":35},{"name":"unk2","type":33},{"name":"unk3","type":32},{"name":"cmd","type":32},{"name":"unk4","type":33}]},"zosungSendIRCode01":{"ID":1,"parameters":[{"name":"zero","type":32},{"name":"seq","type":33},{"name":"length","type":35},{"name":"unk1","type":35},{"name":"unk2","type":33},{"name":"unk3","type":32},{"name":"cmd","type":32},{"name":"unk4","type":33}]},"zosungSendIRCode02":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"position","type":35},{"name":"maxlen","type":32}]},"zosungSendIRCode03":{"ID":3,"parameters":[{"name":"zero","type":32},{"name":"seq","type":33},{"name":"position","type":35},{"name":"msgpart","type":65},{"name":"msgpartcrc","type":32}]},"zosungSendIRCode04":{"ID":4,"parameters":[{"name":"zero0","type":32},{"name":"seq","type":33},{"name":"zero1","type":33}]},"zosungSendIRCode05":{"ID":5,"parameters":[{"name":"seq","type":33},{"name":"zero","type":33}]}},"commandsResponse":{"zosungSendIRCode03Resp":{"ID":3,"parameters":[{"name":"zero","type":32},{"name":"seq","type":33},{"name":"position","type":35},{"name":"msgpart","type":65},{"name":"msgpartcrc","type":32}]},"zosungSendIRCode05Resp":{"ID":5,"parameters":[{"name":"seq","type":33},{"name":"zero","type":33}]}}}},"custom_clusters":{}}'
[2025-01-19 22:58:11] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/bridge/extensions' with data '[]'
[2025-01-19 22:58:11] info: 	z2m: Started frontend on port 8080
[2025-01-19 22:58:12] debug: 	z2m: Discovering entities to Home Assistant in 5s
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/light/milight_hub_3346011/rgb_cct_0x1_1/config' with data '{"schema":"json","name":"Wohnzimmer 1","command_topic":"milight/0x1/rgb_cct/1","state_topic":"milight/states/0x1/rgb_cct/1","uniq_id":"330E5B-Wohnzimmer 1","device":{"manufacturer":"esp8266_milight_hub","sw_version":"1.10.7","identifiers":[3346011,1,"rgb_cct",1]},"availability_topic":"milight/client_status","payload_available":"connected","payload_not_available":"disconnected","brightness":true,"effect":true,"effect_list":["night_mode","white_mode","0","1","2","3","4","5","6","7","8"],"rgb":true,"color_temp":true}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/light/milight_hub_3346011/rgb_cct_0x1_2/config' with data '{"schema":"json","name":"Wohnzimmer 2","command_topic":"milight/0x1/rgb_cct/2","state_topic":"milight/states/0x1/rgb_cct/2","uniq_id":"330E5B-Wohnzimmer 2","device":{"manufacturer":"esp8266_milight_hub","sw_version":"1.10.7","identifiers":[3346011,1,"rgb_cct",2]},"availability_topic":"milight/client_status","payload_available":"connected","payload_not_available":"disconnected","brightness":true,"effect":true,"effect_list":["night_mode","white_mode","0","1","2","3","4","5","6","7","8"],"rgb":true,"color_temp":true}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/light/milight_hub_3346011/rgb_cct_0x1_0/config' with data '{"schema":"json","name":"Wohnzimmer Alle","command_topic":"milight/0x1/rgb_cct/0","state_topic":"milight/states/0x1/rgb_cct/0","uniq_id":"330E5B-Wohnzimmer Alle","device":{"manufacturer":"esp8266_milight_hub","sw_version":"1.10.7","identifiers":[3346011,1,"rgb_cct",0]},"availability_topic":"milight/client_status","payload_available":"connected","payload_not_available":"disconnected","brightness":true,"effect":true,"effect_list":["night_mode","white_mode","0","1","2","3","4","5","6","7","8"],"rgb":true,"color_temp":true}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/light/0xf0d1b800001ffcf2/light/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"brightness":true,"brightness_scale":254,"command_topic":"zigbee2mqtt/Bogenlampe/set","device":{"hw_version":2,"identifiers":["zigbee2mqtt_0xf0d1b800001ffcf2"],"manufacturer":"LEDVANCE","model":"SMART+ lamp E27 RGBW","model_id":"4058075208391","name":"Bogenlampe","sw_version":"03197310","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"effect":true,"effect_list":["blink","breathe","okay","channel_change","finish_effect","stop_effect","colorloop","stop_colorloop"],"max_mireds":370,"min_mireds":153,"name":null,"object_id":"bogenlampe","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"schema":"json","state_topic":"zigbee2mqtt/Bogenlampe","supported_color_modes":["xy","color_temp"],"unique_id":"0xf0d1b800001ffcf2_light_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/light/0xa4c138541ec8ddd2/light/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"brightness":true,"brightness_scale":254,"command_topic":"zigbee2mqtt/Flur/set","device":{"hw_version":0,"identifiers":["zigbee2mqtt_0xa4c138541ec8ddd2"],"manufacturer":"AwoX","model":"LED white","model_id":"33951/33948","name":"Flur","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"effect":true,"effect_list":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"name":null,"object_id":"flur","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"schema":"json","state_topic":"zigbee2mqtt/Flur","unique_id":"0xa4c138541ec8ddd2_light_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/light/0x001788010d1c884e/light/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"brightness":true,"brightness_scale":254,"command_topic":"zigbee2mqtt/Badlampe/set","device":{"hw_version":0,"identifiers":["zigbee2mqtt_0x001788010d1c884e"],"manufacturer":"Philips","model":"Hue Devere M white ambiance white & dimmer","model_id":"915005997601","name":"Badlampe","sw_version":"1.93.7","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"effect":true,"effect_list":["blink","breathe","okay","channel_change","candle","finish_effect","stop_effect","stop_hue_effect"],"max_mireds":454,"min_mireds":153,"name":null,"object_id":"badlampe","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"schema":"json","state_topic":"zigbee2mqtt/Badlampe","supported_color_modes":["color_temp"],"unique_id":"0x001788010d1c884e_light_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/light/0x00158d00053a1aab/light/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"brightness":true,"brightness_scale":254,"command_topic":"zigbee2mqtt/0x00158d00053a1aab/set","device":{"hw_version":21,"identifiers":["zigbee2mqtt_0x00158d00053a1aab"],"manufacturer":"Paulmann","model":"SmartHome led spot","model_id":"50064","name":"0x00158d00053a1aab","sw_version":"00.00.01","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"effect":true,"effect_list":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"max_mireds":500,"min_mireds":150,"name":null,"object_id":"0x00158d00053a1aab","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"schema":"json","state_topic":"zigbee2mqtt/0x00158d00053a1aab","supported_color_modes":["color_temp"],"unique_id":"0x00158d00053a1aab_light_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/light/0x00158d00053c6311/light/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"brightness":true,"brightness_scale":254,"command_topic":"zigbee2mqtt/0x00158d00053c6311/set","device":{"hw_version":21,"identifiers":["zigbee2mqtt_0x00158d00053c6311"],"manufacturer":"Paulmann","model":"SmartHome led spot","model_id":"50064","name":"0x00158d00053c6311","sw_version":"00.00.01","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"effect":true,"effect_list":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"max_mireds":500,"min_mireds":150,"name":null,"object_id":"0x00158d00053c6311","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"schema":"json","state_topic":"zigbee2mqtt/0x00158d00053c6311","supported_color_modes":["color_temp"],"unique_id":"0x00158d00053c6311_light_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/light/0xf0d1b800001388f0/light/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"brightness":true,"brightness_scale":254,"command_topic":"zigbee2mqtt/Flurlicht/set","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xf0d1b800001388f0"],"manufacturer":"OSRAM","model":"SMART+ Candle E14 Dimmable White","model_id":"AC08562","name":"Flurlicht","sw_version":"01056400","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"effect":true,"effect_list":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"name":null,"object_id":"flurlicht","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"schema":"json","state_topic":"zigbee2mqtt/Flurlicht","unique_id":"0xf0d1b800001388f0_light_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/light/0x7cb03eaa0a0176bd/light/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"brightness":true,"brightness_scale":254,"command_topic":"zigbee2mqtt/Küchentisch/set","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x7cb03eaa0a0176bd"],"manufacturer":"OSRAM","model":"LIGHTIFY LED Classic A60 clear","model_id":"AC03641","name":"Küchentisch","sw_version":"V1.05.10","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"effect":true,"effect_list":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"name":null,"object_id":"küchentisch","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"schema":"json","state_topic":"zigbee2mqtt/Küchentisch","unique_id":"0x7cb03eaa0a0176bd_light_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/light/0x00212effff0cb8b6/light/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"brightness":true,"brightness_scale":254,"command_topic":"zigbee2mqtt/Lichtschlauch/set","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x00212effff0cb8b6"],"manufacturer":"dresden elektronik\u0000","model":"Automatically generated definition","model_id":"FLS-PP3 White\u0000","name":"Lichtschlauch","sw_version":"0214.201000F6\u0000","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"effect":true,"effect_list":["blink","breathe","okay","channel_change","finish_effect","stop_effect","colorloop","stop_colorloop"],"name":null,"object_id":"lichtschlauch","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"schema":"json","state_topic":"zigbee2mqtt/Lichtschlauch","unique_id":"0x00212effff0cb8b6_light_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/binary_sensor/1221051039810110150109113116116_0x00212effff04fc2c/connection_state/config' with data '{"device":{"hw_version":"ConBee2/RaspBee2 0x26580700","identifiers":["zigbee2mqtt_bridge_0x00212effff04fc2c"],"manufacturer":"Zigbee2MQTT","model":"Bridge","name":"Zigbee2MQTT Bridge","sw_version":"2.0.0"},"device_class":"connectivity","entity_category":"diagnostic","name":"Connection state","object_id":"zigbee2mqtt_bridge_connection_state","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_off":"offline","payload_on":"online","state_topic":"zigbee2mqtt/bridge/state","unique_id":"bridge_0x00212effff04fc2c_connection_state_zigbee2mqtt","value_template":"{{ value_json.state }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/binary_sensor/1221051039810110150109113116116_0x00212effff04fc2c/restart_required/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"availability_mode":"all","device":{"hw_version":"ConBee2/RaspBee2 0x26580700","identifiers":["zigbee2mqtt_bridge_0x00212effff04fc2c"],"manufacturer":"Zigbee2MQTT","model":"Bridge","name":"Zigbee2MQTT Bridge","sw_version":"2.0.0"},"device_class":"problem","enabled_by_default":false,"entity_category":"diagnostic","name":"Restart required","object_id":"zigbee2mqtt_bridge_restart_required","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_off":false,"payload_on":true,"state_topic":"zigbee2mqtt/bridge/info","unique_id":"bridge_0x00212effff04fc2c_restart_required_zigbee2mqtt","value_template":"{{ value_json.restart_required }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/binary_sensor/0xa4c1384187f0960d/water_leak/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"identifiers":["zigbee2mqtt_0xa4c1384187f0960d"],"manufacturer":"Aubess","model":"Water leak sensor","model_id":"IH-K665","name":"Wasser Sensor Spüle","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"moisture","object_id":"wasser_sensor_spüle_water_leak","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_off":false,"payload_on":true,"state_topic":"zigbee2mqtt/Wasser Sensor Spüle","unique_id":"0xa4c1384187f0960d_water_leak_zigbee2mqtt","value_template":"{{ value_json.water_leak }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/binary_sensor/0xa4c1384187f0960d/battery_low/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"identifiers":["zigbee2mqtt_0xa4c1384187f0960d"],"manufacturer":"Aubess","model":"Water leak sensor","model_id":"IH-K665","name":"Wasser Sensor Spüle","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","entity_category":"diagnostic","object_id":"wasser_sensor_spüle_battery_low","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_off":false,"payload_on":true,"state_topic":"zigbee2mqtt/Wasser Sensor Spüle","unique_id":"0xa4c1384187f0960d_battery_low_zigbee2mqtt","value_template":"{{ value_json.battery_low }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/binary_sensor/0xa4c13864e6c8c400/occupancy/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c13864e6c8c400"],"manufacturer":"Tuya","model":"Motion sensor","model_id":"809WZT","name":"Bewegungsmelder 1","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"occupancy","object_id":"bewegungsmelder_1_occupancy","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_off":false,"payload_on":true,"state_topic":"zigbee2mqtt/Bewegungsmelder 1","unique_id":"0xa4c13864e6c8c400_occupancy_zigbee2mqtt","value_template":"{{ value_json.occupancy }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/binary_sensor/0xa4c13864e6c8c400/battery_low/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c13864e6c8c400"],"manufacturer":"Tuya","model":"Motion sensor","model_id":"809WZT","name":"Bewegungsmelder 1","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","entity_category":"diagnostic","object_id":"bewegungsmelder_1_battery_low","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_off":false,"payload_on":true,"state_topic":"zigbee2mqtt/Bewegungsmelder 1","unique_id":"0xa4c13864e6c8c400_battery_low_zigbee2mqtt","value_template":"{{ value_json.battery_low }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/binary_sensor/0xa4c13864e6c8c400/tamper/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c13864e6c8c400"],"manufacturer":"Tuya","model":"Motion sensor","model_id":"809WZT","name":"Bewegungsmelder 1","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"tamper","object_id":"bewegungsmelder_1_tamper","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_off":false,"payload_on":true,"state_topic":"zigbee2mqtt/Bewegungsmelder 1","unique_id":"0xa4c13864e6c8c400_tamper_zigbee2mqtt","value_template":"{{ value_json.tamper }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/binary_sensor/0xa4c138ef60e2fdbe/contact/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c138ef60e2fdbe"],"manufacturer":"Tuya","model":"Door sensor","model_id":"TS0203","name":"Sensor Terassentür","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"door","object_id":"sensor_terassentür_contact","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_off":true,"payload_on":false,"state_topic":"zigbee2mqtt/Sensor Terassentür","unique_id":"0xa4c138ef60e2fdbe_contact_zigbee2mqtt","value_template":"{{ value_json.contact }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/binary_sensor/0xa4c138ef60e2fdbe/tamper/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c138ef60e2fdbe"],"manufacturer":"Tuya","model":"Door sensor","model_id":"TS0203","name":"Sensor Terassentür","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"tamper","object_id":"sensor_terassentür_tamper","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_off":false,"payload_on":true,"state_topic":"zigbee2mqtt/Sensor Terassentür","unique_id":"0xa4c138ef60e2fdbe_tamper_zigbee2mqtt","value_template":"{{ value_json.tamper }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/binary_sensor/0xa4c138e68023f4c6/water_leak/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":0,"identifiers":["zigbee2mqtt_0xa4c138e68023f4c6"],"manufacturer":"eWeLink","model":"Zigbee water sensor","model_id":"SNZB-05","name":"Wassersensor Keller","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"moisture","object_id":"wassersensor_keller_water_leak","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_off":false,"payload_on":true,"state_topic":"zigbee2mqtt/Wassersensor Keller","unique_id":"0xa4c138e68023f4c6_water_leak_zigbee2mqtt","value_template":"{{ value_json.water_leak }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/binary_sensor/0xa4c138e68023f4c6/battery_low/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":0,"identifiers":["zigbee2mqtt_0xa4c138e68023f4c6"],"manufacturer":"eWeLink","model":"Zigbee water sensor","model_id":"SNZB-05","name":"Wassersensor Keller","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","entity_category":"diagnostic","object_id":"wassersensor_keller_battery_low","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_off":false,"payload_on":true,"state_topic":"zigbee2mqtt/Wassersensor Keller","unique_id":"0xa4c138e68023f4c6_battery_low_zigbee2mqtt","value_template":"{{ value_json.battery_low }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/button/1221051039810110150109113116116_0x00212effff04fc2c/restart/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"availability_mode":"all","command_topic":"zigbee2mqtt/bridge/request/restart","device":{"hw_version":"ConBee2/RaspBee2 0x26580700","identifiers":["zigbee2mqtt_bridge_0x00212effff04fc2c"],"manufacturer":"Zigbee2MQTT","model":"Bridge","name":"Zigbee2MQTT Bridge","sw_version":"2.0.0"},"device_class":"restart","name":"Restart","object_id":"zigbee2mqtt_bridge_restart","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_press":"","unique_id":"bridge_0x00212effff04fc2c_restart_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/1221051039810110150109113116116_0x00212effff04fc2c/log_level/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"availability_mode":"all","command_template":"{\"options\": {\"advanced\": {\"log_level\": \"{{ value }}\" } } }","command_topic":"zigbee2mqtt/bridge/request/options","device":{"hw_version":"ConBee2/RaspBee2 0x26580700","identifiers":["zigbee2mqtt_bridge_0x00212effff04fc2c"],"manufacturer":"Zigbee2MQTT","model":"Bridge","name":"Zigbee2MQTT Bridge","sw_version":"2.0.0"},"entity_category":"config","name":"Log level","object_id":"zigbee2mqtt_bridge_log_level","options":["error","warning","info","debug"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/bridge/info","unique_id":"bridge_0x00212effff04fc2c_log_level_zigbee2mqtt","value_template":"{{ value_json.log_level | lower }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0xf0d1b800001ffcf2/effect/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Bogenlampe/set/effect","device":{"hw_version":2,"identifiers":["zigbee2mqtt_0xf0d1b800001ffcf2"],"manufacturer":"LEDVANCE","model":"SMART+ lamp E27 RGBW","model_id":"4058075208391","name":"Bogenlampe","sw_version":"03197310","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"icon":"mdi:palette","name":"Effect","object_id":"bogenlampe_effect","options":["blink","breathe","okay","channel_change","finish_effect","stop_effect","colorloop","stop_colorloop"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"unique_id":"0xf0d1b800001ffcf2_effect_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0xa4c138541ec8ddd2/effect/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Flur/set/effect","device":{"hw_version":0,"identifiers":["zigbee2mqtt_0xa4c138541ec8ddd2"],"manufacturer":"AwoX","model":"LED white","model_id":"33951/33948","name":"Flur","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"icon":"mdi:palette","name":"Effect","object_id":"flur_effect","options":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"unique_id":"0xa4c138541ec8ddd2_effect_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0xa4c138541ec8ddd2/power_on_behavior/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Flur/set/power_on_behavior","device":{"hw_version":0,"identifiers":["zigbee2mqtt_0xa4c138541ec8ddd2"],"manufacturer":"AwoX","model":"LED white","model_id":"33951/33948","name":"Flur","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"entity_category":"config","icon":"mdi:power-settings","name":"Power-on behavior","object_id":"flur_power_on_behavior","options":["off","on","toggle","previous"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/Flur","unique_id":"0xa4c138541ec8ddd2_power_on_behavior_zigbee2mqtt","value_template":"{{ value_json.power_on_behavior }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0x001788010d1c884e/power_on_behavior/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Badlampe/set/power_on_behavior","device":{"hw_version":0,"identifiers":["zigbee2mqtt_0x001788010d1c884e"],"manufacturer":"Philips","model":"Hue Devere M white ambiance white & dimmer","model_id":"915005997601","name":"Badlampe","sw_version":"1.93.7","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"entity_category":"config","icon":"mdi:power-settings","name":"Power-on behavior","object_id":"badlampe_power_on_behavior","options":["off","on","toggle","previous"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/Badlampe","unique_id":"0x001788010d1c884e_power_on_behavior_zigbee2mqtt","value_template":"{{ value_json.power_on_behavior }}"}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Fernbedienung', payload '{"battery":100,"linkquality":247,"update":{"installed_version":-1,"latest_version":-1,"state":null},"voltage":3000}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":159,"state":"OFF","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/0xa4c138570b1956d9', payload '{"battery":20,"humidity":64.87,"linkquality":7,"temperature":22.35,"voltage":null}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/0xa4c1383ec7aa7d95', payload '{"battery":26,"humidity":58.31,"linkquality":255,"temperature":23.81,"voltage":null}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/0xa4c1383db5531833', payload '{"battery":17,"humidity":73.5,"linkquality":87,"temperature":20.4,"update":{"installed_version":268513281,"latest_version":268513281,"state":"idle"},"voltage":null}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Lichtschlauch', payload '{"brightness_rgb":26,"brightness_white":254,"color":{"x":0.6942,"y":0.2963},"color_mode":"xy","color_mode_rgb":"color_temp","color_mode_white":"color_temp","color_rgb":{"x":0.3445,"y":0.3512},"color_temp_rgb":199,"color_temp_white":365,"color_white":{"x":0.4566,"y":0.4098},"effect":null,"linkquality":255,"power_on_behavior":null,"state":"OFF","state_10":"OFF","state_rgb":"OFF","state_white":"OFF"}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/0x0ceff6fffebf4739', payload '{"linkquality":119}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Flur', payload '{"brightness":152,"effect":null,"linkquality":255,"power_on_behavior":null,"state":"ON"}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Wasser Sensor Spüle', payload '{"battery":100,"battery_low":false,"linkquality":207,"tamper":false,"voltage":2800,"water_leak":false}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Badlampe', payload '{"brightness":254,"color_mode":"color_temp","color_temp":366,"effect":null,"linkquality":87,"power_on_behavior":null,"state":"ON","update":{"installed_version":16784652,"latest_version":16786434,"state":"available"}}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Fernbedienung Bad', payload '{"battery":100,"linkquality":255,"update":{"installed_version":33565954,"latest_version":33565954,"state":"idle"}}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/0x00158d00053a1aab', payload '{"color_mode":"xy","effect":null,"linkquality":255,"power_on_behavior":null,"state":null}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/0x00158d00053c6311', payload '{"color_mode":"xy","effect":null,"linkquality":255,"power_on_behavior":null,"state":"ON"}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bewegungsmelder 1', payload '{"battery":93,"battery_low":false,"linkquality":255,"occupancy":false,"tamper":false,"voltage":2900}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Sensor Terassentür', payload '{"battery":100,"battery_low":false,"contact":true,"linkquality":239,"tamper":false,"voltage":2800}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Flurlicht', payload '{"brightness":229,"effect":null,"linkquality":255,"state":"ON","update":{"installed_version":17130496,"latest_version":17130496,"state":"idle"}}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Küchentisch', payload '{"brightness":254,"effect":null,"linkquality":255,"state":"OFF","update":{"installed_version":16909584,"latest_version":16909584,"state":"idle"}}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Fernbedienung 2', payload '{"battery":100,"linkquality":239,"update":{"installed_version":-1,"latest_version":-1,"state":null},"voltage":3000}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Wassersensor Keller', payload '{"battery":100,"battery_low":false,"linkquality":255,"water_leak":false}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":43,"humidity_calibration":0,"linkquality":255,"temperature":29,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 22:58:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Temperatur Keller', payload '{"battery":100,"humidity":43,"humidity_calibration":0,"linkquality":63,"temperature":20.9,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 22:58:12] info: 	z2m: Zigbee2MQTT started!
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0x001788010d1c884e/effect/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Badlampe/set/effect","device":{"hw_version":0,"identifiers":["zigbee2mqtt_0x001788010d1c884e"],"manufacturer":"Philips","model":"Hue Devere M white ambiance white & dimmer","model_id":"915005997601","name":"Badlampe","sw_version":"1.93.7","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"icon":"mdi:palette","name":"Effect","object_id":"badlampe_effect","options":["blink","breathe","okay","channel_change","candle","finish_effect","stop_effect","stop_hue_effect"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"unique_id":"0x001788010d1c884e_effect_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0x00158d00053a1aab/effect/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/0x00158d00053a1aab/set/effect","device":{"hw_version":21,"identifiers":["zigbee2mqtt_0x00158d00053a1aab"],"manufacturer":"Paulmann","model":"SmartHome led spot","model_id":"50064","name":"0x00158d00053a1aab","sw_version":"00.00.01","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"icon":"mdi:palette","name":"Effect","object_id":"0x00158d00053a1aab_effect","options":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"unique_id":"0x00158d00053a1aab_effect_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0x00158d00053a1aab/power_on_behavior/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/0x00158d00053a1aab/set/power_on_behavior","device":{"hw_version":21,"identifiers":["zigbee2mqtt_0x00158d00053a1aab"],"manufacturer":"Paulmann","model":"SmartHome led spot","model_id":"50064","name":"0x00158d00053a1aab","sw_version":"00.00.01","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"entity_category":"config","icon":"mdi:power-settings","name":"Power-on behavior","object_id":"0x00158d00053a1aab_power_on_behavior","options":["off","on","toggle","previous"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/0x00158d00053a1aab","unique_id":"0x00158d00053a1aab_power_on_behavior_zigbee2mqtt","value_template":"{{ value_json.power_on_behavior }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0x00158d00053c6311/effect/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/0x00158d00053c6311/set/effect","device":{"hw_version":21,"identifiers":["zigbee2mqtt_0x00158d00053c6311"],"manufacturer":"Paulmann","model":"SmartHome led spot","model_id":"50064","name":"0x00158d00053c6311","sw_version":"00.00.01","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"icon":"mdi:palette","name":"Effect","object_id":"0x00158d00053c6311_effect","options":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"unique_id":"0x00158d00053c6311_effect_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0x00158d00053c6311/power_on_behavior/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/0x00158d00053c6311/set/power_on_behavior","device":{"hw_version":21,"identifiers":["zigbee2mqtt_0x00158d00053c6311"],"manufacturer":"Paulmann","model":"SmartHome led spot","model_id":"50064","name":"0x00158d00053c6311","sw_version":"00.00.01","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"entity_category":"config","icon":"mdi:power-settings","name":"Power-on behavior","object_id":"0x00158d00053c6311_power_on_behavior","options":["off","on","toggle","previous"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/0x00158d00053c6311","unique_id":"0x00158d00053c6311_power_on_behavior_zigbee2mqtt","value_template":"{{ value_json.power_on_behavior }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0x7cb03eaa0a0176bd/effect/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Küchentisch/set/effect","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x7cb03eaa0a0176bd"],"manufacturer":"OSRAM","model":"LIGHTIFY LED Classic A60 clear","model_id":"AC03641","name":"Küchentisch","sw_version":"V1.05.10","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"icon":"mdi:palette","name":"Effect","object_id":"küchentisch_effect","options":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"unique_id":"0x7cb03eaa0a0176bd_effect_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0xf0d1b800001388f0/effect/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Flurlicht/set/effect","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xf0d1b800001388f0"],"manufacturer":"OSRAM","model":"SMART+ Candle E14 Dimmable White","model_id":"AC08562","name":"Flurlicht","sw_version":"01056400","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"icon":"mdi:palette","name":"Effect","object_id":"flurlicht_effect","options":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"unique_id":"0xf0d1b800001388f0_effect_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0xa4c1389d42e94844/temperature_unit/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Temperatur Keller/set/temperature_unit","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1389d42e94844"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Temperatur Keller","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"name":"Temperature unit","object_id":"temperatur_keller_temperature_unit","options":["celsius","fahrenheit"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/Temperatur Keller","unique_id":"0xa4c1389d42e94844_temperature_unit_zigbee2mqtt","value_template":"{{ value_json.temperature_unit }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0xa4c13838ba59a1b2/temperature_unit/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Medienschrank Wohnzimmer/set/temperature_unit","device":{"identifiers":["zigbee2mqtt_0xa4c13838ba59a1b2"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Medienschrank Wohnzimmer","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"name":"Temperature unit","object_id":"medienschrank_wohnzimmer_temperature_unit","options":["celsius","fahrenheit"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/Medienschrank Wohnzimmer","unique_id":"0xa4c13838ba59a1b2_temperature_unit_zigbee2mqtt","value_template":"{{ value_json.temperature_unit }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0x00212effff0cb8b6/effect/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Lichtschlauch/set/effect","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x00212effff0cb8b6"],"manufacturer":"dresden elektronik\u0000","model":"Automatically generated definition","model_id":"FLS-PP3 White\u0000","name":"Lichtschlauch","sw_version":"0214.201000F6\u0000","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"icon":"mdi:palette","name":"Effect","object_id":"lichtschlauch_effect","options":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"unique_id":"0x00212effff0cb8b6_effect_zigbee2mqtt"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/select/0x00212effff0cb8b6/power_on_behavior/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Lichtschlauch/set/power_on_behavior","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x00212effff0cb8b6"],"manufacturer":"dresden elektronik\u0000","model":"Automatically generated definition","model_id":"FLS-PP3 White\u0000","name":"Lichtschlauch","sw_version":"0214.201000F6\u0000","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"entity_category":"config","icon":"mdi:power-settings","name":"Power-on behavior","object_id":"lichtschlauch_power_on_behavior","options":["off","on","toggle","previous"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/Lichtschlauch","unique_id":"0x00212effff0cb8b6_power_on_behavior_zigbee2mqtt","value_template":"{{ value_json.power_on_behavior }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/1221051039810110150109113116116_0x00212effff04fc2c/version/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"availability_mode":"all","device":{"hw_version":"ConBee2/RaspBee2 0x26580700","identifiers":["zigbee2mqtt_bridge_0x00212effff04fc2c"],"manufacturer":"Zigbee2MQTT","model":"Bridge","name":"Zigbee2MQTT Bridge","sw_version":"2.0.0"},"entity_category":"diagnostic","icon":"mdi:zigbee","name":"Version","object_id":"zigbee2mqtt_bridge_version","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/bridge/info","unique_id":"bridge_0x00212effff04fc2c_version_zigbee2mqtt","value_template":"{{ value_json.version }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/1221051039810110150109113116116_0x00212effff04fc2c/coordinator_version/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"availability_mode":"all","device":{"hw_version":"ConBee2/RaspBee2 0x26580700","identifiers":["zigbee2mqtt_bridge_0x00212effff04fc2c"],"manufacturer":"Zigbee2MQTT","model":"Bridge","name":"Zigbee2MQTT Bridge","sw_version":"2.0.0"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:chip","name":"Coordinator version","object_id":"zigbee2mqtt_bridge_coordinator_version","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/bridge/info","unique_id":"bridge_0x00212effff04fc2c_coordinator_version_zigbee2mqtt","value_template":"{{ value_json.coordinator.meta.revision }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/1221051039810110150109113116116_0x00212effff04fc2c/network_map/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"availability_mode":"all","device":{"hw_version":"ConBee2/RaspBee2 0x26580700","identifiers":["zigbee2mqtt_bridge_0x00212effff04fc2c"],"manufacturer":"Zigbee2MQTT","model":"Bridge","name":"Zigbee2MQTT Bridge","sw_version":"2.0.0"},"enabled_by_default":false,"entity_category":"diagnostic","json_attributes_template":"{{ value_json.data.value | tojson }}","json_attributes_topic":"zigbee2mqtt/bridge/response/networkmap","name":"Network map","object_id":"zigbee2mqtt_bridge_network_map","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/bridge/response/networkmap","unique_id":"bridge_0x00212effff04fc2c_network_map_zigbee2mqtt","value_template":"{{ now().strftime('%Y-%m-%d %H:%M:%S') }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xf0d1b800001ffcf2/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":2,"identifiers":["zigbee2mqtt_0xf0d1b800001ffcf2"],"manufacturer":"LEDVANCE","model":"SMART+ lamp E27 RGBW","model_id":"4058075208391","name":"Bogenlampe","sw_version":"03197310","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"bogenlampe_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Bogenlampe","unique_id":"0xf0d1b800001ffcf2_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c138570b1956d9/battery/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c138570b1956d9"],"manufacturer":"Tuya","model":"Temperature & humidity sensor","model_id":"RSH-HS06_1","name":"0xa4c138570b1956d9","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","enabled_by_default":true,"entity_category":"diagnostic","object_id":"0xa4c138570b1956d9_battery","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c138570b1956d9","unique_id":"0xa4c138570b1956d9_battery_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.battery }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c138570b1956d9/temperature/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c138570b1956d9"],"manufacturer":"Tuya","model":"Temperature & humidity sensor","model_id":"RSH-HS06_1","name":"0xa4c138570b1956d9","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"temperature","enabled_by_default":true,"object_id":"0xa4c138570b1956d9_temperature","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c138570b1956d9","unique_id":"0xa4c138570b1956d9_temperature_zigbee2mqtt","unit_of_measurement":"°C","value_template":"{{ value_json.temperature }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c138570b1956d9/humidity/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c138570b1956d9"],"manufacturer":"Tuya","model":"Temperature & humidity sensor","model_id":"RSH-HS06_1","name":"0xa4c138570b1956d9","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"humidity","enabled_by_default":true,"object_id":"0xa4c138570b1956d9_humidity","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c138570b1956d9","unique_id":"0xa4c138570b1956d9_humidity_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.humidity }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c138570b1956d9/voltage/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c138570b1956d9"],"manufacturer":"Tuya","model":"Temperature & humidity sensor","model_id":"RSH-HS06_1","name":"0xa4c138570b1956d9","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"voltage","enabled_by_default":false,"entity_category":"diagnostic","object_id":"0xa4c138570b1956d9_voltage","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c138570b1956d9","unique_id":"0xa4c138570b1956d9_voltage_zigbee2mqtt","unit_of_measurement":"mV","value_template":"{{ value_json.voltage }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c138570b1956d9/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c138570b1956d9"],"manufacturer":"Tuya","model":"Temperature & humidity sensor","model_id":"RSH-HS06_1","name":"0xa4c138570b1956d9","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"0xa4c138570b1956d9_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c138570b1956d9","unique_id":"0xa4c138570b1956d9_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1383ec7aa7d95/battery/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1383ec7aa7d95"],"manufacturer":"Tuya","model":"Temperature & humidity sensor","model_id":"RSH-HS06_1","name":"0xa4c1383ec7aa7d95","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","enabled_by_default":true,"entity_category":"diagnostic","object_id":"0xa4c1383ec7aa7d95_battery","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c1383ec7aa7d95","unique_id":"0xa4c1383ec7aa7d95_battery_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.battery }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1383ec7aa7d95/temperature/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1383ec7aa7d95"],"manufacturer":"Tuya","model":"Temperature & humidity sensor","model_id":"RSH-HS06_1","name":"0xa4c1383ec7aa7d95","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"temperature","enabled_by_default":true,"object_id":"0xa4c1383ec7aa7d95_temperature","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c1383ec7aa7d95","unique_id":"0xa4c1383ec7aa7d95_temperature_zigbee2mqtt","unit_of_measurement":"°C","value_template":"{{ value_json.temperature }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1383ec7aa7d95/humidity/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1383ec7aa7d95"],"manufacturer":"Tuya","model":"Temperature & humidity sensor","model_id":"RSH-HS06_1","name":"0xa4c1383ec7aa7d95","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"humidity","enabled_by_default":true,"object_id":"0xa4c1383ec7aa7d95_humidity","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c1383ec7aa7d95","unique_id":"0xa4c1383ec7aa7d95_humidity_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.humidity }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1383ec7aa7d95/voltage/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1383ec7aa7d95"],"manufacturer":"Tuya","model":"Temperature & humidity sensor","model_id":"RSH-HS06_1","name":"0xa4c1383ec7aa7d95","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"voltage","enabled_by_default":false,"entity_category":"diagnostic","object_id":"0xa4c1383ec7aa7d95_voltage","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c1383ec7aa7d95","unique_id":"0xa4c1383ec7aa7d95_voltage_zigbee2mqtt","unit_of_measurement":"mV","value_template":"{{ value_json.voltage }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1383ec7aa7d95/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1383ec7aa7d95"],"manufacturer":"Tuya","model":"Temperature & humidity sensor","model_id":"RSH-HS06_1","name":"0xa4c1383ec7aa7d95","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"0xa4c1383ec7aa7d95_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c1383ec7aa7d95","unique_id":"0xa4c1383ec7aa7d95_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1383db5531833/battery/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1383db5531833"],"manufacturer":"Tuya","model":"Temperature & humidity sensor with display","model_id":"TS0201","name":"0xa4c1383db5531833","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","enabled_by_default":true,"entity_category":"diagnostic","object_id":"0xa4c1383db5531833_battery","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c1383db5531833","unique_id":"0xa4c1383db5531833_battery_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.battery }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1383db5531833/temperature/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1383db5531833"],"manufacturer":"Tuya","model":"Temperature & humidity sensor with display","model_id":"TS0201","name":"0xa4c1383db5531833","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"temperature","enabled_by_default":true,"object_id":"0xa4c1383db5531833_temperature","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c1383db5531833","unique_id":"0xa4c1383db5531833_temperature_zigbee2mqtt","unit_of_measurement":"°C","value_template":"{{ value_json.temperature }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1383db5531833/humidity/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1383db5531833"],"manufacturer":"Tuya","model":"Temperature & humidity sensor with display","model_id":"TS0201","name":"0xa4c1383db5531833","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"humidity","enabled_by_default":true,"object_id":"0xa4c1383db5531833_humidity","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c1383db5531833","unique_id":"0xa4c1383db5531833_humidity_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.humidity }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1383db5531833/voltage/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1383db5531833"],"manufacturer":"Tuya","model":"Temperature & humidity sensor with display","model_id":"TS0201","name":"0xa4c1383db5531833","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"voltage","enabled_by_default":false,"entity_category":"diagnostic","object_id":"0xa4c1383db5531833_voltage","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c1383db5531833","unique_id":"0xa4c1383db5531833_voltage_zigbee2mqtt","unit_of_measurement":"mV","value_template":"{{ value_json.voltage }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1383db5531833/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1383db5531833"],"manufacturer":"Tuya","model":"Temperature & humidity sensor with display","model_id":"TS0201","name":"0xa4c1383db5531833","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"0xa4c1383db5531833_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0xa4c1383db5531833","unique_id":"0xa4c1383db5531833_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0x000d6f00109eb214/battery/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x000d6f00109eb214"],"manufacturer":"OSRAM","model":"Smart+ switch mini","model_id":"AC0251100NJ/AC0251600NJ/AC0251700NJ","name":"Fernbedienung","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","enabled_by_default":true,"entity_category":"diagnostic","object_id":"fernbedienung_battery","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Fernbedienung","unique_id":"0x000d6f00109eb214_battery_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.battery }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0x000d6f00109eb214/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x000d6f00109eb214"],"manufacturer":"OSRAM","model":"Smart+ switch mini","model_id":"AC0251100NJ/AC0251600NJ/AC0251700NJ","name":"Fernbedienung","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"fernbedienung_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Fernbedienung","unique_id":"0x000d6f00109eb214_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0x00212effff0cb8b6/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x00212effff0cb8b6"],"manufacturer":"dresden elektronik\u0000","model":"Automatically generated definition","model_id":"FLS-PP3 White\u0000","name":"Lichtschlauch","sw_version":"0214.201000F6\u0000","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"lichtschlauch_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Lichtschlauch","unique_id":"0x00212effff0cb8b6_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0x0ceff6fffebf4739/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x0ceff6fffebf4739"],"manufacturer":"Tuya","model":"Repeater","model_id":"TS0207_repeater","name":"0x0ceff6fffebf4739","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"0x0ceff6fffebf4739_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0x0ceff6fffebf4739","unique_id":"0x0ceff6fffebf4739_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c138541ec8ddd2/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":0,"identifiers":["zigbee2mqtt_0xa4c138541ec8ddd2"],"manufacturer":"AwoX","model":"LED white","model_id":"33951/33948","name":"Flur","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"flur_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Flur","unique_id":"0xa4c138541ec8ddd2_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1384187f0960d/battery/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"identifiers":["zigbee2mqtt_0xa4c1384187f0960d"],"manufacturer":"Aubess","model":"Water leak sensor","model_id":"IH-K665","name":"Wasser Sensor Spüle","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","enabled_by_default":true,"entity_category":"diagnostic","object_id":"wasser_sensor_spüle_battery","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Wasser Sensor Spüle","unique_id":"0xa4c1384187f0960d_battery_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.battery }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1384187f0960d/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"identifiers":["zigbee2mqtt_0xa4c1384187f0960d"],"manufacturer":"Aubess","model":"Water leak sensor","model_id":"IH-K665","name":"Wasser Sensor Spüle","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"wasser_sensor_spüle_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Wasser Sensor Spüle","unique_id":"0xa4c1384187f0960d_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0x001788010e8a8be7/battery/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch","model_id":"929002398602","name":"Fernbedienung Bad","sw_version":"2.45.2_hF4400CA","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","enabled_by_default":true,"entity_category":"diagnostic","object_id":"fernbedienung_bad_battery","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Fernbedienung Bad","unique_id":"0x001788010e8a8be7_battery_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.battery }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0x001788010e8a8be7/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch","model_id":"929002398602","name":"Fernbedienung Bad","sw_version":"2.45.2_hF4400CA","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"fernbedienung_bad_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Fernbedienung Bad","unique_id":"0x001788010e8a8be7_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c13864e6c8c400/battery/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c13864e6c8c400"],"manufacturer":"Tuya","model":"Motion sensor","model_id":"809WZT","name":"Bewegungsmelder 1","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","enabled_by_default":true,"entity_category":"diagnostic","object_id":"bewegungsmelder_1_battery","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Bewegungsmelder 1","unique_id":"0xa4c13864e6c8c400_battery_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.battery }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c13864e6c8c400/voltage/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c13864e6c8c400"],"manufacturer":"Tuya","model":"Motion sensor","model_id":"809WZT","name":"Bewegungsmelder 1","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"voltage","enabled_by_default":false,"entity_category":"diagnostic","object_id":"bewegungsmelder_1_voltage","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Bewegungsmelder 1","unique_id":"0xa4c13864e6c8c400_voltage_zigbee2mqtt","unit_of_measurement":"mV","value_template":"{{ value_json.voltage }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c13864e6c8c400/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c13864e6c8c400"],"manufacturer":"Tuya","model":"Motion sensor","model_id":"809WZT","name":"Bewegungsmelder 1","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"bewegungsmelder_1_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Bewegungsmelder 1","unique_id":"0xa4c13864e6c8c400_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c138ef60e2fdbe/battery/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c138ef60e2fdbe"],"manufacturer":"Tuya","model":"Door sensor","model_id":"TS0203","name":"Sensor Terassentür","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","enabled_by_default":true,"entity_category":"diagnostic","object_id":"sensor_terassentür_battery","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Sensor Terassentür","unique_id":"0xa4c138ef60e2fdbe_battery_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.battery }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c138ef60e2fdbe/voltage/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c138ef60e2fdbe"],"manufacturer":"Tuya","model":"Door sensor","model_id":"TS0203","name":"Sensor Terassentür","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"voltage","enabled_by_default":false,"entity_category":"diagnostic","object_id":"sensor_terassentür_voltage","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Sensor Terassentür","unique_id":"0xa4c138ef60e2fdbe_voltage_zigbee2mqtt","unit_of_measurement":"mV","value_template":"{{ value_json.voltage }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c138ef60e2fdbe/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c138ef60e2fdbe"],"manufacturer":"Tuya","model":"Door sensor","model_id":"TS0203","name":"Sensor Terassentür","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"sensor_terassentür_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Sensor Terassentür","unique_id":"0xa4c138ef60e2fdbe_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0x001788010d1c884e/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":0,"identifiers":["zigbee2mqtt_0x001788010d1c884e"],"manufacturer":"Philips","model":"Hue Devere M white ambiance white & dimmer","model_id":"915005997601","name":"Badlampe","sw_version":"1.93.7","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"badlampe_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Badlampe","unique_id":"0x001788010d1c884e_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0x00158d00053a1aab/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":21,"identifiers":["zigbee2mqtt_0x00158d00053a1aab"],"manufacturer":"Paulmann","model":"SmartHome led spot","model_id":"50064","name":"0x00158d00053a1aab","sw_version":"00.00.01","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"0x00158d00053a1aab_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0x00158d00053a1aab","unique_id":"0x00158d00053a1aab_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0x00158d00053c6311/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":21,"identifiers":["zigbee2mqtt_0x00158d00053c6311"],"manufacturer":"Paulmann","model":"SmartHome led spot","model_id":"50064","name":"0x00158d00053c6311","sw_version":"00.00.01","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"0x00158d00053c6311_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/0x00158d00053c6311","unique_id":"0x00158d00053c6311_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0x7cb03eaa0a0176bd/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x7cb03eaa0a0176bd"],"manufacturer":"OSRAM","model":"LIGHTIFY LED Classic A60 clear","model_id":"AC03641","name":"Küchentisch","sw_version":"V1.05.10","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"küchentisch_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Küchentisch","unique_id":"0x7cb03eaa0a0176bd_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0x000d6f001417c142/battery/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x000d6f001417c142"],"manufacturer":"OSRAM","model":"Smart+ switch mini","model_id":"AC0251100NJ/AC0251600NJ/AC0251700NJ","name":"Fernbedienung 2","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","enabled_by_default":true,"entity_category":"diagnostic","object_id":"fernbedienung_2_battery","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Fernbedienung 2","unique_id":"0x000d6f001417c142_battery_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.battery }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0x000d6f001417c142/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x000d6f001417c142"],"manufacturer":"OSRAM","model":"Smart+ switch mini","model_id":"AC0251100NJ/AC0251600NJ/AC0251700NJ","name":"Fernbedienung 2","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"fernbedienung_2_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Fernbedienung 2","unique_id":"0x000d6f001417c142_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xf0d1b800001388f0/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xf0d1b800001388f0"],"manufacturer":"OSRAM","model":"SMART+ Candle E14 Dimmable White","model_id":"AC08562","name":"Flurlicht","sw_version":"01056400","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"flurlicht_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Flurlicht","unique_id":"0xf0d1b800001388f0_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c138e68023f4c6/battery/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":0,"identifiers":["zigbee2mqtt_0xa4c138e68023f4c6"],"manufacturer":"eWeLink","model":"Zigbee water sensor","model_id":"SNZB-05","name":"Wassersensor Keller","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","enabled_by_default":true,"entity_category":"diagnostic","object_id":"wassersensor_keller_battery","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Wassersensor Keller","unique_id":"0xa4c138e68023f4c6_battery_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.battery }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c138e68023f4c6/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":0,"identifiers":["zigbee2mqtt_0xa4c138e68023f4c6"],"manufacturer":"eWeLink","model":"Zigbee water sensor","model_id":"SNZB-05","name":"Wassersensor Keller","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"wassersensor_keller_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Wassersensor Keller","unique_id":"0xa4c138e68023f4c6_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1389d42e94844/temperature/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1389d42e94844"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Temperatur Keller","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"temperature","enabled_by_default":true,"object_id":"temperatur_keller_temperature","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Temperatur Keller","unique_id":"0xa4c1389d42e94844_temperature_zigbee2mqtt","unit_of_measurement":"°C","value_template":"{{ value_json.temperature }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1389d42e94844/humidity/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1389d42e94844"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Temperatur Keller","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"humidity","enabled_by_default":true,"object_id":"temperatur_keller_humidity","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Temperatur Keller","unique_id":"0xa4c1389d42e94844_humidity_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.humidity }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1389d42e94844/battery/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1389d42e94844"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Temperatur Keller","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","enabled_by_default":true,"entity_category":"diagnostic","object_id":"temperatur_keller_battery","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Temperatur Keller","unique_id":"0xa4c1389d42e94844_battery_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.battery }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c1389d42e94844/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1389d42e94844"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Temperatur Keller","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"temperatur_keller_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Temperatur Keller","unique_id":"0xa4c1389d42e94844_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c13838ba59a1b2/temperature/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"identifiers":["zigbee2mqtt_0xa4c13838ba59a1b2"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Medienschrank Wohnzimmer","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"temperature","enabled_by_default":true,"object_id":"medienschrank_wohnzimmer_temperature","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Medienschrank Wohnzimmer","unique_id":"0xa4c13838ba59a1b2_temperature_zigbee2mqtt","unit_of_measurement":"°C","value_template":"{{ value_json.temperature }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c13838ba59a1b2/humidity/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"identifiers":["zigbee2mqtt_0xa4c13838ba59a1b2"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Medienschrank Wohnzimmer","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"humidity","enabled_by_default":true,"object_id":"medienschrank_wohnzimmer_humidity","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Medienschrank Wohnzimmer","unique_id":"0xa4c13838ba59a1b2_humidity_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.humidity }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c13838ba59a1b2/battery/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"identifiers":["zigbee2mqtt_0xa4c13838ba59a1b2"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Medienschrank Wohnzimmer","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"battery","enabled_by_default":true,"entity_category":"diagnostic","object_id":"medienschrank_wohnzimmer_battery","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Medienschrank Wohnzimmer","unique_id":"0xa4c13838ba59a1b2_battery_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.battery }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/sensor/0xa4c13838ba59a1b2/linkquality/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"device":{"identifiers":["zigbee2mqtt_0xa4c13838ba59a1b2"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Medienschrank Wohnzimmer","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"entity_category":"diagnostic","icon":"mdi:signal","name":"Linkquality","object_id":"medienschrank_wohnzimmer_linkquality","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_class":"measurement","state_topic":"zigbee2mqtt/Medienschrank Wohnzimmer","unique_id":"0xa4c13838ba59a1b2_linkquality_zigbee2mqtt","unit_of_measurement":"lqi","value_template":"{{ value_json.linkquality }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/switch/1221051039810110150109113116116_0x00212effff04fc2c/permit_join/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"availability_mode":"all","command_topic":"zigbee2mqtt/bridge/request/permit_join","device":{"hw_version":"ConBee2/RaspBee2 0x26580700","identifiers":["zigbee2mqtt_bridge_0x00212effff04fc2c"],"manufacturer":"Zigbee2MQTT","model":"Bridge","name":"Zigbee2MQTT Bridge","sw_version":"2.0.0"},"icon":"mdi:human-greeting-proximity","name":"Permit join","object_id":"zigbee2mqtt_bridge_permit_join","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_off":"{\"time\": 0}","payload_on":"{\"time\": 254}","state_off":"false","state_on":"true","state_topic":"zigbee2mqtt/bridge/info","unique_id":"bridge_0x00212effff04fc2c_permit_join_zigbee2mqtt","value_template":"{{ value_json.permit_join | lower }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/update/0xf0d1b800001ffcf2/update/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/bridge/request/device/ota_update/update","device":{"hw_version":2,"identifiers":["zigbee2mqtt_0xf0d1b800001ffcf2"],"manufacturer":"LEDVANCE","model":"SMART+ lamp E27 RGBW","model_id":"4058075208391","name":"Bogenlampe","sw_version":"03197310","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"firmware","entity_category":"config","entity_picture":"https://github.com/Koenkk/zigbee2mqtt/raw/master/images/logo.png","json_attributes_template":"{\"in_progress\": {{ iif(value_json['update']['state'] == 'updating', 'true', 'false') }} }","json_attributes_topic":"zigbee2mqtt/Bogenlampe","latest_version_template":"{{ value_json['update']['latest_version'] }}","latest_version_topic":"zigbee2mqtt/Bogenlampe","name":null,"object_id":"bogenlampe","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_install":"{\"id\": \"0xf0d1b800001ffcf2\"}","state_topic":"zigbee2mqtt/Bogenlampe","unique_id":"0xf0d1b800001ffcf2_update_zigbee2mqtt","value_template":"{{ value_json['update']['installed_version'] }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/update/0x000d6f00109eb214/update/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/bridge/request/device/ota_update/update","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x000d6f00109eb214"],"manufacturer":"OSRAM","model":"Smart+ switch mini","model_id":"AC0251100NJ/AC0251600NJ/AC0251700NJ","name":"Fernbedienung","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"firmware","entity_category":"config","entity_picture":"https://github.com/Koenkk/zigbee2mqtt/raw/master/images/logo.png","json_attributes_template":"{\"in_progress\": {{ iif(value_json['update']['state'] == 'updating', 'true', 'false') }} }","json_attributes_topic":"zigbee2mqtt/Fernbedienung","latest_version_template":"{{ value_json['update']['latest_version'] }}","latest_version_topic":"zigbee2mqtt/Fernbedienung","name":null,"object_id":"fernbedienung","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_install":"{\"id\": \"0x000d6f00109eb214\"}","state_topic":"zigbee2mqtt/Fernbedienung","unique_id":"0x000d6f00109eb214_update_zigbee2mqtt","value_template":"{{ value_json['update']['installed_version'] }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/update/0x001788010d1c884e/update/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/bridge/request/device/ota_update/update","device":{"hw_version":0,"identifiers":["zigbee2mqtt_0x001788010d1c884e"],"manufacturer":"Philips","model":"Hue Devere M white ambiance white & dimmer","model_id":"915005997601","name":"Badlampe","sw_version":"1.93.7","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"firmware","entity_category":"config","entity_picture":"https://github.com/Koenkk/zigbee2mqtt/raw/master/images/logo.png","json_attributes_template":"{\"in_progress\": {{ iif(value_json['update']['state'] == 'updating', 'true', 'false') }} }","json_attributes_topic":"zigbee2mqtt/Badlampe","latest_version_template":"{{ value_json['update']['latest_version'] }}","latest_version_topic":"zigbee2mqtt/Badlampe","name":null,"object_id":"badlampe","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_install":"{\"id\": \"0x001788010d1c884e\"}","state_topic":"zigbee2mqtt/Badlampe","unique_id":"0x001788010d1c884e_update_zigbee2mqtt","value_template":"{{ value_json['update']['installed_version'] }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/update/0x001788010e8a8be7/update/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/bridge/request/device/ota_update/update","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch","model_id":"929002398602","name":"Fernbedienung Bad","sw_version":"2.45.2_hF4400CA","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"firmware","entity_category":"config","entity_picture":"https://github.com/Koenkk/zigbee2mqtt/raw/master/images/logo.png","json_attributes_template":"{\"in_progress\": {{ iif(value_json['update']['state'] == 'updating', 'true', 'false') }} }","json_attributes_topic":"zigbee2mqtt/Fernbedienung Bad","latest_version_template":"{{ value_json['update']['latest_version'] }}","latest_version_topic":"zigbee2mqtt/Fernbedienung Bad","name":null,"object_id":"fernbedienung_bad","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_install":"{\"id\": \"0x001788010e8a8be7\"}","state_topic":"zigbee2mqtt/Fernbedienung Bad","unique_id":"0x001788010e8a8be7_update_zigbee2mqtt","value_template":"{{ value_json['update']['installed_version'] }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/update/0xa4c1383db5531833/update/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/bridge/request/device/ota_update/update","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1383db5531833"],"manufacturer":"Tuya","model":"Temperature & humidity sensor with display","model_id":"TS0201","name":"0xa4c1383db5531833","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"firmware","entity_category":"config","entity_picture":"https://github.com/Koenkk/zigbee2mqtt/raw/master/images/logo.png","json_attributes_template":"{\"in_progress\": {{ iif(value_json['update']['state'] == 'updating', 'true', 'false') }} }","json_attributes_topic":"zigbee2mqtt/0xa4c1383db5531833","latest_version_template":"{{ value_json['update']['latest_version'] }}","latest_version_topic":"zigbee2mqtt/0xa4c1383db5531833","name":null,"object_id":"0xa4c1383db5531833","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_install":"{\"id\": \"0xa4c1383db5531833\"}","state_topic":"zigbee2mqtt/0xa4c1383db5531833","unique_id":"0xa4c1383db5531833_update_zigbee2mqtt","value_template":"{{ value_json['update']['installed_version'] }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/update/0xf0d1b800001388f0/update/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/bridge/request/device/ota_update/update","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xf0d1b800001388f0"],"manufacturer":"OSRAM","model":"SMART+ Candle E14 Dimmable White","model_id":"AC08562","name":"Flurlicht","sw_version":"01056400","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"firmware","entity_category":"config","entity_picture":"https://github.com/Koenkk/zigbee2mqtt/raw/master/images/logo.png","json_attributes_template":"{\"in_progress\": {{ iif(value_json['update']['state'] == 'updating', 'true', 'false') }} }","json_attributes_topic":"zigbee2mqtt/Flurlicht","latest_version_template":"{{ value_json['update']['latest_version'] }}","latest_version_topic":"zigbee2mqtt/Flurlicht","name":null,"object_id":"flurlicht","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_install":"{\"id\": \"0xf0d1b800001388f0\"}","state_topic":"zigbee2mqtt/Flurlicht","unique_id":"0xf0d1b800001388f0_update_zigbee2mqtt","value_template":"{{ value_json['update']['installed_version'] }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/update/0x7cb03eaa0a0176bd/update/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/bridge/request/device/ota_update/update","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x7cb03eaa0a0176bd"],"manufacturer":"OSRAM","model":"LIGHTIFY LED Classic A60 clear","model_id":"AC03641","name":"Küchentisch","sw_version":"V1.05.10","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"firmware","entity_category":"config","entity_picture":"https://github.com/Koenkk/zigbee2mqtt/raw/master/images/logo.png","json_attributes_template":"{\"in_progress\": {{ iif(value_json['update']['state'] == 'updating', 'true', 'false') }} }","json_attributes_topic":"zigbee2mqtt/Küchentisch","latest_version_template":"{{ value_json['update']['latest_version'] }}","latest_version_topic":"zigbee2mqtt/Küchentisch","name":null,"object_id":"küchentisch","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_install":"{\"id\": \"0x7cb03eaa0a0176bd\"}","state_topic":"zigbee2mqtt/Küchentisch","unique_id":"0x7cb03eaa0a0176bd_update_zigbee2mqtt","value_template":"{{ value_json['update']['installed_version'] }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/update/0x000d6f001417c142/update/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/bridge/request/device/ota_update/update","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x000d6f001417c142"],"manufacturer":"OSRAM","model":"Smart+ switch mini","model_id":"AC0251100NJ/AC0251600NJ/AC0251700NJ","name":"Fernbedienung 2","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"device_class":"firmware","entity_category":"config","entity_picture":"https://github.com/Koenkk/zigbee2mqtt/raw/master/images/logo.png","json_attributes_template":"{\"in_progress\": {{ iif(value_json['update']['state'] == 'updating', 'true', 'false') }} }","json_attributes_topic":"zigbee2mqtt/Fernbedienung 2","latest_version_template":"{{ value_json['update']['latest_version'] }}","latest_version_topic":"zigbee2mqtt/Fernbedienung 2","name":null,"object_id":"fernbedienung_2","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_install":"{\"id\": \"0x000d6f001417c142\"}","state_topic":"zigbee2mqtt/Fernbedienung 2","unique_id":"0x000d6f001417c142_update_zigbee2mqtt","value_template":"{{ value_json['update']['installed_version'] }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x000d6f00109eb214/action_on/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x000d6f00109eb214"],"manufacturer":"OSRAM","model":"Smart+ switch mini (AC0251100NJ/AC0251600NJ/AC0251700NJ)","name":"Fernbedienung","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.39.1","url":"https://www.zigbee2mqtt.io"},"payload":"on","subtype":"on","topic":"zigbee2mqtt/Fernbedienung/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x000d6f00109eb214/action_off/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x000d6f00109eb214"],"manufacturer":"OSRAM","model":"Smart+ switch mini (AC0251100NJ/AC0251600NJ/AC0251700NJ)","name":"Fernbedienung","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.39.1","url":"https://www.zigbee2mqtt.io"},"payload":"off","subtype":"off","topic":"zigbee2mqtt/Fernbedienung/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x000d6f00109eb214/action_brightness_move_to_level/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x000d6f00109eb214"],"manufacturer":"OSRAM","model":"Smart+ switch mini (AC0251100NJ/AC0251600NJ/AC0251700NJ)","name":"Fernbedienung","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.39.1","url":"https://www.zigbee2mqtt.io"},"payload":"brightness_move_to_level","subtype":"brightness_move_to_level","topic":"zigbee2mqtt/Fernbedienung/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x000d6f00109eb214/action_color_temperature_move/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x000d6f00109eb214"],"manufacturer":"OSRAM","model":"Smart+ switch mini (AC0251100NJ/AC0251600NJ/AC0251700NJ)","name":"Fernbedienung","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.39.1","url":"https://www.zigbee2mqtt.io"},"payload":"color_temperature_move","subtype":"color_temperature_move","topic":"zigbee2mqtt/Fernbedienung/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x000d6f00109eb214/action_brightness_move_up/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x000d6f00109eb214"],"manufacturer":"OSRAM","model":"Smart+ switch mini (AC0251100NJ/AC0251600NJ/AC0251700NJ)","name":"Fernbedienung","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.39.1","url":"https://www.zigbee2mqtt.io"},"payload":"brightness_move_up","subtype":"brightness_move_up","topic":"zigbee2mqtt/Fernbedienung/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x000d6f00109eb214/action_brightness_stop/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x000d6f00109eb214"],"manufacturer":"OSRAM","model":"Smart+ switch mini (AC0251100NJ/AC0251600NJ/AC0251700NJ)","name":"Fernbedienung","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.39.1","url":"https://www.zigbee2mqtt.io"},"payload":"brightness_stop","subtype":"brightness_stop","topic":"zigbee2mqtt/Fernbedienung/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x000d6f00109eb214/action_brightness_move_down/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x000d6f00109eb214"],"manufacturer":"OSRAM","model":"Smart+ switch mini (AC0251100NJ/AC0251600NJ/AC0251700NJ)","name":"Fernbedienung","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.42.0","url":"https://www.zigbee2mqtt.io"},"payload":"brightness_move_down","subtype":"brightness_move_down","topic":"zigbee2mqtt/Fernbedienung/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_off_press/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"off_press","subtype":"off_press","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_off_hold/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"off_hold","subtype":"off_hold","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_off_hold_release/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"off_hold_release","subtype":"off_hold_release","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_off_press_release/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"off_press_release","subtype":"off_press_release","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_on_press/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"on_press","subtype":"on_press","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_on_press_release/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"on_press_release","subtype":"on_press_release","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_down_press/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"down_press","subtype":"down_press","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_down_press_release/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"down_press_release","subtype":"down_press_release","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_up_press/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"up_press","subtype":"up_press","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_up_press_release/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"up_press_release","subtype":"up_press_release","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_up_hold/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"up_hold","subtype":"up_hold","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_up_hold_release/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"up_hold_release","subtype":"up_hold_release","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_down_hold/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"down_hold","subtype":"down_hold","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x001788010e8a8be7/action_down_hold_release/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x001788010e8a8be7"],"manufacturer":"Philips","model":"Hue dimmer switch (929002398602)","name":"Fernbedienung Bad","sw_version":"2.44.0_hBB3C188","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.40.2","url":"https://www.zigbee2mqtt.io"},"payload":"down_hold_release","subtype":"down_hold_release","topic":"zigbee2mqtt/Fernbedienung Bad/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x000d6f001417c142/action_off/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x000d6f001417c142"],"manufacturer":"OSRAM","model":"Smart+ switch mini (AC0251100NJ/AC0251600NJ/AC0251700NJ)","name":"Fernbedienung 2","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.42.0","url":"https://www.zigbee2mqtt.io"},"payload":"off","subtype":"off","topic":"zigbee2mqtt/Fernbedienung 2/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x000d6f001417c142/action_on/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x000d6f001417c142"],"manufacturer":"OSRAM","model":"Smart+ switch mini (AC0251100NJ/AC0251600NJ/AC0251700NJ)","name":"Fernbedienung 2","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.42.0","url":"https://www.zigbee2mqtt.io"},"payload":"on","subtype":"on","topic":"zigbee2mqtt/Fernbedienung 2/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x000d6f001417c142/action_brightness_move_to_level/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x000d6f001417c142"],"manufacturer":"OSRAM","model":"Smart+ switch mini (AC0251100NJ/AC0251600NJ/AC0251700NJ)","name":"Fernbedienung 2","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.42.0","url":"https://www.zigbee2mqtt.io"},"payload":"brightness_move_to_level","subtype":"brightness_move_to_level","topic":"zigbee2mqtt/Fernbedienung 2/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/device_automation/0x000d6f001417c142/action_color_temperature_move/config' with data '{"automation_type":"trigger","device":{"identifiers":["zigbee2mqtt_0x000d6f001417c142"],"manufacturer":"OSRAM","model":"Smart+ switch mini (AC0251100NJ/AC0251600NJ/AC0251700NJ)","name":"Fernbedienung 2","sw_version":"e.1.11.0M","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"origin":{"name":"Zigbee2MQTT","sw":"1.42.0","url":"https://www.zigbee2mqtt.io"},"payload":"color_temperature_move","subtype":"color_temperature_move","topic":"zigbee2mqtt/Fernbedienung 2/action","type":"action"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/number/0xa4c1389d42e94844/temperature_calibration/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Temperatur Keller/set/temperature_calibration","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1389d42e94844"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Temperatur Keller","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"entity_category":"config","icon":"mdi:wrench-clock","max":2,"min":-2,"name":"Temperature calibration","object_id":"temperatur_keller_temperature_calibration","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/Temperatur Keller","step":0.1,"unique_id":"0xa4c1389d42e94844_temperature_calibration_zigbee2mqtt","unit_of_measurement":"°C","value_template":"{{ value_json.temperature_calibration }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/number/0xa4c1389d42e94844/humidity_calibration/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Temperatur Keller/set/humidity_calibration","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0xa4c1389d42e94844"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Temperatur Keller","sw_version":"0122052017","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"entity_category":"config","icon":"mdi:wrench-clock","max":30,"min":-30,"name":"Humidity calibration","object_id":"temperatur_keller_humidity_calibration","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/Temperatur Keller","step":1,"unique_id":"0xa4c1389d42e94844_humidity_calibration_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.humidity_calibration }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/number/0xa4c13838ba59a1b2/temperature_calibration/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Medienschrank Wohnzimmer/set/temperature_calibration","device":{"identifiers":["zigbee2mqtt_0xa4c13838ba59a1b2"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Medienschrank Wohnzimmer","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"entity_category":"config","icon":"mdi:wrench-clock","max":2,"min":-2,"name":"Temperature calibration","object_id":"medienschrank_wohnzimmer_temperature_calibration","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/Medienschrank Wohnzimmer","step":0.1,"unique_id":"0xa4c13838ba59a1b2_temperature_calibration_zigbee2mqtt","unit_of_measurement":"°C","value_template":"{{ value_json.temperature_calibration }}"}'
[2025-01-19 22:58:12] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/number/0xa4c13838ba59a1b2/humidity_calibration/config' with data '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Medienschrank Wohnzimmer/set/humidity_calibration","device":{"identifiers":["zigbee2mqtt_0xa4c13838ba59a1b2"],"manufacturer":"Tuya","model":"Temperature and humidity sensor","model_id":"ZG-227Z","name":"Medienschrank Wohnzimmer","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"entity_category":"config","icon":"mdi:wrench-clock","max":30,"min":-30,"name":"Humidity calibration","object_id":"medienschrank_wohnzimmer_humidity_calibration","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"state_topic":"zigbee2mqtt/Medienschrank Wohnzimmer","step":1,"unique_id":"0xa4c13838ba59a1b2_humidity_calibration_zigbee2mqtt","unit_of_measurement":"%","value_template":"{{ value_json.humidity_calibration }}"}'
[2025-01-19 22:58:17] debug: 	z2m: Discovering entities to Home Assistant
[2025-01-19 22:58:17] info: 	z2m:mqtt: MQTT publish: topic 'homeassistant/binary_sensor/1221051039810110150109113116116_0x00212effff04fc2c/connection_state/config', payload '{"device":{"hw_version":"ConBee2/RaspBee2 0x26580700","identifiers":["zigbee2mqtt_bridge_0x00212effff04fc2c"],"manufacturer":"Zigbee2MQTT","model":"Bridge","name":"Zigbee2MQTT Bridge","sw_version":"2.0.0"},"device_class":"connectivity","entity_category":"diagnostic","name":"Connection state","object_id":"zigbee2mqtt_bridge_connection_state","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"payload_off":"offline","payload_on":"online","state_topic":"zigbee2mqtt/bridge/state","unique_id":"bridge_0x00212effff04fc2c_connection_state_zigbee2mqtt","value_template":"{{ value_json.state }}"}'
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'binary_sensor/1221051039810110150109113116116_0x00212effff04fc2c/restart_required/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'button/1221051039810110150109113116116_0x00212effff04fc2c/restart/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/1221051039810110150109113116116_0x00212effff04fc2c/log_level/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/1221051039810110150109113116116_0x00212effff04fc2c/version/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/1221051039810110150109113116116_0x00212effff04fc2c/coordinator_version/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/1221051039810110150109113116116_0x00212effff04fc2c/network_map/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'switch/1221051039810110150109113116116_0x00212effff04fc2c/permit_join/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0x000d6f00109eb214/battery/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0x000d6f00109eb214/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'update/0x000d6f00109eb214/update/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'light/0xf0d1b800001ffcf2/light/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0xf0d1b800001ffcf2/effect/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xf0d1b800001ffcf2/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'update/0xf0d1b800001ffcf2/update/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c138570b1956d9/battery/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c138570b1956d9/temperature/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c138570b1956d9/humidity/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c138570b1956d9/voltage/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c138570b1956d9/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1383ec7aa7d95/battery/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1383ec7aa7d95/temperature/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1383ec7aa7d95/humidity/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1383ec7aa7d95/voltage/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1383ec7aa7d95/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1383db5531833/battery/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1383db5531833/temperature/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1383db5531833/humidity/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1383db5531833/voltage/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1383db5531833/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'update/0xa4c1383db5531833/update/config', already discovered
[2025-01-19 22:58:17] info: 	z2m:mqtt: MQTT publish: topic 'homeassistant/light/0x00212effff0cb8b6/light/config', payload '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"brightness":true,"brightness_scale":254,"command_topic":"zigbee2mqtt/Lichtschlauch/set","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x00212effff0cb8b6"],"manufacturer":"dresden elektronik\u0000","model":"Automatically generated definition","model_id":"FLS-PP3 White\u0000","name":"Lichtschlauch","sw_version":"0214.201000F6\u0000","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"effect":true,"effect_list":["blink","breathe","okay","channel_change","finish_effect","stop_effect","colorloop","stop_colorloop"],"max_mireds":500,"min_mireds":153,"name":null,"object_id":"lichtschlauch","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"schema":"json","state_topic":"zigbee2mqtt/Lichtschlauch","supported_color_modes":["xy","color_temp"],"unique_id":"0x00212effff0cb8b6_light_zigbee2mqtt"}'
[2025-01-19 22:58:17] info: 	z2m:mqtt: MQTT publish: topic 'homeassistant/select/0x00212effff0cb8b6/effect/config', payload '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Lichtschlauch/set/effect","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x00212effff0cb8b6"],"manufacturer":"dresden elektronik\u0000","model":"Automatically generated definition","model_id":"FLS-PP3 White\u0000","name":"Lichtschlauch","sw_version":"0214.201000F6\u0000","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"icon":"mdi:palette","name":"Effect","object_id":"lichtschlauch_effect","options":["blink","breathe","okay","channel_change","finish_effect","stop_effect","colorloop","stop_colorloop"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"unique_id":"0x00212effff0cb8b6_effect_zigbee2mqtt"}'
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0x00212effff0cb8b6/power_on_behavior/config', already discovered
[2025-01-19 22:58:17] info: 	z2m:mqtt: MQTT publish: topic 'homeassistant/light/0x00212effff0cb8b6/light/config', payload '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"brightness":true,"brightness_scale":254,"command_topic":"zigbee2mqtt/Lichtschlauch/set","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x00212effff0cb8b6"],"manufacturer":"dresden elektronik\u0000","model":"Automatically generated definition","model_id":"FLS-PP3 White\u0000","name":"Lichtschlauch","sw_version":"0214.201000F6\u0000","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"effect":true,"effect_list":["blink","breathe","okay","channel_change","finish_effect","stop_effect","colorloop","stop_colorloop"],"name":null,"object_id":"lichtschlauch","origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"schema":"json","state_topic":"zigbee2mqtt/Lichtschlauch","unique_id":"0x00212effff0cb8b6_light_zigbee2mqtt"}'
[2025-01-19 22:58:17] info: 	z2m:mqtt: MQTT publish: topic 'homeassistant/select/0x00212effff0cb8b6/effect/config', payload '{"availability":[{"topic":"zigbee2mqtt/bridge/state","value_template":"{{ value_json.state }}"}],"command_topic":"zigbee2mqtt/Lichtschlauch/set/effect","device":{"hw_version":1,"identifiers":["zigbee2mqtt_0x00212effff0cb8b6"],"manufacturer":"dresden elektronik\u0000","model":"Automatically generated definition","model_id":"FLS-PP3 White\u0000","name":"Lichtschlauch","sw_version":"0214.201000F6\u0000","via_device":"zigbee2mqtt_bridge_0x00212effff04fc2c"},"enabled_by_default":false,"icon":"mdi:palette","name":"Effect","object_id":"lichtschlauch_effect","options":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"origin":{"name":"Zigbee2MQTT","sw":"2.0.0","url":"https://www.zigbee2mqtt.io"},"unique_id":"0x00212effff0cb8b6_effect_zigbee2mqtt"}'
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0x00212effff0cb8b6/power_on_behavior/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0x00212effff0cb8b6/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0x0ceff6fffebf4739/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'light/0xa4c138541ec8ddd2/light/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0xa4c138541ec8ddd2/effect/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0xa4c138541ec8ddd2/power_on_behavior/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c138541ec8ddd2/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'binary_sensor/0xa4c1384187f0960d/water_leak/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'binary_sensor/0xa4c1384187f0960d/battery_low/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1384187f0960d/battery/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1384187f0960d/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'light/0x001788010d1c884e/light/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0x001788010d1c884e/power_on_behavior/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0x001788010d1c884e/effect/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0x001788010d1c884e/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'update/0x001788010d1c884e/update/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0x001788010e8a8be7/battery/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0x001788010e8a8be7/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'update/0x001788010e8a8be7/update/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'light/0x00158d00053a1aab/light/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0x00158d00053a1aab/effect/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0x00158d00053a1aab/power_on_behavior/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0x00158d00053a1aab/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'light/0x00158d00053c6311/light/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0x00158d00053c6311/effect/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0x00158d00053c6311/power_on_behavior/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0x00158d00053c6311/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'binary_sensor/0xa4c13864e6c8c400/occupancy/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'binary_sensor/0xa4c13864e6c8c400/battery_low/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c13864e6c8c400/battery/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c13864e6c8c400/voltage/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'binary_sensor/0xa4c13864e6c8c400/tamper/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c13864e6c8c400/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'binary_sensor/0xa4c138ef60e2fdbe/contact/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c138ef60e2fdbe/battery/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c138ef60e2fdbe/voltage/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'binary_sensor/0xa4c138ef60e2fdbe/tamper/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c138ef60e2fdbe/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'light/0xf0d1b800001388f0/light/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0xf0d1b800001388f0/effect/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xf0d1b800001388f0/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'update/0xf0d1b800001388f0/update/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'light/0x7cb03eaa0a0176bd/light/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0x7cb03eaa0a0176bd/effect/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0x7cb03eaa0a0176bd/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'update/0x7cb03eaa0a0176bd/update/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0x000d6f001417c142/battery/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0x000d6f001417c142/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'update/0x000d6f001417c142/update/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c138e68023f4c6/battery/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'binary_sensor/0xa4c138e68023f4c6/water_leak/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'binary_sensor/0xa4c138e68023f4c6/battery_low/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c138e68023f4c6/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c13838ba59a1b2/temperature/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c13838ba59a1b2/humidity/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0xa4c13838ba59a1b2/temperature_unit/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'number/0xa4c13838ba59a1b2/temperature_calibration/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'number/0xa4c13838ba59a1b2/humidity_calibration/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c13838ba59a1b2/battery/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c13838ba59a1b2/linkquality/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1389d42e94844/temperature/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1389d42e94844/humidity/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'select/0xa4c1389d42e94844/temperature_unit/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'number/0xa4c1389d42e94844/temperature_calibration/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'number/0xa4c1389d42e94844/humidity_calibration/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1389d42e94844/battery/config', already discovered
[2025-01-19 22:58:17] debug: 	z2m: Skipping discovery of 'sensor/0xa4c1389d42e94844/linkquality/config', already discovered
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 11
[2025-01-19 22:58:20] debug: 	zh:deconz:frameparser: device state: 10101010
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 12
[2025-01-19 22:58:20] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 12 srcAddr: 0xf8fd destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 22:58:20] debug: 	zh:deconz:frameparser: response payload: 18fdf8b2a159ba3838c1a480
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:20] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":63741,"eui64":"0xa4c13838ba59a1b2","capabilities":{"alternatePANCoordinator":0,"deviceType":0,"powerSource":0,"rxOnWhenIdle":0,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:58:20] debug: 	zh:controller: Device announce from '0xa4c13838ba59a1b2:63741'
[2025-01-19 22:58:20] debug: 	z2m: Device 'Medienschrank Wohnzimmer' announced itself
[2025-01-19 22:58:20] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Medienschrank Wohnzimmer","ieee_address":"0xa4c13838ba59a1b2"},"type":"device_announce"}'
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 13
[2025-01-19 22:58:20] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 13 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0xef00 lqi: 255
[2025-01-19 22:58:20] debug: 	zh:deconz:frameparser: response payload: 09220200220102000400000120
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:20] debug: 	zh:controller: Received payload: clusterID=61184, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":34,"commandIdentifier":2},"payload":{"seq":8704,"dpValues":[{"dp":1,"datatype":2,"data":{"type":"Buffer","data":[0,0,1,32]}}]},"command":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}],"name":"dataReport"}}
[2025-01-19 22:58:20] debug: 	zh:controller:endpoint: ZCL command 0xa4c13838ba59a1b2/1 manuSpecificTuya.defaultRsp({"cmdId":2,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"transactionSequenceNumber":34,"writeUndiv":false})
[2025-01-19 22:58:20] debug: 	zh:deconz: no response expected (34)
[2025-01-19 22:58:20] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'commandDataReport', cluster 'manuSpecificTuya', data '{"dpValues":[{"data":{"data":[0,0,1,32],"type":"Buffer"},"datatype":2,"dp":1}],"seq":8704}' from endpoint 1 with groupID 0
[2025-01-19 22:58:20] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":43,"humidity_calibration":0,"linkquality":255,"temperature":28.8,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:1 SeqNr. 14 request id: 1
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:20] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 1 status: 0
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 15
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:20] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101110
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:20] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 15 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0xef00 lqi: 255
[2025-01-19 22:58:20] debug: 	zh:deconz:frameparser: response payload: 0923020023020200040000002a
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:20] debug: 	zh:controller: Received payload: clusterID=61184, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":35,"commandIdentifier":2},"payload":{"seq":8960,"dpValues":[{"dp":2,"datatype":2,"data":{"type":"Buffer","data":[0,0,0,42]}}]},"command":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}],"name":"dataReport"}}
[2025-01-19 22:58:20] debug: 	zh:controller:endpoint: ZCL command 0xa4c13838ba59a1b2/1 manuSpecificTuya.defaultRsp({"cmdId":2,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"transactionSequenceNumber":35,"writeUndiv":false})
[2025-01-19 22:58:20] debug: 	zh:deconz: no response expected (35)
[2025-01-19 22:58:20] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'commandDataReport', cluster 'manuSpecificTuya', data '{"dpValues":[{"data":{"data":[0,0,0,42],"type":"Buffer"},"datatype":2,"dp":2}],"seq":8960}' from endpoint 1 with groupID 0
[2025-01-19 22:58:20] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":42,"humidity_calibration":0,"linkquality":255,"temperature":28.8,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 16
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:1 SeqNr. 17 request id: 2
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 18
[2025-01-19 22:58:20] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 2 status: 0
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:20] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 1 confirm status: 0
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:20] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 34
[2025-01-19 22:58:20] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:58:20] debug: 	zh:deconz: resolve request (34)
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 19
[2025-01-19 22:58:20] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:20] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 2 confirm status: 0
[2025-01-19 22:58:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:20] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 35
[2025-01-19 22:58:20] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:58:20] debug: 	zh:deconz: resolve request (35)
[2025-01-19 22:58:21] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 20
[2025-01-19 22:58:21] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 20 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0xef00 lqi: 255
[2025-01-19 22:58:21] debug: 	zh:deconz:frameparser: response payload: 0931020031020200040000002a
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:21] debug: 	zh:controller: Received payload: clusterID=61184, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":49,"commandIdentifier":2},"payload":{"seq":12544,"dpValues":[{"dp":2,"datatype":2,"data":{"type":"Buffer","data":[0,0,0,42]}}]},"command":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}],"name":"dataReport"}}
[2025-01-19 22:58:21] debug: 	zh:controller:endpoint: ZCL command 0xa4c13838ba59a1b2/1 manuSpecificTuya.defaultRsp({"cmdId":2,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"transactionSequenceNumber":49,"writeUndiv":false})
[2025-01-19 22:58:21] debug: 	zh:deconz: no response expected (49)
[2025-01-19 22:58:21] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'commandDataReport', cluster 'manuSpecificTuya', data '{"dpValues":[{"data":{"data":[0,0,0,42],"type":"Buffer"},"datatype":2,"dp":2}],"seq":12544}' from endpoint 1 with groupID 0
[2025-01-19 22:58:21] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":42,"humidity_calibration":0,"linkquality":255,"temperature":28.8,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:1 SeqNr. 21 request id: 3
[2025-01-19 22:58:21] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 3 status: 0
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:21] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 22
[2025-01-19 22:58:21] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 3 confirm status: 0
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:21] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 49
[2025-01-19 22:58:21] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:58:21] debug: 	zh:deconz: resolve request (49)
[2025-01-19 22:58:21] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 23
[2025-01-19 22:58:21] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 23 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0x402 lqi: 255
[2025-01-19 22:58:21] debug: 	zh:deconz:frameparser: response payload: 18320a000029040b
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:21] debug: 	zh:controller: Received payload: clusterID=1026, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":50,"commandIdentifier":10},"payload":[{"attrId":0,"dataType":41,"attrData":2820}],"command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}}
[2025-01-19 22:58:21] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'attributeReport', cluster 'msTemperatureMeasurement', data '{"measuredValue":2820}' from endpoint 1 with groupID 0
[2025-01-19 22:58:21] debug: 	z2m: No converter available for 'ZG-227Z' with cluster 'msTemperatureMeasurement' and type 'attributeReport' and data '{"measuredValue":2820}'
[2025-01-19 22:58:21] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 24
[2025-01-19 22:58:21] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 24 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0x405 lqi: 255
[2025-01-19 22:58:21] debug: 	zh:deconz:frameparser: response payload: 18330a0000217210
[2025-01-19 22:58:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:21] debug: 	zh:controller: Received payload: clusterID=1029, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":51,"commandIdentifier":10},"payload":[{"attrId":0,"dataType":33,"attrData":4210}],"command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}}
[2025-01-19 22:58:21] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'attributeReport', cluster 'msRelativeHumidity', data '{"measuredValue":4210}' from endpoint 1 with groupID 0
[2025-01-19 22:58:21] debug: 	z2m: No converter available for 'ZG-227Z' with cluster 'msRelativeHumidity' and type 'attributeReport' and data '{"measuredValue":4210}'
[2025-01-19 22:58:22] debug: 	z2m: Retrieving state of 'Medienschrank Wohnzimmer' after reconnect
[2025-01-19 22:58:27] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:27] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:27] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:27] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 25
[2025-01-19 22:58:27] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 25 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 22:58:27] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 22:58:27] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:27] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:58:27] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 22:58:27] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 22:58:27] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 22:58:28] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:28] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:28] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:28] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 26
[2025-01-19 22:58:28] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 26 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 159
[2025-01-19 22:58:28] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:58:28] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:28] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:58:28] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:58:28] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:58:28] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:58:29] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 22:58:29] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:58:29] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 27 request id: 4
[2025-01-19 22:58:29] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 4 status: 0
[2025-01-19 22:58:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:30] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 22:58:30] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:58:30] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 28 request id: 5
[2025-01-19 22:58:30] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 5 status: 0
[2025-01-19 22:58:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:30] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 29
[2025-01-19 22:58:30] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 22:58:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:31] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:31] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:31] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 30
[2025-01-19 22:58:31] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 30 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 159
[2025-01-19 22:58:31] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:58:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:31] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:58:31] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:58:31] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:58:32] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:58:34] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 22:58:34] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:58:34] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 31 request id: 6
[2025-01-19 22:58:34] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 6 status: 0
[2025-01-19 22:58:34] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:34] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:58:34] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:34] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:34] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 32
[2025-01-19 22:58:34] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 6 confirm status: 0
[2025-01-19 22:58:34] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:34] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 4
[2025-01-19 22:58:34] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 22:58:34] debug: 	zh:deconz: resolve request (4)
[2025-01-19 22:58:39] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:58:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:39] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:39] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 33
[2025-01-19 22:58:39] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 4 confirm status: 0
[2025-01-19 22:58:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:39] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 2
[2025-01-19 22:58:39] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 22:58:39] debug: 	zh:deconz: resolve request (2)
[2025-01-19 22:58:40] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (2) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 22:58:40] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (2) Error: waiting for response TIMEOUT))
[2025-01-19 22:58:40] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 34
[2025-01-19 22:58:40] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:58:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:40] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:40] debug: 	zh:deconz:frameparser: device state: 10100110
[2025-01-19 22:58:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:40] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 35
[2025-01-19 22:58:40] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:40] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 36
[2025-01-19 22:58:40] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 5 confirm status: 0
[2025-01-19 22:58:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:40] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 3
[2025-01-19 22:58:40] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 22:58:40] debug: 	zh:deconz: resolve request (3)
[2025-01-19 22:58:40] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (3) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 22:58:40] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (3) Error: waiting for response TIMEOUT))
[2025-01-19 22:58:43] debug: 	z2m:mqtt: Received MQTT message on 'homeassistant/status' with data 'online'
[2025-01-19 22:58:44] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (4) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 22:58:44] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (4) Error: waiting for response TIMEOUT))
[2025-01-19 22:58:48] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:48] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:48] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 37
[2025-01-19 22:58:48] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 37 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0xef00 lqi: 255
[2025-01-19 22:58:48] debug: 	zh:deconz:frameparser: response payload: 09340200340102000400000116
[2025-01-19 22:58:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:48] debug: 	zh:controller: Received payload: clusterID=61184, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":52,"commandIdentifier":2},"payload":{"seq":13312,"dpValues":[{"dp":1,"datatype":2,"data":{"type":"Buffer","data":[0,0,1,22]}}]},"command":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}],"name":"dataReport"}}
[2025-01-19 22:58:48] debug: 	zh:controller:endpoint: ZCL command 0xa4c13838ba59a1b2/1 manuSpecificTuya.defaultRsp({"cmdId":2,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"transactionSequenceNumber":52,"writeUndiv":false})
[2025-01-19 22:58:48] debug: 	zh:deconz: no response expected (52)
[2025-01-19 22:58:48] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'commandDataReport', cluster 'manuSpecificTuya', data '{"dpValues":[{"data":{"data":[0,0,1,22],"type":"Buffer"},"datatype":2,"dp":1}],"seq":13312}' from endpoint 1 with groupID 0
[2025-01-19 22:58:48] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":42,"humidity_calibration":0,"linkquality":255,"temperature":27.8,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 22:58:48] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:1 SeqNr. 38 request id: 7
[2025-01-19 22:58:48] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 7 status: 0
[2025-01-19 22:58:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:48] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:58:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:48] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:48] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 39
[2025-01-19 22:58:48] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 7 confirm status: 0
[2025-01-19 22:58:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:48] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 52
[2025-01-19 22:58:48] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:58:48] debug: 	zh:deconz: resolve request (52)
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 40
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 40 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0xef00 lqi: 255
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: response payload: 0935020035020200040000002a
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:49] debug: 	zh:controller: Received payload: clusterID=61184, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":53,"commandIdentifier":2},"payload":{"seq":13568,"dpValues":[{"dp":2,"datatype":2,"data":{"type":"Buffer","data":[0,0,0,42]}}]},"command":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}],"name":"dataReport"}}
[2025-01-19 22:58:49] debug: 	zh:controller:endpoint: ZCL command 0xa4c13838ba59a1b2/1 manuSpecificTuya.defaultRsp({"cmdId":2,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"transactionSequenceNumber":53,"writeUndiv":false})
[2025-01-19 22:58:49] debug: 	zh:deconz: no response expected (53)
[2025-01-19 22:58:49] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'commandDataReport', cluster 'manuSpecificTuya', data '{"dpValues":[{"data":{"data":[0,0,0,42],"type":"Buffer"},"datatype":2,"dp":2}],"seq":13568}' from endpoint 1 with groupID 0
[2025-01-19 22:58:49] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":42,"humidity_calibration":0,"linkquality":255,"temperature":27.8,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:1 SeqNr. 41 request id: 8
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 8 status: 0
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 42
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 42 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:49] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:58:49] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 22:58:49] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 22:58:49] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 43
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101110
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 44
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 43 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 159
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:49] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:58:49] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:58:49] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:58:49] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 45
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 46
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 8 confirm status: 0
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:49] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 53
[2025-01-19 22:58:49] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:58:49] debug: 	zh:deconz: resolve request (53)
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 47
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 47 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0x402 lqi: 255
[2025-01-19 22:58:49] debug: 	zh:deconz:frameparser: response payload: 18360a000029dc0a
[2025-01-19 22:58:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:49] debug: 	zh:controller: Received payload: clusterID=1026, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":54,"commandIdentifier":10},"payload":[{"attrId":0,"dataType":41,"attrData":2780}],"command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}}
[2025-01-19 22:58:49] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'attributeReport', cluster 'msTemperatureMeasurement', data '{"measuredValue":2780}' from endpoint 1 with groupID 0
[2025-01-19 22:58:49] debug: 	z2m: No converter available for 'ZG-227Z' with cluster 'msTemperatureMeasurement' and type 'attributeReport' and data '{"measuredValue":2780}'
[2025-01-19 22:58:50] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:50] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:50] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 48
[2025-01-19 22:58:50] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 48 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0x405 lqi: 255
[2025-01-19 22:58:50] debug: 	zh:deconz:frameparser: response payload: 18370a0000219010
[2025-01-19 22:58:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:50] debug: 	zh:controller: Received payload: clusterID=1029, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":55,"commandIdentifier":10},"payload":[{"attrId":0,"dataType":33,"attrData":4240}],"command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}}
[2025-01-19 22:58:50] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'attributeReport', cluster 'msRelativeHumidity', data '{"measuredValue":4240}' from endpoint 1 with groupID 0
[2025-01-19 22:58:50] debug: 	z2m: No converter available for 'ZG-227Z' with cluster 'msRelativeHumidity' and type 'attributeReport' and data '{"measuredValue":4240}'
[2025-01-19 22:58:50] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 49
[2025-01-19 22:58:50] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 22:58:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:51] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 22:58:51] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 50 request id: 9
[2025-01-19 22:58:51] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 9 status: 0
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:51] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 22:58:51] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 51 request id: 10
[2025-01-19 22:58:51] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 10 status: 0
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:51] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 52
[2025-01-19 22:58:51] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 10 confirm status: 0
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:51] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 6
[2025-01-19 22:58:51] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 22:58:51] debug: 	zh:deconz: resolve request (6)
[2025-01-19 22:58:51] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 53
[2025-01-19 22:58:51] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 53 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 255
[2025-01-19 22:58:51] debug: 	zh:deconz:frameparser: response payload: 0806010000001000
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:51] debug: 	zh:controller: Received payload: clusterID=6, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":6,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":16,"attrData":0}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 22:58:51] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":6,"writeUndiv":false})
[2025-01-19 22:58:51] debug: 	zh:deconz: no response expected (6)
[2025-01-19 22:58:51] debug: 	zh:deconz: response received (6)
[2025-01-19 22:58:51] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genOnOff', data '{"onOff":0}' from endpoint 1 with groupID 0
[2025-01-19 22:58:51] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":255,"state":"OFF","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 54 request id: 11
[2025-01-19 22:58:51] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 11 status: 0
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:51] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 55
[2025-01-19 22:58:51] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 11 confirm status: 0
[2025-01-19 22:58:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:51] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 6
[2025-01-19 22:58:51] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:58:51] debug: 	zh:deconz: resolve request (6)
[2025-01-19 22:58:53] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:53] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:53] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 56
[2025-01-19 22:58:53] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 56 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 159
[2025-01-19 22:58:53] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:58:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:53] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:58:53] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:58:53] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:58:53] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:58:53] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:53] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:53] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 57
[2025-01-19 22:58:53] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 57 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 159
[2025-01-19 22:58:53] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:58:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:53] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:58:53] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:58:53] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:58:53] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:58:55] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:55] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:55] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:55] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 58
[2025-01-19 22:58:55] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 58 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 151
[2025-01-19 22:58:55] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:58:55] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:55] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:58:55] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:58:55] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:58:55] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:58:57] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 22:58:57] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 59 request id: 12
[2025-01-19 22:58:57] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 12 status: 0
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:57] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 60
[2025-01-19 22:58:57] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 12 confirm status: 0
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:57] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 7
[2025-01-19 22:58:57] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 22:58:57] debug: 	zh:deconz: resolve request (7)
[2025-01-19 22:58:57] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 61
[2025-01-19 22:58:57] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 61 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 151
[2025-01-19 22:58:57] debug: 	zh:deconz:frameparser: response payload: 0807010000001000
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:57] debug: 	zh:controller: Received payload: clusterID=6, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=151, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":7,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":16,"attrData":0}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 22:58:57] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":7,"writeUndiv":false})
[2025-01-19 22:58:57] debug: 	zh:deconz: no response expected (7)
[2025-01-19 22:58:57] debug: 	zh:deconz: response received (7)
[2025-01-19 22:58:57] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genOnOff', data '{"onOff":0}' from endpoint 1 with groupID 0
[2025-01-19 22:58:57] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":151,"state":"OFF","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 62 request id: 13
[2025-01-19 22:58:57] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 13 status: 0
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:57] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 63
[2025-01-19 22:58:57] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 13 confirm status: 0
[2025-01-19 22:58:57] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:58:57] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 7
[2025-01-19 22:58:57] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:58:57] debug: 	zh:deconz: resolve request (7)
[2025-01-19 22:59:00] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 64
[2025-01-19 22:59:00] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 22:59:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:01] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:01] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:01] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:01] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 65
[2025-01-19 22:59:01] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 9 confirm status: 0
[2025-01-19 22:59:01] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:01] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 5
[2025-01-19 22:59:01] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 22:59:01] debug: 	zh:deconz: resolve request (5)
[2025-01-19 22:59:01] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (5) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 22:59:01] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (5) Error: waiting for response TIMEOUT))
[2025-01-19 22:59:10] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 66
[2025-01-19 22:59:10] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 22:59:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Fernbedienung', payload '{"battery":100,"linkquality":247,"update":{"installed_version":-1,"latest_version":-1,"state":null},"voltage":3000}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":151,"state":"OFF","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/0xa4c138570b1956d9', payload '{"battery":20,"humidity":64.87,"linkquality":7,"temperature":22.35,"voltage":null}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/0xa4c1383ec7aa7d95', payload '{"battery":26,"humidity":58.31,"linkquality":255,"temperature":23.81,"voltage":null}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/0xa4c1383db5531833', payload '{"battery":17,"humidity":73.5,"linkquality":87,"temperature":20.4,"update":{"installed_version":268513281,"latest_version":268513281,"state":"idle"},"voltage":null}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Lichtschlauch', payload '{"brightness_rgb":26,"brightness_white":254,"color":{"x":0.6942,"y":0.2963},"color_mode":"xy","color_mode_rgb":"color_temp","color_mode_white":"color_temp","color_rgb":{"x":0.3445,"y":0.3512},"color_temp_rgb":199,"color_temp_white":365,"color_white":{"x":0.4566,"y":0.4098},"effect":null,"linkquality":255,"power_on_behavior":null,"state":"OFF","state_10":"OFF","state_rgb":"OFF","state_white":"OFF"}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/0x0ceff6fffebf4739', payload '{"linkquality":119}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Flur', payload '{"brightness":152,"effect":null,"linkquality":255,"power_on_behavior":null,"state":"ON"}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Wasser Sensor Spüle', payload '{"battery":100,"battery_low":false,"linkquality":207,"tamper":false,"voltage":2800,"water_leak":false}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Badlampe', payload '{"brightness":254,"color_mode":"color_temp","color_temp":366,"effect":null,"linkquality":87,"power_on_behavior":null,"state":"ON","update":{"installed_version":16784652,"latest_version":16786434,"state":"available"}}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Fernbedienung Bad', payload '{"battery":100,"linkquality":255,"update":{"installed_version":33565954,"latest_version":33565954,"state":"idle"}}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/0x00158d00053a1aab', payload '{"color_mode":"xy","effect":null,"linkquality":255,"power_on_behavior":null,"state":null}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/0x00158d00053c6311', payload '{"color_mode":"xy","effect":null,"linkquality":255,"power_on_behavior":null,"state":"ON"}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bewegungsmelder 1', payload '{"battery":93,"battery_low":false,"linkquality":255,"occupancy":false,"tamper":false,"voltage":2900}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Sensor Terassentür', payload '{"battery":100,"battery_low":false,"contact":true,"linkquality":239,"tamper":false,"voltage":2800}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Flurlicht', payload '{"brightness":229,"effect":null,"linkquality":255,"state":"ON","update":{"installed_version":17130496,"latest_version":17130496,"state":"idle"}}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Küchentisch', payload '{"brightness":254,"effect":null,"linkquality":255,"state":"OFF","update":{"installed_version":16909584,"latest_version":16909584,"state":"idle"}}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Fernbedienung 2', payload '{"battery":100,"linkquality":239,"update":{"installed_version":-1,"latest_version":-1,"state":null},"voltage":3000}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Wassersensor Keller', payload '{"battery":100,"battery_low":false,"linkquality":255,"water_leak":false}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":42,"humidity_calibration":0,"linkquality":255,"temperature":27.8,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 22:59:13] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Temperatur Keller', payload '{"battery":100,"humidity":43,"humidity_calibration":0,"linkquality":63,"temperature":20.9,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 22:59:17] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:17] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:17] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 67
[2025-01-19 22:59:17] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 67 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 22:59:17] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 22:59:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:17] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:59:17] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 22:59:17] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 22:59:17] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 22:59:17] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:17] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:17] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 68
[2025-01-19 22:59:17] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 68 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 159
[2025-01-19 22:59:17] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:59:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:17] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:59:17] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:59:17] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:59:17] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 69
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 69 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0xef00 lqi: 255
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: response payload: 09380200380102000400000113
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:controller: Received payload: clusterID=61184, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":56,"commandIdentifier":2},"payload":{"seq":14336,"dpValues":[{"dp":1,"datatype":2,"data":{"type":"Buffer","data":[0,0,1,19]}}]},"command":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}],"name":"dataReport"}}
[2025-01-19 22:59:19] debug: 	zh:controller:endpoint: ZCL command 0xa4c13838ba59a1b2/1 manuSpecificTuya.defaultRsp({"cmdId":2,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"transactionSequenceNumber":56,"writeUndiv":false})
[2025-01-19 22:59:19] debug: 	zh:deconz: no response expected (56)
[2025-01-19 22:59:19] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'commandDataReport', cluster 'manuSpecificTuya', data '{"dpValues":[{"data":{"data":[0,0,1,19],"type":"Buffer"},"datatype":2,"dp":1}],"seq":14336}' from endpoint 1 with groupID 0
[2025-01-19 22:59:19] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":42,"humidity_calibration":0,"linkquality":255,"temperature":27.5,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:1 SeqNr. 70 request id: 14
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 14 status: 0
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 71
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 14 confirm status: 0
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 56
[2025-01-19 22:59:19] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:59:19] debug: 	zh:deconz: resolve request (56)
[2025-01-19 22:59:19] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 22:59:19] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 72 request id: 15
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 15 status: 0
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 22:59:19] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 73 request id: 16
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 16 status: 0
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 74
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101110
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 75
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 74 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0xef00 lqi: 255
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: response payload: 0939020039020200040000002b
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:controller: Received payload: clusterID=61184, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":57,"commandIdentifier":2},"payload":{"seq":14592,"dpValues":[{"dp":2,"datatype":2,"data":{"type":"Buffer","data":[0,0,0,43]}}]},"command":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}],"name":"dataReport"}}
[2025-01-19 22:59:19] debug: 	zh:controller:endpoint: ZCL command 0xa4c13838ba59a1b2/1 manuSpecificTuya.defaultRsp({"cmdId":2,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"transactionSequenceNumber":57,"writeUndiv":false})
[2025-01-19 22:59:19] debug: 	zh:deconz: no response expected (57)
[2025-01-19 22:59:19] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'commandDataReport', cluster 'manuSpecificTuya', data '{"dpValues":[{"data":{"data":[0,0,0,43],"type":"Buffer"},"datatype":2,"dp":2}],"seq":14592}' from endpoint 1 with groupID 0
[2025-01-19 22:59:19] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":43,"humidity_calibration":0,"linkquality":255,"temperature":27.5,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 76
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:1 SeqNr. 77 request id: 17
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 78
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 16 confirm status: 0
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 9
[2025-01-19 22:59:19] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 22:59:19] debug: 	zh:deconz: resolve request (9)
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 17 status: 0
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 79
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101110
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 79 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 159
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: response payload: 0809010000001000
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:controller: Received payload: clusterID=6, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=159, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":9,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":16,"attrData":0}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 22:59:19] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":9,"writeUndiv":false})
[2025-01-19 22:59:19] debug: 	zh:deconz: no response expected (9)
[2025-01-19 22:59:19] debug: 	zh:deconz: response received (9)
[2025-01-19 22:59:19] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genOnOff', data '{"onOff":0}' from endpoint 1 with groupID 0
[2025-01-19 22:59:19] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":159,"state":"OFF","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 80 request id: 18
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 81
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 18 status: 0
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 82
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 17 confirm status: 0
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 57
[2025-01-19 22:59:19] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:59:19] debug: 	zh:deconz: resolve request (57)
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 83
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 18 confirm status: 0
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 9
[2025-01-19 22:59:19] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:59:19] debug: 	zh:deconz: resolve request (9)
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 84
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 85
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 85 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 159
[2025-01-19 22:59:19] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:59:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:19] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:59:19] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:59:19] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:59:20] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:59:20] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:20] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:20] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 86
[2025-01-19 22:59:20] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 86 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 159
[2025-01-19 22:59:20] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:59:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:20] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:59:20] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:59:20] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:59:20] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:59:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 87
[2025-01-19 22:59:20] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 22:59:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:22] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 22:59:22] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:59:22] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 88 request id: 19
[2025-01-19 22:59:22] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 19 status: 0
[2025-01-19 22:59:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:22] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:22] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:22] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 89
[2025-01-19 22:59:22] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 19 confirm status: 0
[2025-01-19 22:59:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:22] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 10
[2025-01-19 22:59:22] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 22:59:22] debug: 	zh:deconz: resolve request (10)
[2025-01-19 22:59:24] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:24] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:24] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 90
[2025-01-19 22:59:24] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 90 srcAddr: 0xec54 destAddr: 0x0 profile id: 0x104 cluster id: 0x500 lqi: 255
[2025-01-19 22:59:24] debug: 	zh:deconz:frameparser: response payload: 08210a13002001
[2025-01-19 22:59:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:24] debug: 	zh:controller: Received payload: clusterID=1280, address=60500, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":33,"commandIdentifier":10},"payload":[{"attrId":19,"dataType":32,"attrData":1}],"command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}}
[2025-01-19 22:59:24] debug: 	zh:controller:endpoint: ZCL command 0xa4c138e68023f4c6/1 ssIasZone.defaultRsp({"cmdId":10,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":33,"writeUndiv":false})
[2025-01-19 22:59:24] debug: 	zh:controller:endpoint: Request Queue (0xa4c138e68023f4c6/1): send defaultRsp request immediately (sendPolicy=undefined)
[2025-01-19 22:59:24] debug: 	zh:deconz: no response expected (33)
[2025-01-19 22:59:24] debug: 	z2m: Received Zigbee message from 'Wassersensor Keller', type 'attributeReport', cluster 'ssIasZone', data '{"currentZoneSensitivityLevel":1}' from endpoint 1 with groupID 0
[2025-01-19 22:59:24] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xec54 EP:1 SeqNr. 91 request id: 20
[2025-01-19 22:59:24] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 20 status: 0
[2025-01-19 22:59:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:24] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:24] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:24] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 92
[2025-01-19 22:59:24] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xec54 request id: 20 confirm status: 0
[2025-01-19 22:59:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:24] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 33
[2025-01-19 22:59:24] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:59:24] debug: 	zh:deconz: resolve request (33)
[2025-01-19 22:59:27] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:27] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:27] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:27] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 93
[2025-01-19 22:59:27] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 93 srcAddr: 0xec54 destAddr: 0x0 profile id: 0x104 cluster id: 0x1 lqi: 255
[2025-01-19 22:59:27] debug: 	zh:deconz:frameparser: response payload: 08250a2000201d
[2025-01-19 22:59:27] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:27] debug: 	zh:controller: Received payload: clusterID=1, address=60500, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":37,"commandIdentifier":10},"payload":[{"attrId":32,"dataType":32,"attrData":29}],"command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}}
[2025-01-19 22:59:27] debug: 	zh:controller:endpoint: ZCL command 0xa4c138e68023f4c6/1 genPowerCfg.defaultRsp({"cmdId":10,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":37,"writeUndiv":false})
[2025-01-19 22:59:27] debug: 	zh:controller:endpoint: Request Queue (0xa4c138e68023f4c6/1): send defaultRsp request immediately (sendPolicy=undefined)
[2025-01-19 22:59:27] debug: 	zh:deconz: no response expected (37)
[2025-01-19 22:59:27] debug: 	z2m: Received Zigbee message from 'Wassersensor Keller', type 'attributeReport', cluster 'genPowerCfg', data '{"batteryVoltage":29}' from endpoint 1 with groupID 0
[2025-01-19 22:59:27] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xec54 EP:1 SeqNr. 94 request id: 21
[2025-01-19 22:59:27] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 21 status: 0
[2025-01-19 22:59:27] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:27] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:27] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:27] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:27] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 95
[2025-01-19 22:59:27] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xec54 request id: 21 confirm status: 0
[2025-01-19 22:59:27] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:27] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 37
[2025-01-19 22:59:27] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:59:27] debug: 	zh:deconz: resolve request (37)
[2025-01-19 22:59:29] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:29] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:29] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 96
[2025-01-19 22:59:29] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 15 confirm status: 0
[2025-01-19 22:59:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:29] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 8
[2025-01-19 22:59:29] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 22:59:29] debug: 	zh:deconz: resolve request (8)
[2025-01-19 22:59:29] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (8) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 22:59:29] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (8) Error: waiting for response TIMEOUT))
[2025-01-19 22:59:30] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 97
[2025-01-19 22:59:30] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 22:59:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:32] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (10) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 22:59:32] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (10) Error: waiting for response TIMEOUT))
[2025-01-19 22:59:40] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 98
[2025-01-19 22:59:40] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 22:59:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:45] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:45] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:45] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:45] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 99
[2025-01-19 22:59:45] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 99 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 22:59:45] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:59:45] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:45] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:59:45] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:59:45] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:59:45] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:59:45] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:45] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:45] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:45] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 100
[2025-01-19 22:59:45] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 100 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 22:59:45] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 22:59:45] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:45] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:59:45] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 22:59:45] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 22:59:45] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 22:59:46] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Bogenlampe/set' with data '{"state":"ON"}'
[2025-01-19 22:59:46] debug: 	z2m: Publishing 'set' 'state' to 'Bogenlampe'
[2025-01-19 22:59:47] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 101 request id: 22
[2025-01-19 22:59:47] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 22 status: 0
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:47] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 102
[2025-01-19 22:59:47] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 22 confirm status: 0
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:47] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 11
[2025-01-19 22:59:47] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 22:59:47] debug: 	zh:deconz: resolve request (11)
[2025-01-19 22:59:47] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 22:59:47] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 103 request id: 23
[2025-01-19 22:59:47] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 23 status: 0
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:47] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 104
[2025-01-19 22:59:47] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 23 confirm status: 0
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:47] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 12
[2025-01-19 22:59:47] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 22:59:47] debug: 	zh:deconz: resolve request (12)
[2025-01-19 22:59:47] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 22:59:47] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 105 request id: 24
[2025-01-19 22:59:47] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 24 status: 0
[2025-01-19 22:59:47] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:48] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Bogenlampe/set' with data '{"state":"OFF"}'
[2025-01-19 22:59:48] debug: 	z2m: Publishing 'set' 'state' to 'Bogenlampe'
[2025-01-19 22:59:48] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:59:48] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 106 request id: 25
[2025-01-19 22:59:48] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 25 status: 0
[2025-01-19 22:59:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:48] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:48] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:48] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 107
[2025-01-19 22:59:48] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 25 confirm status: 0
[2025-01-19 22:59:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:48] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 14
[2025-01-19 22:59:48] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 22:59:48] debug: 	zh:deconz: resolve request (14)
[2025-01-19 22:59:48] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:48] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:48] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 108
[2025-01-19 22:59:48] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 108 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 22:59:48] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:59:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:48] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:59:48] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:59:48] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:59:49] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:59:49] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:49] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:49] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 109
[2025-01-19 22:59:49] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 109 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 22:59:49] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:59:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:49] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:59:49] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:59:49] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:59:49] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:59:49] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:49] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:49] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 110
[2025-01-19 22:59:49] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 110 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 22:59:49] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:59:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:49] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:59:49] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:59:49] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:59:49] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:59:50] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 111
[2025-01-19 22:59:50] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 22:59:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:51] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 22:59:51] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 112 request id: 26
[2025-01-19 22:59:51] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 26 status: 0
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:51] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 113
[2025-01-19 22:59:51] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 26 confirm status: 0
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:51] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 15
[2025-01-19 22:59:51] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 22:59:51] debug: 	zh:deconz: resolve request (15)
[2025-01-19 22:59:51] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 114
[2025-01-19 22:59:51] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 114 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 167
[2025-01-19 22:59:51] debug: 	zh:deconz:frameparser: response payload: 080f010000001000
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:51] debug: 	zh:controller: Received payload: clusterID=6, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=167, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":15,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":16,"attrData":0}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 22:59:51] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":15,"writeUndiv":false})
[2025-01-19 22:59:51] debug: 	zh:deconz: no response expected (15)
[2025-01-19 22:59:51] debug: 	zh:deconz: response received (15)
[2025-01-19 22:59:51] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genOnOff', data '{"onOff":0}' from endpoint 1 with groupID 0
[2025-01-19 22:59:51] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":167,"state":"OFF","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 115 request id: 27
[2025-01-19 22:59:51] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 27 status: 0
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:51] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 116
[2025-01-19 22:59:51] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 27 confirm status: 0
[2025-01-19 22:59:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:51] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 15
[2025-01-19 22:59:51] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:59:51] debug: 	zh:deconz: resolve request (15)
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 117
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 117 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0xef00 lqi: 255
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: response payload: 093c02003c0102000400000110
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:52] debug: 	zh:controller: Received payload: clusterID=61184, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":60,"commandIdentifier":2},"payload":{"seq":15360,"dpValues":[{"dp":1,"datatype":2,"data":{"type":"Buffer","data":[0,0,1,16]}}]},"command":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}],"name":"dataReport"}}
[2025-01-19 22:59:52] debug: 	zh:controller:endpoint: ZCL command 0xa4c13838ba59a1b2/1 manuSpecificTuya.defaultRsp({"cmdId":2,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"transactionSequenceNumber":60,"writeUndiv":false})
[2025-01-19 22:59:52] debug: 	zh:deconz: no response expected (60)
[2025-01-19 22:59:52] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'commandDataReport', cluster 'manuSpecificTuya', data '{"dpValues":[{"data":{"data":[0,0,1,16],"type":"Buffer"},"datatype":2,"dp":1}],"seq":15360}' from endpoint 1 with groupID 0
[2025-01-19 22:59:52] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":43,"humidity_calibration":0,"linkquality":255,"temperature":27.2,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:1 SeqNr. 118 request id: 28
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 28 status: 0
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 119
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 28 confirm status: 0
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:52] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 60
[2025-01-19 22:59:52] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:59:52] debug: 	zh:deconz: resolve request (60)
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 120
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 120 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0xef00 lqi: 255
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: response payload: 093d02003d020200040000002b
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:52] debug: 	zh:controller: Received payload: clusterID=61184, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":61,"commandIdentifier":2},"payload":{"seq":15616,"dpValues":[{"dp":2,"datatype":2,"data":{"type":"Buffer","data":[0,0,0,43]}}]},"command":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}],"name":"dataReport"}}
[2025-01-19 22:59:52] debug: 	zh:controller:endpoint: ZCL command 0xa4c13838ba59a1b2/1 manuSpecificTuya.defaultRsp({"cmdId":2,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"transactionSequenceNumber":61,"writeUndiv":false})
[2025-01-19 22:59:52] debug: 	zh:deconz: no response expected (61)
[2025-01-19 22:59:52] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'commandDataReport', cluster 'manuSpecificTuya', data '{"dpValues":[{"data":{"data":[0,0,0,43],"type":"Buffer"},"datatype":2,"dp":2}],"seq":15616}' from endpoint 1 with groupID 0
[2025-01-19 22:59:52] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":43,"humidity_calibration":0,"linkquality":255,"temperature":27.2,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:1 SeqNr. 121 request id: 29
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 29 status: 0
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 122
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 29 confirm status: 0
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:52] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 61
[2025-01-19 22:59:52] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:59:52] debug: 	zh:deconz: resolve request (61)
[2025-01-19 22:59:52] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Flurlicht/set' with data '{"state":"OFF"}'
[2025-01-19 22:59:52] debug: 	z2m: Publishing 'set' 'state' to 'Flurlicht'
[2025-01-19 22:59:52] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 123 request id: 30
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 30 status: 0
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 124
[2025-01-19 22:59:52] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 30 confirm status: 0
[2025-01-19 22:59:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:52] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 16
[2025-01-19 22:59:52] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 22:59:52] debug: 	zh:deconz: resolve request (16)
[2025-01-19 22:59:53] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 125
[2025-01-19 22:59:53] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 125 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0x402 lqi: 255
[2025-01-19 22:59:53] debug: 	zh:deconz:frameparser: response payload: 183e0a000029a00a
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:53] debug: 	zh:controller: Received payload: clusterID=1026, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":62,"commandIdentifier":10},"payload":[{"attrId":0,"dataType":41,"attrData":2720}],"command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}}
[2025-01-19 22:59:53] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'attributeReport', cluster 'msTemperatureMeasurement', data '{"measuredValue":2720}' from endpoint 1 with groupID 0
[2025-01-19 22:59:53] debug: 	z2m: No converter available for 'ZG-227Z' with cluster 'msTemperatureMeasurement' and type 'attributeReport' and data '{"measuredValue":2720}'
[2025-01-19 22:59:53] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 126
[2025-01-19 22:59:53] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 126 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0x405 lqi: 255
[2025-01-19 22:59:53] debug: 	zh:deconz:frameparser: response payload: 183f0a000021cc10
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:53] debug: 	zh:controller: Received payload: clusterID=1029, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":63,"commandIdentifier":10},"payload":[{"attrId":0,"dataType":33,"attrData":4300}],"command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}}
[2025-01-19 22:59:53] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'attributeReport', cluster 'msRelativeHumidity', data '{"measuredValue":4300}' from endpoint 1 with groupID 0
[2025-01-19 22:59:53] debug: 	z2m: No converter available for 'ZG-227Z' with cluster 'msRelativeHumidity' and type 'attributeReport' and data '{"measuredValue":4300}'
[2025-01-19 22:59:53] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Flurlicht/set' with data '{"state":"ON"}'
[2025-01-19 22:59:53] debug: 	z2m: Publishing 'set' 'state' to 'Flurlicht'
[2025-01-19 22:59:53] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 127 request id: 31
[2025-01-19 22:59:53] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 31 status: 0
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:53] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 128
[2025-01-19 22:59:53] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 31 confirm status: 0
[2025-01-19 22:59:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:53] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 17
[2025-01-19 22:59:53] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 22:59:53] debug: 	zh:deconz: resolve request (17)
[2025-01-19 22:59:54] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:54] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:54] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:54] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 129
[2025-01-19 22:59:54] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 129 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 183
[2025-01-19 22:59:54] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:59:54] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:54] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:59:54] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:59:54] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:59:54] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:59:56] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 22:59:56] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 130 request id: 32
[2025-01-19 22:59:56] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 32 status: 0
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:56] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 131
[2025-01-19 22:59:56] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 32 confirm status: 0
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:56] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 18
[2025-01-19 22:59:56] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 22:59:56] debug: 	zh:deconz: resolve request (18)
[2025-01-19 22:59:56] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 132
[2025-01-19 22:59:56] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 132 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 175
[2025-01-19 22:59:56] debug: 	zh:deconz:frameparser: response payload: 0812010000001000
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:56] debug: 	zh:controller: Received payload: clusterID=6, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=175, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":18,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":16,"attrData":0}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 22:59:56] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":18,"writeUndiv":false})
[2025-01-19 22:59:56] debug: 	zh:deconz: no response expected (18)
[2025-01-19 22:59:56] debug: 	zh:deconz: response received (18)
[2025-01-19 22:59:56] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genOnOff', data '{"onOff":0}' from endpoint 1 with groupID 0
[2025-01-19 22:59:56] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":175,"state":"OFF","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 133 request id: 33
[2025-01-19 22:59:56] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 33 status: 0
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:56] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 134
[2025-01-19 22:59:56] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 33 confirm status: 0
[2025-01-19 22:59:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:56] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 18
[2025-01-19 22:59:56] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 22:59:56] debug: 	zh:deconz: resolve request (18)
[2025-01-19 22:59:57] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (11) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 22:59:57] error: 	z2m: Publish 'set' 'state' to 'Bogenlampe' failed: 'Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (11) Error: waiting for response TIMEOUT)'
[2025-01-19 22:59:57] debug: 	z2m: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (11) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 22:59:58] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 22:59:58] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:58] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 22:59:58] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 135
[2025-01-19 22:59:58] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 24 confirm status: 0
[2025-01-19 22:59:58] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:58] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 13
[2025-01-19 22:59:58] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 22:59:58] debug: 	zh:deconz: resolve request (13)
[2025-01-19 22:59:58] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (13) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 22:59:58] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (12) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 22:59:58] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (13) Error: waiting for response TIMEOUT))
[2025-01-19 22:59:58] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (12) Error: waiting for response TIMEOUT))
[2025-01-19 22:59:58] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 22:59:58] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:58] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 22:59:58] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 136
[2025-01-19 22:59:58] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 136 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 22:59:58] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 22:59:58] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 22:59:58] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 22:59:58] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 22:59:58] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 22:59:58] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 22:59:59] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (14) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 22:59:59] error: 	z2m: Publish 'set' 'state' to 'Bogenlampe' failed: 'Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (14) Error: waiting for response TIMEOUT)'
[2025-01-19 22:59:59] debug: 	z2m: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (14) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 23:00:00] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:00:00] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:00:00] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 137 request id: 34
[2025-01-19 23:00:00] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 34 status: 0
[2025-01-19 23:00:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:00] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:00] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:00] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 138
[2025-01-19 23:00:00] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 34 confirm status: 0
[2025-01-19 23:00:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:00] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 19
[2025-01-19 23:00:00] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:00:00] debug: 	zh:deconz: resolve request (19)
[2025-01-19 23:00:00] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 139
[2025-01-19 23:00:00] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:00:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:03] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (16) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
[2025-01-19 23:00:03] error: 	z2m: Publish 'set' 'state' to 'Flurlicht' failed: 'Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (16) Error: waiting for response TIMEOUT)'
[2025-01-19 23:00:03] debug: 	z2m: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (16) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
[2025-01-19 23:00:04] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (17) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 23:00:04] error: 	z2m: Publish 'set' 'state' to 'Flurlicht' failed: 'Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (17) Error: waiting for response TIMEOUT)'
[2025-01-19 23:00:04] debug: 	z2m: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (17) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 23:00:06] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:00:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:06] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:00:06] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 140
[2025-01-19 23:00:06] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 140 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:00:06] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:00:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:06] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:00:06] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:00:06] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:00:06] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:00:06] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:00:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:06] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:00:06] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 141
[2025-01-19 23:00:06] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 141 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 23:00:06] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 23:00:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:06] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:00:06] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 23:00:06] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 23:00:06] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 23:00:08] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:00:08] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:00:08] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 142 request id: 35
[2025-01-19 23:00:08] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 35 status: 0
[2025-01-19 23:00:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:08] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:08] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:08] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 143
[2025-01-19 23:00:08] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 35 confirm status: 0
[2025-01-19 23:00:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:08] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 20
[2025-01-19 23:00:08] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:00:08] debug: 	zh:deconz: resolve request (20)
[2025-01-19 23:00:08] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 23:00:08] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:00:08] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 144 request id: 36
[2025-01-19 23:00:08] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 36 status: 0
[2025-01-19 23:00:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:10] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 145
[2025-01-19 23:00:10] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:00:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:11] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (19) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:00:11] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (19) Error: waiting for response TIMEOUT))
[2025-01-19 23:00:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 146
[2025-01-19 23:00:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 36 confirm status: 0
[2025-01-19 23:00:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 21
[2025-01-19 23:00:18] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:00:18] debug: 	zh:deconz: resolve request (21)
[2025-01-19 23:00:19] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (21) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:00:19] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (20) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:00:19] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (21) Error: waiting for response TIMEOUT))
[2025-01-19 23:00:19] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (20) Error: waiting for response TIMEOUT))
[2025-01-19 23:00:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 147
[2025-01-19 23:00:20] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:00:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:23] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:00:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:23] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:00:23] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 148
[2025-01-19 23:00:23] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 148 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:00:23] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:00:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:23] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:00:23] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:00:23] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:00:23] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:00:24] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:00:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:24] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:00:24] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 149
[2025-01-19 23:00:24] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 149 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:00:24] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 23:00:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:24] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:00:24] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 23:00:24] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 23:00:24] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 23:00:25] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:00:25] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:00:25] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 150 request id: 37
[2025-01-19 23:00:25] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 37 status: 0
[2025-01-19 23:00:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:25] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:25] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:25] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 151
[2025-01-19 23:00:25] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 37 confirm status: 0
[2025-01-19 23:00:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:25] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 22
[2025-01-19 23:00:25] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:00:25] debug: 	zh:deconz: resolve request (22)
[2025-01-19 23:00:26] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 23:00:26] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:00:26] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 152 request id: 38
[2025-01-19 23:00:26] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 38 status: 0
[2025-01-19 23:00:26] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:30] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Lichtschlauch/get' with data '{"state":""}'
[2025-01-19 23:00:30] debug: 	z2m: Publishing get 'get' 'state' to 'Lichtschlauch'
[2025-01-19 23:00:30] debug: 	zh:controller:endpoint: ZCL command 0x00212effff0cb8b6/10 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:00:30] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x2c6e EP:10 SeqNr. 153 request id: 39
[2025-01-19 23:00:30] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 39 status: 0
[2025-01-19 23:00:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:30] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 154
[2025-01-19 23:00:30] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:00:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:31] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Lichtschlauch/set' with data '{"state":"ON"}'
[2025-01-19 23:00:31] debug: 	z2m: Publishing 'set' 'state' to 'Lichtschlauch'
[2025-01-19 23:00:31] debug: 	zh:controller:endpoint: ZCL command 0x00212effff0cb8b6/10 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:00:31] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x2c6e EP:10 SeqNr. 155 request id: 40
[2025-01-19 23:00:31] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 40 status: 0
[2025-01-19 23:00:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:31] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:31] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:31] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 156
[2025-01-19 23:00:31] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x2c6e request id: 40 confirm status: 0
[2025-01-19 23:00:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:31] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 25
[2025-01-19 23:00:31] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:00:31] debug: 	zh:deconz: resolve request (25)
[2025-01-19 23:00:32] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:00:32] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:32] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:00:32] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 157
[2025-01-19 23:00:32] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 157 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:00:32] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:00:32] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:32] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:00:32] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:00:32] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:00:32] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:00:33] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:00:33] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:33] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:00:33] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 158
[2025-01-19 23:00:33] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 158 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:00:33] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:00:33] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:33] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:00:33] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:00:33] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:00:33] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:00:34] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:00:34] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:34] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:00:34] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 159
[2025-01-19 23:00:34] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 159 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:00:34] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:00:34] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:34] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:00:34] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:00:34] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:00:34] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:00:35] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Lichtschlauch/set' with data '{"state":"OFF"}'
[2025-01-19 23:00:35] debug: 	z2m: Publishing 'set' 'state' to 'Lichtschlauch'
[2025-01-19 23:00:35] debug: 	zh:controller:endpoint: ZCL command 0x00212effff0cb8b6/10 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:00:35] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x2c6e EP:10 SeqNr. 160 request id: 41
[2025-01-19 23:00:35] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 41 status: 0
[2025-01-19 23:00:35] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:35] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:35] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:35] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:35] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 161
[2025-01-19 23:00:35] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x2c6e request id: 41 confirm status: 0
[2025-01-19 23:00:35] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:35] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 26
[2025-01-19 23:00:35] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:00:35] debug: 	zh:deconz: resolve request (26)
[2025-01-19 23:00:36] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:00:36] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:00:36] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 162 request id: 42
[2025-01-19 23:00:36] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (22) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:00:36] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (22) Error: waiting for response TIMEOUT))
[2025-01-19 23:00:36] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 42 status: 0
[2025-01-19 23:00:36] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:36] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:36] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:36] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:36] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 163
[2025-01-19 23:00:36] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 42 confirm status: 0
[2025-01-19 23:00:36] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:36] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 27
[2025-01-19 23:00:36] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:00:36] debug: 	zh:deconz: resolve request (27)
[2025-01-19 23:00:37] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:37] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:37] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:37] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 164
[2025-01-19 23:00:37] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 38 confirm status: 0
[2025-01-19 23:00:37] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:37] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 23
[2025-01-19 23:00:37] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:00:37] debug: 	zh:deconz: resolve request (23)
[2025-01-19 23:00:37] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (23) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:00:37] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (23) Error: waiting for response TIMEOUT))
[2025-01-19 23:00:39] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:39] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:39] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 165
[2025-01-19 23:00:39] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x2c6e request id: 39 confirm status: 0
[2025-01-19 23:00:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:39] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 24
[2025-01-19 23:00:39] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:00:39] debug: 	zh:deconz: resolve request (24)
[2025-01-19 23:00:40] debug: 	zh:controller:endpoint: Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (24) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:276:21)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 23:00:40] error: 	z2m: Publish 'get' 'state' to 'Lichtschlauch' failed: 'Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (24) Error: waiting for response TIMEOUT)'
[2025-01-19 23:00:40] debug: 	z2m: Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (24) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:276:21)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 23:00:40] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 166
[2025-01-19 23:00:40] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:00:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:42] debug: 	zh:controller:endpoint: Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (25) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 23:00:42] error: 	z2m: Publish 'set' 'state' to 'Lichtschlauch' failed: 'Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (25) Error: waiting for response TIMEOUT)'
[2025-01-19 23:00:42] debug: 	z2m: Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (25) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 23:00:45] debug: 	zh:controller:endpoint: Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (26) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 23:00:45] error: 	z2m: Publish 'set' 'state' to 'Lichtschlauch' failed: 'Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (26) Error: waiting for response TIMEOUT)'
[2025-01-19 23:00:45] debug: 	z2m: Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (26) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 23:00:46] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (27) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:00:46] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (27) Error: waiting for response TIMEOUT))
[2025-01-19 23:00:46] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Lichtschlauch/set' with data '{"state":"ON"}'
[2025-01-19 23:00:46] debug: 	z2m: Publishing 'set' 'state' to 'Lichtschlauch'
[2025-01-19 23:00:46] debug: 	zh:controller:endpoint: ZCL command 0x00212effff0cb8b6/10 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:00:46] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x2c6e EP:10 SeqNr. 167 request id: 43
[2025-01-19 23:00:46] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 43 status: 0
[2025-01-19 23:00:46] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:47] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:00:47] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:47] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:00:47] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 168
[2025-01-19 23:00:47] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 168 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 159
[2025-01-19 23:00:47] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:00:47] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:47] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:00:47] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:00:47] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:00:47] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:00:47] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:00:47] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:47] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:00:47] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 169
[2025-01-19 23:00:47] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 169 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 23:00:47] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 23:00:47] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:47] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:00:47] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 23:00:47] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 23:00:47] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 23:00:48] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:00:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:48] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:00:48] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 170
[2025-01-19 23:00:48] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 170 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 159
[2025-01-19 23:00:48] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:00:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:48] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:00:48] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:00:48] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:00:48] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:00:48] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Lichtschlauch/set' with data '{"state":"OFF"}'
[2025-01-19 23:00:48] debug: 	z2m: Publishing 'set' 'state' to 'Lichtschlauch'
[2025-01-19 23:00:48] debug: 	zh:controller:endpoint: ZCL command 0x00212effff0cb8b6/10 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:00:48] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x2c6e EP:10 SeqNr. 171 request id: 44
[2025-01-19 23:00:48] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 44 status: 0
[2025-01-19 23:00:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:48] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:48] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:48] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 172
[2025-01-19 23:00:48] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x2c6e request id: 44 confirm status: 0
[2025-01-19 23:00:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:48] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 29
[2025-01-19 23:00:48] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:00:48] debug: 	zh:deconz: resolve request (29)
[2025-01-19 23:00:49] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 23:00:49] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:00:49] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 173 request id: 45
[2025-01-19 23:00:49] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 45 status: 0
[2025-01-19 23:00:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:50] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:00:50] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 174 request id: 46
[2025-01-19 23:00:50] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 46 status: 0
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:50] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 175
[2025-01-19 23:00:50] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 46 confirm status: 0
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:50] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 31
[2025-01-19 23:00:50] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:00:50] debug: 	zh:deconz: resolve request (31)
[2025-01-19 23:00:50] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 176
[2025-01-19 23:00:50] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 176 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 167
[2025-01-19 23:00:50] debug: 	zh:deconz:frameparser: response payload: 081f010000001000
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:50] debug: 	zh:controller: Received payload: clusterID=6, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=167, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":31,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":16,"attrData":0}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:00:50] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":31,"writeUndiv":false})
[2025-01-19 23:00:50] debug: 	zh:deconz: no response expected (31)
[2025-01-19 23:00:50] debug: 	zh:deconz: response received (31)
[2025-01-19 23:00:50] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genOnOff', data '{"onOff":0}' from endpoint 1 with groupID 0
[2025-01-19 23:00:50] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":167,"state":"OFF","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 177 request id: 47
[2025-01-19 23:00:50] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 47 status: 0
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:50] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 178
[2025-01-19 23:00:50] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 47 confirm status: 0
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:50] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 31
[2025-01-19 23:00:50] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:00:50] debug: 	zh:deconz: resolve request (31)
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 179
[2025-01-19 23:00:50] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:00:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:56] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:56] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:56] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 180
[2025-01-19 23:00:56] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x2c6e request id: 43 confirm status: 0
[2025-01-19 23:00:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:56] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 28
[2025-01-19 23:00:56] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:00:56] debug: 	zh:deconz: resolve request (28)
[2025-01-19 23:00:57] debug: 	zh:controller:endpoint: Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (28) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 23:00:57] error: 	z2m: Publish 'set' 'state' to 'Lichtschlauch' failed: 'Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (28) Error: waiting for response TIMEOUT)'
[2025-01-19 23:00:57] debug: 	z2m: Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (28) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 23:00:59] debug: 	zh:controller:endpoint: Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (29) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
[2025-01-19 23:00:59] error: 	z2m: Publish 'set' 'state' to 'Lichtschlauch' failed: 'Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (29) Error: waiting for response TIMEOUT)'
[2025-01-19 23:00:59] debug: 	z2m: Error: ZCL command 0x00212effff0cb8b6/10 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (29) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.command (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:721:23)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:48:17)
    at Object.convertSet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1160:33)
    at Publish.onMQTTMessage (/app/lib/extension/publish.ts:250:36)
[2025-01-19 23:00:59] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:00:59] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:59] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:00:59] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 181
[2025-01-19 23:00:59] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 45 confirm status: 0
[2025-01-19 23:00:59] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:00:59] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 30
[2025-01-19 23:00:59] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:00:59] debug: 	zh:deconz: resolve request (30)
[2025-01-19 23:01:00] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (30) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:01:00] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (30) Error: waiting for response TIMEOUT))
[2025-01-19 23:01:00] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 182
[2025-01-19 23:01:00] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:01:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:10] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 183
[2025-01-19 23:01:10] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:01:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:17] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/bridge/request/device/interview' with data '{"id":"Bogenlampe","transaction":"g1g21-1"}'
[2025-01-19 23:01:17] info: 	z2m: Interviewing 'Bogenlampe'
[2025-01-19 23:01:17] debug: 	zh:controller:device: Interview - start device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:0 SeqNr. 184 request id: 48
[2025-01-19 23:01:17] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 48 status: 0
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:17] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 185
[2025-01-19 23:01:17] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 48 confirm status: 0
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:17] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 186
[2025-01-19 23:01:17] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 186 srcAddr: 0x45e destAddr: 0x0 profile id: 0x0 cluster id: 0x8002 lqi: 159
[2025-01-19 23:01:17] debug: 	zh:deconz:frameparser: response payload: 30005e0401408e8911525200002c520000
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:17] debug: 	zh:controller: Received ZDO response: clusterId=NODE_DESCRIPTOR_RESPONSE, status=SUCCESS, payload={"nwkAddress":1118,"logicalType":1,"apsFlags":0,"frequencyBand":8,"capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1},"manufacturerCode":4489,"maxBufSize":82,"maxIncTxSize":82,"serverMask":{"primaryTrustCenter":0,"backupTrustCenter":0,"deprecated1":0,"deprecated2":0,"deprecated3":0,"deprecated4":0,"networkManager":0,"reserved1":0,"reserved2":0,"stackComplianceRevision":22},"maxOutTxSize":82,"deprecated1":0,"tlvs":[]}
[2025-01-19 23:01:17] debug: 	zh:controller:device: Interview - got node descriptor for device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:0 SeqNr. 187 request id: 49
[2025-01-19 23:01:17] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 49 status: 0
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:17] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:17] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 188
[2025-01-19 23:01:17] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 49 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 189
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 189 srcAddr: 0x45e destAddr: 0x0 profile id: 0x0 cluster id: 0x8005 lqi: 159
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: response payload: 31005e040201f2
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:controller: Received ZDO response: clusterId=ACTIVE_ENDPOINTS_RESPONSE, status=SUCCESS, payload={"nwkAddress":1118,"endpointList":[1,242]}
[2025-01-19 23:01:18] debug: 	zh:controller:device: Interview - got active endpoints for device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:0 SeqNr. 190 request id: 50
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 50 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 191
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 50 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 192
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 192 srcAddr: 0x45e destAddr: 0x0 profile id: 0x0 cluster id: 0x8004 lqi: 159
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: response payload: 32005e041a0104010d0101080000030004000500060008000003050b011900
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:controller: Received ZDO response: clusterId=SIMPLE_DESCRIPTOR_RESPONSE, status=SUCCESS, payload={"nwkAddress":1118,"length":26,"endpoint":1,"profileId":260,"deviceId":269,"deviceVersion":1,"inClusterList":[0,3,4,5,6,8,768,2821],"outClusterList":[25]}
[2025-01-19 23:01:18] debug: 	zh:controller:device: Interview - got simple descriptor for endpoint '1' device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.read(["modelId"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false,"sendPolicy":"immediate"})
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 193 request id: 51
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 51 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 194
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 51 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 32
[2025-01-19 23:01:18] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:01:18] debug: 	zh:deconz: resolve request (32)
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 195
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 195 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x0 lqi: 159
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: response payload: 0820010500004209413630532052474257
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:controller: Received payload: clusterID=0, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=159, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":32,"commandIdentifier":1},"payload":[{"attrId":5,"status":0,"dataType":66,"attrData":"A60S RGBW"}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:01:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":32,"writeUndiv":false})
[2025-01-19 23:01:18] debug: 	zh:deconz: no response expected (32)
[2025-01-19 23:01:18] debug: 	zh:deconz: response received (32)
[2025-01-19 23:01:18] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genBasic', data '{"modelId":"A60S RGBW"}' from endpoint 1 with groupID 0
[2025-01-19 23:01:18] debug: 	z2m: Skipping message, still interviewing
[2025-01-19 23:01:18] debug: 	zh:controller:device: Interview - got 'modelID' for device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.read(["manufacturerName"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false,"sendPolicy":"immediate"})
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 196 request id: 52
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 52 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 197 request id: 53
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 53 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 198
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 52 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 32
[2025-01-19 23:01:18] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:01:18] debug: 	zh:deconz: resolve request (32)
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 199
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 53 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 33
[2025-01-19 23:01:18] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:01:18] debug: 	zh:deconz: resolve request (33)
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 200
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 200 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x0 lqi: 159
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: response payload: 08210104000042084c454456414e4345
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:controller: Received payload: clusterID=0, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=159, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":33,"commandIdentifier":1},"payload":[{"attrId":4,"status":0,"dataType":66,"attrData":"LEDVANCE"}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:01:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":33,"writeUndiv":false})
[2025-01-19 23:01:18] debug: 	zh:deconz: no response expected (33)
[2025-01-19 23:01:18] debug: 	zh:deconz: response received (33)
[2025-01-19 23:01:18] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genBasic', data '{"manufacturerName":"LEDVANCE"}' from endpoint 1 with groupID 0
[2025-01-19 23:01:18] debug: 	z2m: Skipping message, still interviewing
[2025-01-19 23:01:18] debug: 	zh:controller:device: Interview - got 'manufacturerName' for device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.read(["powerSource"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false,"sendPolicy":"immediate"})
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 201 request id: 54
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 54 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 202 request id: 55
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 55 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 203
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 54 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 33
[2025-01-19 23:01:18] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:01:18] debug: 	zh:deconz: resolve request (33)
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 204
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 55 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 34
[2025-01-19 23:01:18] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:01:18] debug: 	zh:deconz: resolve request (34)
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 205
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 206
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 206 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x0 lqi: 151
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: response payload: 0822010700003000
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:controller: Received payload: clusterID=0, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=151, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":34,"commandIdentifier":1},"payload":[{"attrId":7,"status":0,"dataType":48,"attrData":0}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:01:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":34,"writeUndiv":false})
[2025-01-19 23:01:18] debug: 	zh:deconz: no response expected (34)
[2025-01-19 23:01:18] debug: 	zh:deconz: response received (34)
[2025-01-19 23:01:18] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genBasic', data '{"powerSource":0}' from endpoint 1 with groupID 0
[2025-01-19 23:01:18] debug: 	z2m: Skipping message, still interviewing
[2025-01-19 23:01:18] debug: 	zh:controller:device: Interview - got 'powerSource' for device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.read(["zclVersion"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false,"sendPolicy":"immediate"})
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 207 request id: 56
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 56 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 208 request id: 57
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 57 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 209
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 56 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 34
[2025-01-19 23:01:18] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:01:18] debug: 	zh:deconz: resolve request (34)
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 210
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 57 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 35
[2025-01-19 23:01:18] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:01:18] debug: 	zh:deconz: resolve request (35)
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 211
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 211 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x0 lqi: 159
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: response payload: 0823010000002008
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:controller: Received payload: clusterID=0, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=159, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":35,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":8}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:01:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":35,"writeUndiv":false})
[2025-01-19 23:01:18] debug: 	zh:deconz: no response expected (35)
[2025-01-19 23:01:18] debug: 	zh:deconz: response received (35)
[2025-01-19 23:01:18] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genBasic', data '{"zclVersion":8}' from endpoint 1 with groupID 0
[2025-01-19 23:01:18] debug: 	z2m: Skipping message, still interviewing
[2025-01-19 23:01:18] debug: 	zh:controller:device: Interview - got 'zclVersion' for device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.read(["appVersion"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false,"sendPolicy":"immediate"})
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 212 request id: 58
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 58 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 213 request id: 59
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 59 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 214
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 58 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 35
[2025-01-19 23:01:18] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:01:18] debug: 	zh:deconz: resolve request (35)
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 215
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 59 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 36
[2025-01-19 23:01:18] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:01:18] debug: 	zh:deconz: resolve request (36)
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 216
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 216 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x0 lqi: 159
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: response payload: 0824010100002000
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:controller: Received payload: clusterID=0, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=159, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":36,"commandIdentifier":1},"payload":[{"attrId":1,"status":0,"dataType":32,"attrData":0}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:01:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":36,"writeUndiv":false})
[2025-01-19 23:01:18] debug: 	zh:deconz: no response expected (36)
[2025-01-19 23:01:18] debug: 	zh:deconz: response received (36)
[2025-01-19 23:01:18] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genBasic', data '{"appVersion":0}' from endpoint 1 with groupID 0
[2025-01-19 23:01:18] debug: 	z2m: Skipping message, still interviewing
[2025-01-19 23:01:18] debug: 	zh:controller:device: Interview - got 'applicationVersion' for device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.read(["stackVersion"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false,"sendPolicy":"immediate"})
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 217 request id: 60
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 60 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 218 request id: 61
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 61 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 219
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 60 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 36
[2025-01-19 23:01:18] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:01:18] debug: 	zh:deconz: resolve request (36)
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 220
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 61 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 37
[2025-01-19 23:01:18] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:01:18] debug: 	zh:deconz: resolve request (37)
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 221
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 222
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 222 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x0 lqi: 159
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: response payload: 0825010200002000
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:controller: Received payload: clusterID=0, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=159, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":37,"commandIdentifier":1},"payload":[{"attrId":2,"status":0,"dataType":32,"attrData":0}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:01:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":37,"writeUndiv":false})
[2025-01-19 23:01:18] debug: 	zh:deconz: no response expected (37)
[2025-01-19 23:01:18] debug: 	zh:deconz: response received (37)
[2025-01-19 23:01:18] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genBasic', data '{"stackVersion":0}' from endpoint 1 with groupID 0
[2025-01-19 23:01:18] debug: 	z2m: Skipping message, still interviewing
[2025-01-19 23:01:18] debug: 	zh:controller:device: Interview - got 'stackVersion' for device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.read(["hwVersion"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false,"sendPolicy":"immediate"})
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 223 request id: 62
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 62 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 224 request id: 63
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 63 status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 225
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 62 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 37
[2025-01-19 23:01:18] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:01:18] debug: 	zh:deconz: resolve request (37)
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 226
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 63 confirm status: 0
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 38
[2025-01-19 23:01:18] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:01:18] debug: 	zh:deconz: resolve request (38)
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 227
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 227 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 159
[2025-01-19 23:01:18] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:01:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:18] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:01:18] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:01:18] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:01:19] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:01:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 228
[2025-01-19 23:01:20] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:01:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:21] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:01:21] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:01:21] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 229 request id: 64
[2025-01-19 23:01:21] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 64 status: 0
[2025-01-19 23:01:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:21] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:21] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:21] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 230
[2025-01-19 23:01:21] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 64 confirm status: 0
[2025-01-19 23:01:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:21] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 39
[2025-01-19 23:01:21] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:01:21] debug: 	zh:deconz: resolve request (39)
[2025-01-19 23:01:29] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genBasic.read(["hwVersion"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false,"sendPolicy":"immediate"}) failed (no response received (38) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Device.interviewInternal (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/device.ts:933:42)
    at Device.interview (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/device.ts:750:13)
    at Bridge.deviceInterview (/app/lib/extension/bridge.ts:517:13)
    at Bridge.onMQTTMessage (/app/lib/extension/bridge.ts:205:34)
    at EventEmitter.wrappedCallback (/app/lib/eventBus.ts:204:17)
[2025-01-19 23:01:29] debug: 	zh:controller:device: Interview - failed to read attribute 'hardwareVersion' from endpoint '1' (Error: ZCL command 0xf0d1b800001ffcf2/1 genBasic.read(["hwVersion"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false,"sendPolicy":"immediate"}) failed (no response received (38) Error: waiting for response TIMEOUT))
[2025-01-19 23:01:29] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.read(["dateCode"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false,"sendPolicy":"immediate"})
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 231 request id: 65
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 65 status: 0
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 232
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 65 confirm status: 0
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 40
[2025-01-19 23:01:29] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:01:29] debug: 	zh:deconz: resolve request (40)
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 233
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 233 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x0 lqi: 159
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: response payload: 08280106000042083230323430353233
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:controller: Received payload: clusterID=0, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=159, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":40,"commandIdentifier":1},"payload":[{"attrId":6,"status":0,"dataType":66,"attrData":"20240523"}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:01:29] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":40,"writeUndiv":false})
[2025-01-19 23:01:29] debug: 	zh:deconz: no response expected (40)
[2025-01-19 23:01:29] debug: 	zh:deconz: response received (40)
[2025-01-19 23:01:29] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genBasic', data '{"dateCode":"20240523"}' from endpoint 1 with groupID 0
[2025-01-19 23:01:29] debug: 	z2m: Skipping message, still interviewing
[2025-01-19 23:01:29] debug: 	zh:controller:device: Interview - got 'dateCode' for device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:29] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.read(["swBuildId"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false,"sendPolicy":"immediate"})
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 234 request id: 66
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 66 status: 0
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 235 request id: 67
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 67 status: 0
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 236
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 66 confirm status: 0
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 40
[2025-01-19 23:01:29] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:01:29] debug: 	zh:deconz: resolve request (40)
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 237
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 67 confirm status: 0
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 41
[2025-01-19 23:01:29] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:01:29] debug: 	zh:deconz: resolve request (41)
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 238
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 239
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 239 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x0 lqi: 159
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: response payload: 08290100400042083033313937333130
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:controller: Received payload: clusterID=0, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=159, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":41,"commandIdentifier":1},"payload":[{"attrId":16384,"status":0,"dataType":66,"attrData":"03197310"}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:01:29] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genBasic.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":41,"writeUndiv":false})
[2025-01-19 23:01:29] debug: 	zh:deconz: no response expected (41)
[2025-01-19 23:01:29] debug: 	zh:deconz: response received (41)
[2025-01-19 23:01:29] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genBasic', data '{"swBuildId":"03197310"}' from endpoint 1 with groupID 0
[2025-01-19 23:01:29] debug: 	z2m: Skipping message, still interviewing
[2025-01-19 23:01:29] debug: 	zh:controller:device: Interview - got 'softwareBuildID' for device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 240 request id: 68
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:0 SeqNr. 241 request id: 69
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 68 status: 0
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 69 status: 0
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 242
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 68 confirm status: 0
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 41
[2025-01-19 23:01:29] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:01:29] debug: 	zh:deconz: resolve request (41)
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 243
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 69 confirm status: 0
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 244
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 244 srcAddr: 0x45e destAddr: 0x0 profile id: 0x0 cluster id: 0x8004 lqi: 159
[2025-01-19 23:01:29] debug: 	zh:deconz:frameparser: response payload: 45005e040af2e0a161000100012100
[2025-01-19 23:01:29] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:29] debug: 	zh:controller: Received ZDO response: clusterId=SIMPLE_DESCRIPTOR_RESPONSE, status=SUCCESS, payload={"nwkAddress":1118,"length":10,"endpoint":242,"profileId":41440,"deviceId":97,"deviceVersion":1,"inClusterList":[],"outClusterList":[33]}
[2025-01-19 23:01:29] debug: 	zh:controller:device: Interview - got simple descriptor for endpoint '242' device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:29] debug: 	zh:controller:device: Interview - completed for device '0xf0d1b800001ffcf2'
[2025-01-19 23:01:29] debug: 	zh:controller:database: Writing database to '/app/data/database.db'
[2025-01-19 23:01:30] info: 	z2m: Successfully interviewed 'Bogenlampe'
[2025-01-19 23:01:30] debug: 	z2m: Skipping discovery of 'light/0xf0d1b800001ffcf2/light/config', already discovered
[2025-01-19 23:01:30] debug: 	z2m: Skipping discovery of 'select/0xf0d1b800001ffcf2/effect/config', already discovered
[2025-01-19 23:01:30] debug: 	z2m: Skipping discovery of 'sensor/0xf0d1b800001ffcf2/linkquality/config', already discovered
[2025-01-19 23:01:30] debug: 	z2m: Skipping discovery of 'update/0xf0d1b800001ffcf2/update/config', already discovered
[2025-01-19 23:01:30] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/response/device/interview', payload '{"data":{"id":"Bogenlampe"},"status":"ok","transaction":"g1g21-1"}'
[2025-01-19 23:01:30] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 245
[2025-01-19 23:01:30] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:01:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:31] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (39) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:01:31] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (39) Error: waiting for response TIMEOUT))
[2025-01-19 23:01:40] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 246
[2025-01-19 23:01:40] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:01:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:50] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 247
[2025-01-19 23:01:50] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:01:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:53] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:53] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:53] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 248
[2025-01-19 23:01:53] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 248 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 23:01:53] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 23:01:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:53] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:01:53] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 23:01:53] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 23:01:53] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 23:01:53] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:01:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:53] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:01:53] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 249
[2025-01-19 23:01:53] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 249 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 159
[2025-01-19 23:01:53] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:01:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:53] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:01:53] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:01:53] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:01:53] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:01:55] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 23:01:55] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:01:55] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 250 request id: 70
[2025-01-19 23:01:55] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 70 status: 0
[2025-01-19 23:01:55] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:55] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:55] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:55] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:55] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 251
[2025-01-19 23:01:55] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 70 confirm status: 0
[2025-01-19 23:01:55] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:55] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 42
[2025-01-19 23:01:55] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:01:55] debug: 	zh:deconz: resolve request (42)
[2025-01-19 23:01:55] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:01:55] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:01:55] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 252 request id: 71
[2025-01-19 23:01:55] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 71 status: 0
[2025-01-19 23:01:55] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:55] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:01:55] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:56] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:01:56] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 253
[2025-01-19 23:01:56] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 71 confirm status: 0
[2025-01-19 23:01:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:01:56] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 43
[2025-01-19 23:01:56] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:01:56] debug: 	zh:deconz: resolve request (43)
[2025-01-19 23:02:00] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 254
[2025-01-19 23:02:00] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:02:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:02:01] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/bridge/request/device/interview' with data '{"id":"Medienschrank Wohnzimmer","transaction":"g1g21-2"}'
[2025-01-19 23:02:01] info: 	z2m: Interviewing 'Medienschrank Wohnzimmer'
[2025-01-19 23:02:01] debug: 	zh:controller:device: Interview - start device '0xa4c13838ba59a1b2'
[2025-01-19 23:02:02] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:0 SeqNr. 1 request id: 72
[2025-01-19 23:02:02] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 72 status: 0
[2025-01-19 23:02:02] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:02:02] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:02:02] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:02:02] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:02:02] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 2
[2025-01-19 23:02:02] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 72 confirm status: 0
[2025-01-19 23:02:02] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:02:05] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (42) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:02:05] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (42) Error: waiting for response TIMEOUT))
[2025-01-19 23:02:06] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (43) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:02:06] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (43) Error: waiting for response TIMEOUT))
[2025-01-19 23:02:10] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 3
[2025-01-19 23:02:10] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:02:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:02:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 4
[2025-01-19 23:02:20] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:02:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:02:30] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 5
[2025-01-19 23:02:30] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:02:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:02:40] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 6
[2025-01-19 23:02:40] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:02:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:02:50] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 7
[2025-01-19 23:02:50] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:02:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:02:58] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/bridge/request/networkmap' with data '{"routes":false,"transaction":"g1g21-3","type":"raw"}'
[2025-01-19 23:02:58] info: 	z2m: Starting network scan (includeRoutes 'false')
[2025-01-19 23:02:59] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x0 EP:0 SeqNr. 8 request id: 73
[2025-01-19 23:02:59] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 73 status: 0
[2025-01-19 23:02:59] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:02:59] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101110
[2025-01-19 23:02:59] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:02:59] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:02:59] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 9
[2025-01-19 23:02:59] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:02:59] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x0 request id: 73 confirm status: 0
[2025-01-19 23:02:59] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:02:59] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:02:59] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 10
[2025-01-19 23:02:59] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 10 srcAddr: 0x0 destAddr: 0x0 profile id: 0x0 cluster id: 0x8031 lqi: 213
[2025-01-19 23:02:59] debug: 	zh:deconz:frameparser: response payload: 4900020002ddddddddddddddddf2fc1f0000b8d1f05e04250101a4ddddddddddddddddb6b80cffff2e21006e2c250101fc
[2025-01-19 23:02:59] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:02:59] debug: 	zh:controller: Received ZDO response: clusterId=LQI_TABLE_RESPONSE, status=SUCCESS, payload={"neighborTableEntries":2,"startIndex":0,"entryList":[{"extendedPanId":[221,221,221,221,221,221,221,221],"eui64":"0xf0d1b800001ffcf2","nwkAddress":1118,"deviceType":1,"rxOnWhenIdle":1,"relationship":2,"reserved1":0,"permitJoining":1,"reserved2":0,"depth":1,"lqi":164},{"extendedPanId":[221,221,221,221,221,221,221,221],"eui64":"0x00212effff0cb8b6","nwkAddress":11374,"deviceType":1,"rxOnWhenIdle":1,"relationship":2,"reserved1":0,"permitJoining":1,"reserved2":0,"depth":1,"lqi":252}]}
[2025-01-19 23:02:59] debug: 	z2m: LQI succeeded for 'Coordinator'
[2025-01-19 23:02:59] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 11
[2025-01-19 23:03:00] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 12
[2025-01-19 23:03:00] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:03:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:00] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:0 SeqNr. 13 request id: 74
[2025-01-19 23:03:00] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 74 status: 0
[2025-01-19 23:03:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:00] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:03:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:00] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:03:00] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 14
[2025-01-19 23:03:00] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 74 confirm status: 0
[2025-01-19 23:03:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:00] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:03:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:00] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:03:00] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 15
[2025-01-19 23:03:00] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 15 srcAddr: 0x45e destAddr: 0x0 profile id: 0x0 cluster id: 0x8031 lqi: 167
[2025-01-19 23:03:00] debug: 	zh:deconz:frameparser: response payload: 4a00030003dddddddddddddddd2cfc04ffff2e2100000004020091ddddddddddddddddb6b80cffff2e21006e2c25020fa7ddddddddddddddddbefde260ef38c1a424b012000200
[2025-01-19 23:03:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:00] debug: 	zh:controller: Received ZDO response: clusterId=LQI_TABLE_RESPONSE, status=SUCCESS, payload={"neighborTableEntries":3,"startIndex":0,"entryList":[{"extendedPanId":[221,221,221,221,221,221,221,221],"eui64":"0x00212effff04fc2c","nwkAddress":0,"deviceType":0,"rxOnWhenIdle":1,"relationship":0,"reserved1":0,"permitJoining":2,"reserved2":0,"depth":0,"lqi":145},{"extendedPanId":[221,221,221,221,221,221,221,221],"eui64":"0x00212effff0cb8b6","nwkAddress":11374,"deviceType":1,"rxOnWhenIdle":1,"relationship":2,"reserved1":0,"permitJoining":2,"reserved2":0,"depth":15,"lqi":167},{"extendedPanId":[221,221,221,221,221,221,221,221],"eui64":"0xa4c138ef60e2fdbe","nwkAddress":45092,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"reserved1":0,"permitJoining":0,"reserved2":0,"depth":2,"lqi":0}]}
[2025-01-19 23:03:00] debug: 	z2m: LQI succeeded for 'Bogenlampe'
[2025-01-19 23:03:01] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x2c6e EP:0 SeqNr. 16 request id: 75
[2025-01-19 23:03:01] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 75 status: 0
[2025-01-19 23:03:01] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:02] debug: 	zh:controller:device: Interview - quirks check for 'TS0601'-'_TZE200_a8sdabtg'-'EndDevice'
[2025-01-19 23:03:02] debug: 	zh:controller:device: Interview - quirks matched for Tuya end device
[2025-01-19 23:03:02] debug: 	zh:controller:device: Interview - completed for device '0xa4c13838ba59a1b2' because of quirks ('Error: waiting for response TIMEOUT')
[2025-01-19 23:03:02] debug: 	zh:controller:device: Interview - completed for device '0xa4c13838ba59a1b2'
[2025-01-19 23:03:02] debug: 	zh:controller:database: Writing database to '/app/data/database.db'
[2025-01-19 23:03:02] info: 	z2m: Successfully interviewed 'Medienschrank Wohnzimmer'
[2025-01-19 23:03:02] debug: 	z2m: Skipping discovery of 'sensor/0xa4c13838ba59a1b2/temperature/config', already discovered
[2025-01-19 23:03:02] debug: 	z2m: Skipping discovery of 'sensor/0xa4c13838ba59a1b2/humidity/config', already discovered
[2025-01-19 23:03:02] debug: 	z2m: Skipping discovery of 'select/0xa4c13838ba59a1b2/temperature_unit/config', already discovered
[2025-01-19 23:03:02] debug: 	z2m: Skipping discovery of 'number/0xa4c13838ba59a1b2/temperature_calibration/config', already discovered
[2025-01-19 23:03:02] debug: 	z2m: Skipping discovery of 'number/0xa4c13838ba59a1b2/humidity_calibration/config', already discovered
[2025-01-19 23:03:02] debug: 	z2m: Skipping discovery of 'sensor/0xa4c13838ba59a1b2/battery/config', already discovered
[2025-01-19 23:03:02] debug: 	z2m: Skipping discovery of 'sensor/0xa4c13838ba59a1b2/linkquality/config', already discovered
[2025-01-19 23:03:02] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/response/device/interview', payload '{"data":{"id":"Medienschrank Wohnzimmer"},"status":"ok","transaction":"g1g21-2"}'
[2025-01-19 23:03:04] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:03:04] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:04] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:03:04] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 17
[2025-01-19 23:03:04] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 17 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:03:04] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:03:04] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:04] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:03:04] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:03:04] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:03:04] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:03:05] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:03:05] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:05] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:03:05] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 18
[2025-01-19 23:03:05] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 18 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:03:05] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:03:05] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:05] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:03:05] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:03:05] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:03:05] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:03:07] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:03:07] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:03:07] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 19 request id: 76
[2025-01-19 23:03:07] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 76 status: 0
[2025-01-19 23:03:07] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:07] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:03:07] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:07] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:03:07] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 20
[2025-01-19 23:03:07] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 76 confirm status: 0
[2025-01-19 23:03:07] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:07] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 44
[2025-01-19 23:03:07] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:03:07] debug: 	zh:deconz: resolve request (44)
[2025-01-19 23:03:09] debug: 	z2m: Saving state to file /app/data/state.json
[2025-01-19 23:03:10] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 21
[2025-01-19 23:03:10] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:03:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:11] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:03:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:11] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:03:11] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 22
[2025-01-19 23:03:11] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x2c6e request id: 75 confirm status: 0
[2025-01-19 23:03:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:18] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (44) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:03:18] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (44) Error: waiting for response TIMEOUT))
[2025-01-19 23:03:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 23
[2025-01-19 23:03:20] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:03:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:30] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 24
[2025-01-19 23:03:30] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:03:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:40] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 25
[2025-01-19 23:03:40] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:03:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:03:50] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 26
[2025-01-19 23:03:50] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:03:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:00] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 27
[2025-01-19 23:04:00] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:04:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:07] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x2c6e EP:0 SeqNr. 28 request id: 77
[2025-01-19 23:04:07] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 77 status: 0
[2025-01-19 23:04:07] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:10] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 29
[2025-01-19 23:04:10] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:04:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:17] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:04:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:17] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:04:17] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 30
[2025-01-19 23:04:17] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x2c6e request id: 77 confirm status: 0
[2025-01-19 23:04:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 31
[2025-01-19 23:04:20] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:04:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:30] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 32
[2025-01-19 23:04:30] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:04:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:40] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 33
[2025-01-19 23:04:40] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:04:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:42] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Bogenlampe/set' with data '{"state":"ON","brightness":105,"color_temp":370}'
[2025-01-19 23:04:42] debug: 	z2m: Publishing 'set' 'brightness' to 'Bogenlampe'
[2025-01-19 23:04:42] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.moveToLevelWithOnOff({"level":105,"transtime":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 34 request id: 78
[2025-01-19 23:04:42] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 78 status: 0
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:42] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 35
[2025-01-19 23:04:42] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 78 confirm status: 0
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:42] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 45
[2025-01-19 23:04:42] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:04:42] debug: 	zh:deconz: resolve request (45)
[2025-01-19 23:04:42] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 36
[2025-01-19 23:04:42] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 36 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 151
[2025-01-19 23:04:42] debug: 	zh:deconz:frameparser: response payload: 082d0b0400
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:42] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=151, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":45,"commandIdentifier":11},"payload":{"cmdId":4,"statusCode":0},"command":{"ID":11,"name":"defaultRsp","parameters":[{"name":"cmdId","type":32},{"name":"statusCode","type":32}]}}
[2025-01-19 23:04:42] debug: 	zh:deconz: response received (45)
[2025-01-19 23:04:42] debug: 	z2m: Publishing 'set' 'color_temp' to 'Bogenlampe'
[2025-01-19 23:04:42] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 lightingColorCtrl.moveToColorTemp({"colortemp":370,"transtime":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 37 request id: 79
[2025-01-19 23:04:42] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 79 status: 0
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:42] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 38
[2025-01-19 23:04:42] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 79 confirm status: 0
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:42] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 46
[2025-01-19 23:04:42] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:04:42] debug: 	zh:deconz: resolve request (46)
[2025-01-19 23:04:42] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 39
[2025-01-19 23:04:42] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 39 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x300 lqi: 151
[2025-01-19 23:04:42] debug: 	zh:deconz:frameparser: response payload: 082e0b0a00
[2025-01-19 23:04:42] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:42] debug: 	zh:controller: Received payload: clusterID=768, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=151, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":46,"commandIdentifier":11},"payload":{"cmdId":10,"statusCode":0},"command":{"ID":11,"name":"defaultRsp","parameters":[{"name":"cmdId","type":32},{"name":"statusCode","type":32}]}}
[2025-01-19 23:04:42] debug: 	zh:deconz: response received (46)
[2025-01-19 23:04:42] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":151,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:04:43] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:04:43] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:43] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:43] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 40
[2025-01-19 23:04:43] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 40 srcAddr: 0xe707 destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 23:04:43] debug: 	zh:deconz:frameparser: response payload: 0007e7bd76010aaa3eb07c8e
[2025-01-19 23:04:43] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:43] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":59143,"eui64":"0x7cb03eaa0a0176bd","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:04:43] debug: 	zh:controller: Device announce from '0x7cb03eaa0a0176bd:59143'
[2025-01-19 23:04:43] debug: 	z2m: Device 'Küchentisch' announced itself
[2025-01-19 23:04:43] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Küchentisch","ieee_address":"0x7cb03eaa0a0176bd"},"type":"device_announce"}'
[2025-01-19 23:04:44] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Bogenlampe/set' with data '{"state":"ON","brightness":105,"color_temp":370}'
[2025-01-19 23:04:44] debug: 	z2m: Publishing 'set' 'brightness' to 'Bogenlampe'
[2025-01-19 23:04:44] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.moveToLevelWithOnOff({"level":105,"transtime":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 41 request id: 80
[2025-01-19 23:04:44] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 80 status: 0
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:44] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 42
[2025-01-19 23:04:44] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 80 confirm status: 0
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:44] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 47
[2025-01-19 23:04:44] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:04:44] debug: 	zh:deconz: resolve request (47)
[2025-01-19 23:04:44] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 43
[2025-01-19 23:04:44] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 43 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 143
[2025-01-19 23:04:44] debug: 	zh:deconz:frameparser: response payload: 082f0b0400
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:44] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=143, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":47,"commandIdentifier":11},"payload":{"cmdId":4,"statusCode":0},"command":{"ID":11,"name":"defaultRsp","parameters":[{"name":"cmdId","type":32},{"name":"statusCode","type":32}]}}
[2025-01-19 23:04:44] debug: 	zh:deconz: response received (47)
[2025-01-19 23:04:44] debug: 	z2m: Publishing 'set' 'color_temp' to 'Bogenlampe'
[2025-01-19 23:04:44] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 lightingColorCtrl.moveToColorTemp({"colortemp":370,"transtime":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 44 request id: 81
[2025-01-19 23:04:44] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 81 status: 0
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:44] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 45
[2025-01-19 23:04:44] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 81 confirm status: 0
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:44] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 48
[2025-01-19 23:04:44] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:04:44] debug: 	zh:deconz: resolve request (48)
[2025-01-19 23:04:44] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 46
[2025-01-19 23:04:44] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 46 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x300 lqi: 151
[2025-01-19 23:04:44] debug: 	zh:deconz:frameparser: response payload: 08300b0a00
[2025-01-19 23:04:44] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:44] debug: 	zh:controller: Received payload: clusterID=768, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=151, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":48,"commandIdentifier":11},"payload":{"cmdId":10,"statusCode":0},"command":{"ID":11,"name":"defaultRsp","parameters":[{"name":"cmdId","type":32},{"name":"statusCode","type":32}]}}
[2025-01-19 23:04:44] debug: 	zh:deconz: response received (48)
[2025-01-19 23:04:44] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":151,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:04:45] debug: 	z2m: Retrieving state of 'Küchentisch' after reconnect
[2025-01-19 23:04:45] debug: 	zh:controller:endpoint: ZCL command 0x7cb03eaa0a0176bd/3 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:04:45] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xe707 EP:3 SeqNr. 47 request id: 82
[2025-01-19 23:04:45] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 82 status: 0
[2025-01-19 23:04:45] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:45] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:04:45] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:45] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:04:45] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 48
[2025-01-19 23:04:45] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xe707 request id: 82 confirm status: 0
[2025-01-19 23:04:45] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:45] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 49
[2025-01-19 23:04:45] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:04:45] debug: 	zh:deconz: resolve request (49)
[2025-01-19 23:04:45] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:04:45] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:45] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:45] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 49
[2025-01-19 23:04:45] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 49 srcAddr: 0xe707 destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 255
[2025-01-19 23:04:45] debug: 	zh:deconz:frameparser: response payload: 1831010000001001
[2025-01-19 23:04:45] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:45] debug: 	zh:controller: Received payload: clusterID=6, address=59143, groupID=0, endpoint=3, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":49,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":16,"attrData":1}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:04:45] debug: 	zh:deconz: response received (49)
[2025-01-19 23:04:45] debug: 	z2m: Received Zigbee message from 'Küchentisch', type 'readResponse', cluster 'genOnOff', data '{"onOff":1}' from endpoint 3 with groupID 0
[2025-01-19 23:04:45] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Küchentisch', payload '{"brightness":254,"effect":null,"linkquality":255,"state":"ON","update":{"installed_version":16909584,"latest_version":16909584,"state":"idle"}}'
[2025-01-19 23:04:48] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Küchentisch/set' with data '{"state":"OFF"}'
[2025-01-19 23:04:48] debug: 	z2m: Publishing 'set' 'state' to 'Küchentisch'
[2025-01-19 23:04:48] debug: 	zh:controller:endpoint: ZCL command 0x7cb03eaa0a0176bd/3 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xe707 EP:3 SeqNr. 50 request id: 83
[2025-01-19 23:04:48] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 83 status: 0
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:48] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:04:48] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101110
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 51
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 52
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:48] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xe707 request id: 83 confirm status: 0
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:48] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 50
[2025-01-19 23:04:48] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:04:48] debug: 	zh:deconz: resolve request (50)
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 53
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 54
[2025-01-19 23:04:48] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 53 srcAddr: 0xe707 destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 255
[2025-01-19 23:04:48] debug: 	zh:deconz:frameparser: response payload: 18320b0000
[2025-01-19 23:04:48] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:48] debug: 	zh:controller: Received payload: clusterID=6, address=59143, groupID=0, endpoint=3, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":50,"commandIdentifier":11},"payload":{"cmdId":0,"statusCode":0},"command":{"ID":11,"name":"defaultRsp","parameters":[{"name":"cmdId","type":32},{"name":"statusCode","type":32}]}}
[2025-01-19 23:04:48] debug: 	zh:deconz: response received (50)
[2025-01-19 23:04:48] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Küchentisch', payload '{"brightness":254,"effect":null,"linkquality":255,"state":"OFF","update":{"installed_version":16909584,"latest_version":16909584,"state":"idle"}}'
[2025-01-19 23:04:49] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:04:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:49] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:49] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 55
[2025-01-19 23:04:49] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 55 srcAddr: 0xe707 destAddr: 0xfffd profile id: 0x0 cluster id: 0x6 lqi: 255
[2025-01-19 23:04:49] debug: 	zh:deconz:frameparser: response payload: 01fdff040101190000
[2025-01-19 23:04:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:49] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - Error: Unsupported response reading for cluster ID '6'.
[2025-01-19 23:04:49] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:04:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:49] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:49] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 56
[2025-01-19 23:04:49] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 56 srcAddr: 0xe707 destAddr: 0x0 profile id: 0x0 cluster id: 0x1 lqi: 255
[2025-01-19 23:04:49] debug: 	zh:deconz:frameparser: response payload: 0200000000
[2025-01-19 23:04:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:49] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - Error: Unsupported response reading for cluster ID '1'.
[2025-01-19 23:04:49] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:04:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:49] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:49] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 57
[2025-01-19 23:04:49] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 57 srcAddr: 0xe707 destAddr: 0x0 profile id: 0x104 cluster id: 0x19 lqi: 255
[2025-01-19 23:04:49] debug: 	zh:deconz:frameparser: response payload: 110001000c11130010050201
[2025-01-19 23:04:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:49] debug: 	zh:controller: Received payload: clusterID=25, address=59143, groupID=0, endpoint=3, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":0,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":0,"commandIdentifier":1},"payload":{"fieldControl":0,"manufacturerCode":4364,"imageType":19,"fileVersion":16909584},"command":{"ID":1,"response":2,"parameters":[{"name":"fieldControl","type":32},{"name":"manufacturerCode","type":33},{"name":"imageType","type":33},{"name":"fileVersion","type":35}],"name":"queryNextImageRequest"}}
[2025-01-19 23:04:49] debug: 	z2m: Received Zigbee message from 'Küchentisch', type 'commandQueryNextImageRequest', cluster 'genOta', data '{"fieldControl":0,"fileVersion":16909584,"imageType":19,"manufacturerCode":4364}' from endpoint 3 with groupID 0
[2025-01-19 23:04:49] debug: 	z2m: Device 'Küchentisch' requested OTA
[2025-01-19 23:04:49] debug: 	zhc:ota: [0x7cb03eaa0a0176bd | Classic A60 W clear - LIGHTIFY] Checking if an update is available
[2025-01-19 23:04:49] debug: 	zhc:ota: [0x7cb03eaa0a0176bd | Classic A60 W clear - LIGHTIFY] Checking latest image availability, current: {"fieldControl":0,"manufacturerCode":4364,"imageType":19,"fileVersion":16909584}
[2025-01-19 23:04:49] debug: 	zhc:ota: [0x7cb03eaa0a0176bd | Classic A60 W clear - LIGHTIFY] Getting image metadata...
[2025-01-19 23:04:50] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Küchentisch/set' with data '{"state":"ON"}'
[2025-01-19 23:04:50] debug: 	z2m: Publishing 'set' 'state' to 'Küchentisch'
[2025-01-19 23:04:50] debug: 	zh:controller:endpoint: ZCL command 0x7cb03eaa0a0176bd/3 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 58
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xe707 EP:3 SeqNr. 59 request id: 84
[2025-01-19 23:04:50] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:50] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 84 status: 0
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:50] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:50] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101110
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 60
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 61
[2025-01-19 23:04:50] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xe707 request id: 84 confirm status: 0
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:50] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 51
[2025-01-19 23:04:50] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:04:50] debug: 	zh:deconz: resolve request (51)
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 62
[2025-01-19 23:04:50] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 61 srcAddr: 0xe707 destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 255
[2025-01-19 23:04:50] debug: 	zh:deconz:frameparser: response payload: 18330b0100
[2025-01-19 23:04:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:50] debug: 	zh:controller: Received payload: clusterID=6, address=59143, groupID=0, endpoint=3, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":51,"commandIdentifier":11},"payload":{"cmdId":1,"statusCode":0},"command":{"ID":11,"name":"defaultRsp","parameters":[{"name":"cmdId","type":32},{"name":"statusCode","type":32}]}}
[2025-01-19 23:04:50] debug: 	zh:deconz: response received (51)
[2025-01-19 23:04:50] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Küchentisch', payload '{"brightness":254,"effect":null,"linkquality":255,"state":"ON","update":{"installed_version":16909584,"latest_version":16909584,"state":"idle"}}'
[2025-01-19 23:04:50] debug: 	zhc:ota: Downloaded main index
[2025-01-19 23:04:50] debug: 	zhc:ota: [0x7cb03eaa0a0176bd | Classic A60 W clear - LIGHTIFY] Result for latest image availability, meta: '{"fileName":"ZLL_MK_0x01020510_CLA60_W_CLEAR.ota","fileVersion":16909584,"fileSize":123884,"url":"https://github.com/Koenkk/zigbee-OTA/raw/master/images/Osram/ZLL_MK_0x01020510_CLA60_W_CLEAR.ota","imageType":19,"manufacturerCode":4364,"sha512":"7f4bb423aed7d3d81a43c054897796f76e05c049911fee9ffc36d4c4a4baa44369bb35a8d44d8e3630e26ec65a3a59e5ada97d75109887422c7e6a75b2a9bcf5","otaHeaderString":"NULL\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000"}'
[2025-01-19 23:04:50] debug: 	zhc:ota: [0x7cb03eaa0a0176bd | Classic A60 W clear - LIGHTIFY] Upgrade available: NO
[2025-01-19 23:04:50] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Küchentisch', payload '{"brightness":254,"effect":null,"linkquality":255,"state":"ON","update":{"installed_version":16909584,"latest_version":16909584,"state":"idle"}}'
[2025-01-19 23:04:50] debug: 	zh:controller:endpoint: CommandResponse 0x7cb03eaa0a0176bd/3 genOta.queryNextImageResponse({"status":152}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:04:51] debug: 	zh:deconz: no response expected (52)
[2025-01-19 23:04:51] debug: 	z2m: Responded to OTA request of 'Küchentisch' with 'NO_IMAGE_AVAILABLE'
[2025-01-19 23:04:51] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xe707 EP:3 SeqNr. 63 request id: 85
[2025-01-19 23:04:51] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 85 status: 0
[2025-01-19 23:04:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:51] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:04:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:51] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:04:51] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 64
[2025-01-19 23:04:51] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xe707 request id: 85 confirm status: 0
[2025-01-19 23:04:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:51] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 52
[2025-01-19 23:04:51] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:04:51] debug: 	zh:deconz: resolve request (52)
[2025-01-19 23:04:52] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Flurlicht/set' with data '{"state":"OFF"}'
[2025-01-19 23:04:52] debug: 	z2m: Publishing 'set' 'state' to 'Flurlicht'
[2025-01-19 23:04:52] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:04:52] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 65 request id: 86
[2025-01-19 23:04:52] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 86 status: 0
[2025-01-19 23:04:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:52] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:04:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:52] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:04:52] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 66
[2025-01-19 23:04:52] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 86 confirm status: 0
[2025-01-19 23:04:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:52] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 53
[2025-01-19 23:04:52] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:04:52] debug: 	zh:deconz: resolve request (53)
[2025-01-19 23:04:52] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:04:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:52] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:52] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 67
[2025-01-19 23:04:52] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 67 srcAddr: 0xb9ef destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 255
[2025-01-19 23:04:52] debug: 	zh:deconz:frameparser: response payload: 08350b0000
[2025-01-19 23:04:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:52] debug: 	zh:controller: Received payload: clusterID=6, address=47599, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":53,"commandIdentifier":11},"payload":{"cmdId":0,"statusCode":0},"command":{"ID":11,"name":"defaultRsp","parameters":[{"name":"cmdId","type":32},{"name":"statusCode","type":32}]}}
[2025-01-19 23:04:52] debug: 	zh:deconz: response received (53)
[2025-01-19 23:04:52] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Flurlicht', payload '{"brightness":229,"effect":null,"linkquality":255,"state":"OFF","update":{"installed_version":17130496,"latest_version":17130496,"state":"idle"}}'
[2025-01-19 23:04:53] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Flurlicht/set' with data '{"state":"ON"}'
[2025-01-19 23:04:53] debug: 	z2m: Publishing 'set' 'state' to 'Flurlicht'
[2025-01-19 23:04:53] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:04:53] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 68 request id: 87
[2025-01-19 23:04:53] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 87 status: 0
[2025-01-19 23:04:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:53] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:04:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:53] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:04:53] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 69
[2025-01-19 23:04:53] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 87 confirm status: 0
[2025-01-19 23:04:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:54] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 54
[2025-01-19 23:04:54] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:04:54] debug: 	zh:deconz: resolve request (54)
[2025-01-19 23:04:54] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:04:54] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:54] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:04:54] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 70
[2025-01-19 23:04:54] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 70 srcAddr: 0xb9ef destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 255
[2025-01-19 23:04:54] debug: 	zh:deconz:frameparser: response payload: 08360b0100
[2025-01-19 23:04:54] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:04:54] debug: 	zh:controller: Received payload: clusterID=6, address=47599, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":54,"commandIdentifier":11},"payload":{"cmdId":1,"statusCode":0},"command":{"ID":11,"name":"defaultRsp","parameters":[{"name":"cmdId","type":32},{"name":"statusCode","type":32}]}}
[2025-01-19 23:04:54] debug: 	zh:deconz: response received (54)
[2025-01-19 23:04:54] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Flurlicht', payload '{"brightness":229,"effect":null,"linkquality":255,"state":"ON","update":{"installed_version":17130496,"latest_version":17130496,"state":"idle"}}'
[2025-01-19 23:05:00] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 71
[2025-01-19 23:05:00] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:05:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:07] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Küchentisch/set' with data '{"state":"OFF"}'
[2025-01-19 23:05:07] debug: 	z2m: Publishing 'set' 'state' to 'Küchentisch'
[2025-01-19 23:05:07] debug: 	zh:controller:endpoint: ZCL command 0x7cb03eaa0a0176bd/3 genOnOff.off({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:05:07] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xe707 EP:3 SeqNr. 72 request id: 88
[2025-01-19 23:05:07] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 88 status: 0
[2025-01-19 23:05:07] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:07] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:05:07] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:07] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:05:07] error: 	z2m: Failed to execute LQI for 'Lichtschlauch'
[2025-01-19 23:05:07] debug: 	z2m: Error: waiting for response TIMEOUT
    at DeconzAdapter.checkReceivedDataPayload (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:703:28)
    at Timeout._onTimeout (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:75:18)
    at listOnTimeout (node:internal/timers:569:17)
    at processTimers (node:internal/timers:512:7)
[2025-01-19 23:05:07] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 73
[2025-01-19 23:05:07] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101110
[2025-01-19 23:05:07] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:07] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xe707 request id: 88 confirm status: 0
[2025-01-19 23:05:07] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:07] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 55
[2025-01-19 23:05:07] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:05:07] debug: 	zh:deconz: resolve request (55)
[2025-01-19 23:05:07] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:07] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 74
[2025-01-19 23:05:07] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 74 srcAddr: 0xe707 destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 255
[2025-01-19 23:05:07] debug: 	zh:deconz:frameparser: response payload: 18370b0000
[2025-01-19 23:05:07] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:07] debug: 	zh:controller: Received payload: clusterID=6, address=59143, groupID=0, endpoint=3, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":55,"commandIdentifier":11},"payload":{"cmdId":0,"statusCode":0},"command":{"ID":11,"name":"defaultRsp","parameters":[{"name":"cmdId","type":32},{"name":"statusCode","type":32}]}}
[2025-01-19 23:05:07] debug: 	zh:deconz: response received (55)
[2025-01-19 23:05:07] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Küchentisch', payload '{"brightness":254,"effect":null,"linkquality":255,"state":"OFF","update":{"installed_version":16909584,"latest_version":16909584,"state":"idle"}}'
[2025-01-19 23:05:08] debug: 	z2m:mqtt: Received MQTT message on 'zigbee2mqtt/Küchentisch/set' with data '{"state":"ON"}'
[2025-01-19 23:05:08] debug: 	z2m: Publishing 'set' 'state' to 'Küchentisch'
[2025-01-19 23:05:08] debug: 	zh:controller:endpoint: ZCL command 0x7cb03eaa0a0176bd/3 genOnOff.on({}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:05:08] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xe707 EP:3 SeqNr. 75 request id: 89
[2025-01-19 23:05:08] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 89 status: 0
[2025-01-19 23:05:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:08] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:05:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:08] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:05:08] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 76
[2025-01-19 23:05:08] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xe707 request id: 89 confirm status: 0
[2025-01-19 23:05:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:08] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 56
[2025-01-19 23:05:08] debug: 	zh:deconz: false, false, false, 10000
[2025-01-19 23:05:08] debug: 	zh:deconz: resolve request (56)
[2025-01-19 23:05:08] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:08] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:08] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 77
[2025-01-19 23:05:08] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 77 srcAddr: 0xe707 destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 255
[2025-01-19 23:05:08] debug: 	zh:deconz:frameparser: response payload: 18380b0100
[2025-01-19 23:05:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:08] debug: 	zh:controller: Received payload: clusterID=6, address=59143, groupID=0, endpoint=3, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":56,"commandIdentifier":11},"payload":{"cmdId":1,"statusCode":0},"command":{"ID":11,"name":"defaultRsp","parameters":[{"name":"cmdId","type":32},{"name":"statusCode","type":32}]}}
[2025-01-19 23:05:08] debug: 	zh:deconz: response received (56)
[2025-01-19 23:05:08] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Küchentisch', payload '{"brightness":254,"effect":null,"linkquality":255,"state":"ON","update":{"installed_version":16909584,"latest_version":16909584,"state":"idle"}}'
[2025-01-19 23:05:08] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xe60e EP:0 SeqNr. 78 request id: 90
[2025-01-19 23:05:08] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 90 status: 0
[2025-01-19 23:05:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:09] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:09] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:09] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:09] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 79
[2025-01-19 23:05:09] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 79 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 175
[2025-01-19 23:05:09] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:05:09] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:09] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:05:09] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:05:09] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:05:10] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:05:10] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 80
[2025-01-19 23:05:10] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:05:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:10] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:10] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:10] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 81
[2025-01-19 23:05:10] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 81 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 23:05:10] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 23:05:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:10] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:05:10] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 23:05:10] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 23:05:11] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 23:05:12] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:05:12] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 82 request id: 91
[2025-01-19 23:05:12] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 91 status: 0
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:12] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 83
[2025-01-19 23:05:12] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 91 confirm status: 0
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:12] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 57
[2025-01-19 23:05:12] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:05:12] debug: 	zh:deconz: resolve request (57)
[2025-01-19 23:05:12] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 84
[2025-01-19 23:05:12] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 84 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 167
[2025-01-19 23:05:12] debug: 	zh:deconz:frameparser: response payload: 0839010000001001
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:12] debug: 	zh:controller: Received payload: clusterID=6, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=167, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":57,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":16,"attrData":1}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:05:12] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":57,"writeUndiv":false})
[2025-01-19 23:05:12] debug: 	zh:deconz: no response expected (57)
[2025-01-19 23:05:12] debug: 	zh:deconz: response received (57)
[2025-01-19 23:05:12] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genOnOff', data '{"onOff":1}' from endpoint 1 with groupID 0
[2025-01-19 23:05:12] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":167,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 85 request id: 92
[2025-01-19 23:05:12] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 92 status: 0
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:12] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 86
[2025-01-19 23:05:12] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 92 confirm status: 0
[2025-01-19 23:05:12] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:12] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 57
[2025-01-19 23:05:12] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:05:12] debug: 	zh:deconz: resolve request (57)
[2025-01-19 23:05:13] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 23:05:13] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:05:13] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 87 request id: 93
[2025-01-19 23:05:13] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 93 status: 0
[2025-01-19 23:05:13] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:13] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:05:13] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:13] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:05:13] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 88
[2025-01-19 23:05:13] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 93 confirm status: 0
[2025-01-19 23:05:13] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:13] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 58
[2025-01-19 23:05:13] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:05:13] debug: 	zh:deconz: resolve request (58)
[2025-01-19 23:05:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:05:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:05:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 89
[2025-01-19 23:05:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xe60e request id: 90 confirm status: 0
[2025-01-19 23:05:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 90
[2025-01-19 23:05:20] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:05:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:22] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 91
[2025-01-19 23:05:22] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 91 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0xef00 lqi: 255
[2025-01-19 23:05:22] debug: 	zh:deconz:frameparser: response payload: 09580200580102000400000100
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:22] debug: 	zh:controller: Received payload: clusterID=61184, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":88,"commandIdentifier":2},"payload":{"seq":22528,"dpValues":[{"dp":1,"datatype":2,"data":{"type":"Buffer","data":[0,0,1,0]}}]},"command":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}],"name":"dataReport"}}
[2025-01-19 23:05:22] debug: 	zh:controller:endpoint: ZCL command 0xa4c13838ba59a1b2/1 manuSpecificTuya.defaultRsp({"cmdId":2,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"transactionSequenceNumber":88,"writeUndiv":false})
[2025-01-19 23:05:22] debug: 	zh:deconz: no response expected (88)
[2025-01-19 23:05:22] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'commandDataReport', cluster 'manuSpecificTuya', data '{"dpValues":[{"data":{"data":[0,0,1,0],"type":"Buffer"},"datatype":2,"dp":1}],"seq":22528}' from endpoint 1 with groupID 0
[2025-01-19 23:05:22] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":43,"humidity_calibration":0,"linkquality":255,"temperature":25.6,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:1 SeqNr. 92 request id: 94
[2025-01-19 23:05:22] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 94 status: 0
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:22] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 93
[2025-01-19 23:05:22] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 94 confirm status: 0
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:22] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 88
[2025-01-19 23:05:22] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:05:22] debug: 	zh:deconz: resolve request (88)
[2025-01-19 23:05:22] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 94
[2025-01-19 23:05:22] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 94 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0xef00 lqi: 255
[2025-01-19 23:05:22] debug: 	zh:deconz:frameparser: response payload: 0959020059020200040000002d
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:22] debug: 	zh:controller: Received payload: clusterID=61184, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":89,"commandIdentifier":2},"payload":{"seq":22784,"dpValues":[{"dp":2,"datatype":2,"data":{"type":"Buffer","data":[0,0,0,45]}}]},"command":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}],"name":"dataReport"}}
[2025-01-19 23:05:22] debug: 	zh:controller:endpoint: ZCL command 0xa4c13838ba59a1b2/1 manuSpecificTuya.defaultRsp({"cmdId":2,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"transactionSequenceNumber":89,"writeUndiv":false})
[2025-01-19 23:05:22] debug: 	zh:deconz: no response expected (89)
[2025-01-19 23:05:22] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'commandDataReport', cluster 'manuSpecificTuya', data '{"dpValues":[{"data":{"data":[0,0,0,45],"type":"Buffer"},"datatype":2,"dp":2}],"seq":22784}' from endpoint 1 with groupID 0
[2025-01-19 23:05:22] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":45,"humidity_calibration":0,"linkquality":255,"temperature":25.6,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:1 SeqNr. 95 request id: 95
[2025-01-19 23:05:22] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 95 status: 0
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:22] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 96
[2025-01-19 23:05:22] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 95 confirm status: 0
[2025-01-19 23:05:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:22] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 89
[2025-01-19 23:05:22] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:05:22] debug: 	zh:deconz: resolve request (89)
[2025-01-19 23:05:23] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:23] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:23] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 97
[2025-01-19 23:05:23] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 97 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0x402 lqi: 255
[2025-01-19 23:05:23] debug: 	zh:deconz:frameparser: response payload: 185a0a000029000a
[2025-01-19 23:05:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:23] debug: 	zh:controller: Received payload: clusterID=1026, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":90,"commandIdentifier":10},"payload":[{"attrId":0,"dataType":41,"attrData":2560}],"command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}}
[2025-01-19 23:05:23] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'attributeReport', cluster 'msTemperatureMeasurement', data '{"measuredValue":2560}' from endpoint 1 with groupID 0
[2025-01-19 23:05:23] debug: 	z2m: No converter available for 'ZG-227Z' with cluster 'msTemperatureMeasurement' and type 'attributeReport' and data '{"measuredValue":2560}'
[2025-01-19 23:05:23] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (58) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:05:23] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (58) Error: waiting for response TIMEOUT))
[2025-01-19 23:05:23] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:23] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:23] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 98
[2025-01-19 23:05:23] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 98 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0x405 lqi: 255
[2025-01-19 23:05:23] debug: 	zh:deconz:frameparser: response payload: 185b0a000021b211
[2025-01-19 23:05:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:23] debug: 	zh:controller: Received payload: clusterID=1029, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":91,"commandIdentifier":10},"payload":[{"attrId":0,"dataType":33,"attrData":4530}],"command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}}
[2025-01-19 23:05:23] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'attributeReport', cluster 'msRelativeHumidity', data '{"measuredValue":4530}' from endpoint 1 with groupID 0
[2025-01-19 23:05:23] debug: 	z2m: No converter available for 'ZG-227Z' with cluster 'msRelativeHumidity' and type 'attributeReport' and data '{"measuredValue":4530}'
[2025-01-19 23:05:24] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:24] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:24] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 99
[2025-01-19 23:05:24] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 99 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 23:05:24] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:05:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:24] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:05:24] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:05:24] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:05:24] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:05:24] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:24] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:24] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 100
[2025-01-19 23:05:24] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 100 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 23:05:24] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:05:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:24] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:05:24] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:05:24] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:05:24] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:05:26] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:26] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:26] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:26] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 101
[2025-01-19 23:05:26] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 101 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:05:26] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:05:26] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:26] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:05:26] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:05:26] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:05:26] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:05:28] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:05:28] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 102 request id: 96
[2025-01-19 23:05:28] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 96 status: 0
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:28] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 103
[2025-01-19 23:05:28] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 96 confirm status: 0
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:28] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 59
[2025-01-19 23:05:28] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:05:28] debug: 	zh:deconz: resolve request (59)
[2025-01-19 23:05:28] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 104
[2025-01-19 23:05:28] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 104 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x6 lqi: 167
[2025-01-19 23:05:28] debug: 	zh:deconz:frameparser: response payload: 083b010000001001
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:28] debug: 	zh:controller: Received payload: clusterID=6, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=167, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":59,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":16,"attrData":1}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:05:28] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":59,"writeUndiv":false})
[2025-01-19 23:05:28] debug: 	zh:deconz: no response expected (59)
[2025-01-19 23:05:28] debug: 	zh:deconz: response received (59)
[2025-01-19 23:05:28] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genOnOff', data '{"onOff":1}' from endpoint 1 with groupID 0
[2025-01-19 23:05:28] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":167,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 105 request id: 97
[2025-01-19 23:05:28] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 97 status: 0
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:28] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 106
[2025-01-19 23:05:28] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 97 confirm status: 0
[2025-01-19 23:05:28] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:28] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 59
[2025-01-19 23:05:28] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:05:28] debug: 	zh:deconz: resolve request (59)
[2025-01-19 23:05:30] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 107
[2025-01-19 23:05:30] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:05:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:40] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 108
[2025-01-19 23:05:40] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:05:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:44] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:44] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:44] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:44] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 109
[2025-01-19 23:05:44] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 109 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x6 lqi: 175
[2025-01-19 23:05:44] debug: 	zh:deconz:frameparser: response payload: 01fdff040101190000
[2025-01-19 23:05:44] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:44] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - Error: Unsupported response reading for cluster ID '6'.
[2025-01-19 23:05:46] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:05:46] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:46] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:05:46] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 110
[2025-01-19 23:05:46] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 110 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x19 lqi: 255
[2025-01-19 23:05:46] debug: 	zh:deconz:frameparser: response payload: 010301018911a000107319030200
[2025-01-19 23:05:46] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:46] debug: 	zh:controller: Received payload: clusterID=25, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":0,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":3,"commandIdentifier":1},"payload":{"fieldControl":1,"manufacturerCode":4489,"imageType":160,"fileVersion":51999504},"command":{"ID":1,"response":2,"parameters":[{"name":"fieldControl","type":32},{"name":"manufacturerCode","type":33},{"name":"imageType","type":33},{"name":"fileVersion","type":35}],"name":"queryNextImageRequest"}}
[2025-01-19 23:05:46] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'commandQueryNextImageRequest', cluster 'genOta', data '{"fieldControl":1,"fileVersion":51999504,"imageType":160,"manufacturerCode":4489}' from endpoint 1 with groupID 0
[2025-01-19 23:05:46] debug: 	z2m: Device 'Bogenlampe' requested OTA
[2025-01-19 23:05:46] debug: 	zhc:ota: [0xf0d1b800001ffcf2 | A60S RGBW] Checking if an update is available
[2025-01-19 23:05:46] debug: 	zhc:ota: [0xf0d1b800001ffcf2 | A60S RGBW] Checking latest image availability, current: {"fieldControl":1,"manufacturerCode":4489,"imageType":160,"fileVersion":51999504}
[2025-01-19 23:05:46] debug: 	zhc:ota: [0xf0d1b800001ffcf2 | A60S RGBW] Getting image metadata...
[2025-01-19 23:05:46] debug: 	zhc:ota: Downloaded main index
[2025-01-19 23:05:46] debug: 	zhc:ota: [0xf0d1b800001ffcf2 | A60S RGBW] Result for latest image availability, meta: '{"fileName":"A60S_RGBW-0x1189-0x00A0-0x03197310-MF_DIS-20240523095111-3221010102432.ota","fileVersion":51999504,"fileSize":314466,"originalUrl":"https://api.update.ledvance.com/v1/zigbee/firmwares/download?company=4489&product=160&version=3.25.115.16","url":"https://github.com/Koenkk/zigbee-OTA/raw/master/images/LEDVANCE/A60S_RGBW-0x1189-0x00A0-0x03197310-MF_DIS-20240523095111-3221010102432.ota","imageType":160,"manufacturerCode":4489,"sha512":"d0ccca81ba3598d79b70ab4ee836c230d725cf02e5ee4b6feff7d4301c3c86afbe2b30504e96cee88b5333aec580d2c1e1b09cfbc4d4e359f744b86deb6f26cc","otaHeaderString":"A60S_RGBW\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000\u0000","releaseNotes":"(1) Security patch\r\n(2) Refine RGBW color control.\r\n(3) Support sleep mode in Hue automation settings. "}'
[2025-01-19 23:05:46] info: 	zhc:ota: [0xf0d1b800001ffcf2 | A60S RGBW] Firmware release notes: (1) Security patch(2) Refine RGBW color control.(3) Support sleep mode in Hue automation settings. 
[2025-01-19 23:05:46] debug: 	zhc:ota: [0xf0d1b800001ffcf2 | A60S RGBW] Upgrade available: NO
[2025-01-19 23:05:46] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":255,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:05:46] debug: 	zh:controller:endpoint: CommandResponse 0xf0d1b800001ffcf2/1 genOta.queryNextImageResponse({"status":152}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:05:46] debug: 	zh:deconz: no response expected (3)
[2025-01-19 23:05:46] debug: 	z2m: Responded to OTA request of 'Bogenlampe' with 'NO_IMAGE_AVAILABLE'
[2025-01-19 23:05:46] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 111 request id: 98
[2025-01-19 23:05:46] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 98 status: 0
[2025-01-19 23:05:46] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:46] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:05:46] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:46] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:05:46] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 112
[2025-01-19 23:05:46] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 98 confirm status: 0
[2025-01-19 23:05:46] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:05:46] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 3
[2025-01-19 23:05:46] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:05:46] debug: 	zh:deconz: resolve request (3)
[2025-01-19 23:05:50] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 113
[2025-01-19 23:05:50] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:05:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:00] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 114
[2025-01-19 23:06:00] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:06:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:10] debug: 	zh:deconz:driver: send write parameter request from queue. seqNr: 115 paramId: 38 param: 600
[2025-01-19 23:06:10] debug: 	zh:deconz:frameparser: write parameter response - parameter id: 38 - status: 0
[2025-01-19 23:06:10] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 116
[2025-01-19 23:06:10] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:06:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:13] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xe60e EP:0 SeqNr. 117 request id: 99
[2025-01-19 23:06:13] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 99 status: 0
[2025-01-19 23:06:13] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 118
[2025-01-19 23:06:20] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:06:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:22] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:06:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:22] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:06:22] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 119
[2025-01-19 23:06:22] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 119 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0xef00 lqi: 255
[2025-01-19 23:06:22] debug: 	zh:deconz:frameparser: response payload: 095c02005c01020004000000fe
[2025-01-19 23:06:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:22] debug: 	zh:controller: Received payload: clusterID=61184, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":92,"commandIdentifier":2},"payload":{"seq":23552,"dpValues":[{"dp":1,"datatype":2,"data":{"type":"Buffer","data":[0,0,0,254]}}]},"command":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}],"name":"dataReport"}}
[2025-01-19 23:06:22] debug: 	zh:controller:endpoint: ZCL command 0xa4c13838ba59a1b2/1 manuSpecificTuya.defaultRsp({"cmdId":2,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"transactionSequenceNumber":92,"writeUndiv":false})
[2025-01-19 23:06:22] debug: 	zh:deconz: no response expected (92)
[2025-01-19 23:06:22] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'commandDataReport', cluster 'manuSpecificTuya', data '{"dpValues":[{"data":{"data":[0,0,0,254],"type":"Buffer"},"datatype":2,"dp":1}],"seq":23552}' from endpoint 1 with groupID 0
[2025-01-19 23:06:22] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":45,"humidity_calibration":0,"linkquality":255,"temperature":25.4,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 23:06:22] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:1 SeqNr. 120 request id: 100
[2025-01-19 23:06:22] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 100 status: 0
[2025-01-19 23:06:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:22] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:06:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:22] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:06:22] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 121
[2025-01-19 23:06:22] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 100 confirm status: 0
[2025-01-19 23:06:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:22] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 92
[2025-01-19 23:06:22] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:06:22] debug: 	zh:deconz: resolve request (92)
[2025-01-19 23:06:23] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 122
[2025-01-19 23:06:23] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 122 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0xef00 lqi: 255
[2025-01-19 23:06:23] debug: 	zh:deconz:frameparser: response payload: 095d02005d020200040000002e
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:23] debug: 	zh:controller: Received payload: clusterID=61184, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":93,"commandIdentifier":2},"payload":{"seq":23808,"dpValues":[{"dp":2,"datatype":2,"data":{"type":"Buffer","data":[0,0,0,46]}}]},"command":{"ID":2,"parameters":[{"name":"seq","type":33},{"name":"dpValues","type":1011}],"name":"dataReport"}}
[2025-01-19 23:06:23] debug: 	zh:controller:endpoint: ZCL command 0xa4c13838ba59a1b2/1 manuSpecificTuya.defaultRsp({"cmdId":2,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"transactionSequenceNumber":93,"writeUndiv":false})
[2025-01-19 23:06:23] debug: 	zh:deconz: no response expected (93)
[2025-01-19 23:06:23] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'commandDataReport', cluster 'manuSpecificTuya', data '{"dpValues":[{"data":{"data":[0,0,0,46],"type":"Buffer"},"datatype":2,"dp":2}],"seq":23808}' from endpoint 1 with groupID 0
[2025-01-19 23:06:23] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Medienschrank Wohnzimmer', payload '{"battery":50,"humidity":46,"humidity_calibration":0,"linkquality":255,"temperature":25.4,"temperature_calibration":0,"temperature_unit":"celsius"}'
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xf8fd EP:1 SeqNr. 123 request id: 101
[2025-01-19 23:06:23] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 101 status: 0
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:23] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 124
[2025-01-19 23:06:23] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xf8fd request id: 101 confirm status: 0
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:23] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 93
[2025-01-19 23:06:23] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:06:23] debug: 	zh:deconz: resolve request (93)
[2025-01-19 23:06:23] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 125
[2025-01-19 23:06:23] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xe60e request id: 99 confirm status: 0
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:23] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 126
[2025-01-19 23:06:23] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 126 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0x402 lqi: 255
[2025-01-19 23:06:23] debug: 	zh:deconz:frameparser: response payload: 185e0a000029ec09
[2025-01-19 23:06:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:23] debug: 	zh:controller: Received payload: clusterID=1026, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":94,"commandIdentifier":10},"payload":[{"attrId":0,"dataType":41,"attrData":2540}],"command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}}
[2025-01-19 23:06:23] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'attributeReport', cluster 'msTemperatureMeasurement', data '{"measuredValue":2540}' from endpoint 1 with groupID 0
[2025-01-19 23:06:23] debug: 	z2m: No converter available for 'ZG-227Z' with cluster 'msTemperatureMeasurement' and type 'attributeReport' and data '{"measuredValue":2540}'
[2025-01-19 23:06:24] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:06:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:24] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:06:24] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 127
[2025-01-19 23:06:24] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 127 srcAddr: 0xf8fd destAddr: 0x0 profile id: 0x104 cluster id: 0x405 lqi: 255
[2025-01-19 23:06:24] debug: 	zh:deconz:frameparser: response payload: 185f0a000021d011
[2025-01-19 23:06:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:24] debug: 	zh:controller: Received payload: clusterID=1029, address=63741, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":95,"commandIdentifier":10},"payload":[{"attrId":0,"dataType":33,"attrData":4560}],"command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}}
[2025-01-19 23:06:24] debug: 	z2m: Received Zigbee message from 'Medienschrank Wohnzimmer', type 'attributeReport', cluster 'msRelativeHumidity', data '{"measuredValue":4560}' from endpoint 1 with groupID 0
[2025-01-19 23:06:24] debug: 	z2m: No converter available for 'ZG-227Z' with cluster 'msRelativeHumidity' and type 'attributeReport' and data '{"measuredValue":4560}'
[2025-01-19 23:06:30] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 128
[2025-01-19 23:06:30] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:06:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:40] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 129
[2025-01-19 23:06:40] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:06:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:06:50] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 130
[2025-01-19 23:06:50] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:06:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 131 request id: 102
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 102 status: 0
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 132
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 102 confirm status: 0
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 60
[2025-01-19 23:07:00] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:07:00] debug: 	zh:deconz: resolve request (60)
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 133
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 134
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 134 srcAddr: 0xb9ef destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 255
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: response payload: 183c0100000020e5
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:controller: Received payload: clusterID=8, address=47599, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=255, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":60,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":229}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:07:00] debug: 	zh:deconz: response received (60)
[2025-01-19 23:07:00] debug: 	z2m: Received Zigbee message from 'Flurlicht', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":229}' from endpoint 1 with groupID 0
[2025-01-19 23:07:00] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Flurlicht', payload '{"brightness":229,"effect":null,"linkquality":255,"state":"ON","update":{"installed_version":17130496,"latest_version":17130496,"state":"idle"}}'
[2025-01-19 23:07:00] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 135 request id: 103
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 103 status: 0
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 136
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 103 confirm status: 0
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 61
[2025-01-19 23:07:00] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:07:00] debug: 	zh:deconz: resolve request (61)
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 137
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 137 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 175
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: response payload: 083d010000002069
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=175, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":61,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":105}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:07:00] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":61,"writeUndiv":false})
[2025-01-19 23:07:00] debug: 	zh:deconz: no response expected (61)
[2025-01-19 23:07:00] debug: 	zh:deconz: response received (61)
[2025-01-19 23:07:00] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":105}' from endpoint 1 with groupID 0
[2025-01-19 23:07:00] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":175,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 138 request id: 104
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 104 status: 0
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 139
[2025-01-19 23:07:00] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 104 confirm status: 0
[2025-01-19 23:07:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:00] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 61
[2025-01-19 23:07:00] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:07:00] debug: 	zh:deconz: resolve request (61)
[2025-01-19 23:07:04] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 140 request id: 105
[2025-01-19 23:07:04] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 105 status: 0
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:04] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 141
[2025-01-19 23:07:04] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 105 confirm status: 0
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:04] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 62
[2025-01-19 23:07:04] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:07:04] debug: 	zh:deconz: resolve request (62)
[2025-01-19 23:07:04] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 142
[2025-01-19 23:07:04] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 142 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 175
[2025-01-19 23:07:04] debug: 	zh:deconz:frameparser: response payload: 083e010000002069
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:04] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=175, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":62,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":105}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:07:04] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":62,"writeUndiv":false})
[2025-01-19 23:07:04] debug: 	zh:deconz: no response expected (62)
[2025-01-19 23:07:04] debug: 	zh:deconz: response received (62)
[2025-01-19 23:07:04] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":105}' from endpoint 1 with groupID 0
[2025-01-19 23:07:04] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":175,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 143 request id: 106
[2025-01-19 23:07:04] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 106 status: 0
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:04] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 144
[2025-01-19 23:07:04] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 106 confirm status: 0
[2025-01-19 23:07:04] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:04] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 62
[2025-01-19 23:07:04] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:07:04] debug: 	zh:deconz: resolve request (62)
[2025-01-19 23:07:08] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:07:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:08] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:07:08] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 145
[2025-01-19 23:07:08] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 145 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 175
[2025-01-19 23:07:08] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:07:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:08] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:07:08] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:07:08] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:07:08] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:07:09] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:07:09] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:09] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:07:09] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 146
[2025-01-19 23:07:09] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 146 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:07:09] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:07:09] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:09] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:07:09] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:07:09] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:07:09] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:07:10] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 147
[2025-01-19 23:07:10] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:07:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:11] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 148
[2025-01-19 23:07:11] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 148 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 175
[2025-01-19 23:07:11] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:11] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:07:11] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 23:07:11] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 23:07:11] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 23:07:11] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:07:11] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 149 request id: 107
[2025-01-19 23:07:11] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 150 request id: 108
[2025-01-19 23:07:11] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 107 status: 0
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:11] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:11] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 108 status: 0
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:11] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 151
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 152
[2025-01-19 23:07:11] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 107 confirm status: 0
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:11] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 108 confirm status: 0
[2025-01-19 23:07:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:11] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 63
[2025-01-19 23:07:11] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:07:11] debug: 	zh:deconz: resolve request (63)
[2025-01-19 23:07:11] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 64
[2025-01-19 23:07:11] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:07:11] debug: 	zh:deconz: resolve request (64)
[2025-01-19 23:07:13] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 23:07:13] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:13] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 153 request id: 109
[2025-01-19 23:07:13] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 109 status: 0
[2025-01-19 23:07:13] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:13] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:13] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:13] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:13] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 154
[2025-01-19 23:07:13] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 109 confirm status: 0
[2025-01-19 23:07:13] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:13] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 65
[2025-01-19 23:07:13] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:07:13] debug: 	zh:deconz: resolve request (65)
[2025-01-19 23:07:13] error: 	z2m: Failed to execute LQI for '0x0ceff6fffebf4739'
[2025-01-19 23:07:13] debug: 	z2m: Error: waiting for response TIMEOUT
    at DeconzAdapter.checkReceivedDataPayload (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:703:28)
    at Timeout._onTimeout (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:75:18)
    at listOnTimeout (node:internal/timers:569:17)
    at processTimers (node:internal/timers:512:7)
[2025-01-19 23:07:14] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x267f EP:0 SeqNr. 155 request id: 110
[2025-01-19 23:07:14] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 110 status: 0
[2025-01-19 23:07:14] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:16] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:07:16] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:16] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:07:16] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 156
[2025-01-19 23:07:16] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 156 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:07:16] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:07:16] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:16] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:07:16] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:07:16] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:07:17] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:07:17] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:17] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 157 request id: 111
[2025-01-19 23:07:17] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 111 status: 0
[2025-01-19 23:07:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:17] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:17] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:17] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 158
[2025-01-19 23:07:17] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 111 confirm status: 0
[2025-01-19 23:07:17] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:17] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 66
[2025-01-19 23:07:17] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:07:17] debug: 	zh:deconz: resolve request (66)
[2025-01-19 23:07:19] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:07:19] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:19] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 159 request id: 112
[2025-01-19 23:07:19] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 112 status: 0
[2025-01-19 23:07:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:19] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:19] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:19] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 160
[2025-01-19 23:07:19] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 112 confirm status: 0
[2025-01-19 23:07:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:19] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 67
[2025-01-19 23:07:19] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:07:19] debug: 	zh:deconz: resolve request (67)
[2025-01-19 23:07:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 161
[2025-01-19 23:07:20] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:07:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:21] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:21] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 162 request id: 113
[2025-01-19 23:07:21] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 113 status: 0
[2025-01-19 23:07:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:22] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (64) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1198:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:07:22] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (63) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:07:22] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (64) Error: waiting for response TIMEOUT))
[2025-01-19 23:07:22] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (63) Error: waiting for response TIMEOUT))
[2025-01-19 23:07:22] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:07:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:22] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:07:22] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 163
[2025-01-19 23:07:22] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 163 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 23:07:22] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:07:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:22] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:07:22] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:07:22] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:07:23] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:07:23] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:07:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:23] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:07:23] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 164
[2025-01-19 23:07:23] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 164 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 175
[2025-01-19 23:07:23] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:07:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:23] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:07:23] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:07:23] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:07:23] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (65) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:07:23] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (65) Error: waiting for response TIMEOUT))
[2025-01-19 23:07:23] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:07:25] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:25] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:25] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 165
[2025-01-19 23:07:25] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x267f request id: 110 confirm status: 0
[2025-01-19 23:07:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:25] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:07:25] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:25] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 166 request id: 114
[2025-01-19 23:07:25] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 114 status: 0
[2025-01-19 23:07:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:25] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:25] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:25] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 167
[2025-01-19 23:07:25] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 114 confirm status: 0
[2025-01-19 23:07:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:25] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 69
[2025-01-19 23:07:25] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:07:25] debug: 	zh:deconz: resolve request (69)
[2025-01-19 23:07:28] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (66) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1198:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:07:28] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (66) Error: waiting for response TIMEOUT))
[2025-01-19 23:07:29] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (67) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:07:29] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (67) Error: waiting for response TIMEOUT))
[2025-01-19 23:07:30] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 168
[2025-01-19 23:07:30] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:07:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:32] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:32] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:32] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:32] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 169
[2025-01-19 23:07:32] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 113 confirm status: 0
[2025-01-19 23:07:32] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:32] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 68
[2025-01-19 23:07:32] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:07:32] debug: 	zh:deconz: resolve request (68)
[2025-01-19 23:07:32] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (68) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1198:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:07:32] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (68) Error: waiting for response TIMEOUT))
[2025-01-19 23:07:36] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (69) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:07:36] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (69) Error: waiting for response TIMEOUT))
[2025-01-19 23:07:39] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 170 request id: 115
[2025-01-19 23:07:39] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 115 status: 0
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:39] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 171
[2025-01-19 23:07:39] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 115 confirm status: 0
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:39] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 70
[2025-01-19 23:07:39] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:07:39] debug: 	zh:deconz: resolve request (70)
[2025-01-19 23:07:39] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 172
[2025-01-19 23:07:39] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 172 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 175
[2025-01-19 23:07:39] debug: 	zh:deconz:frameparser: response payload: 0846010000002069
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:39] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=175, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":70,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":105}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:07:39] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":70,"writeUndiv":false})
[2025-01-19 23:07:39] debug: 	zh:deconz: no response expected (70)
[2025-01-19 23:07:39] debug: 	zh:deconz: response received (70)
[2025-01-19 23:07:39] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":105}' from endpoint 1 with groupID 0
[2025-01-19 23:07:39] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":175,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 173 request id: 116
[2025-01-19 23:07:39] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 116 status: 0
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:39] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 174
[2025-01-19 23:07:39] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 116 confirm status: 0
[2025-01-19 23:07:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:39] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 70
[2025-01-19 23:07:39] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:07:39] debug: 	zh:deconz: resolve request (70)
[2025-01-19 23:07:40] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 175
[2025-01-19 23:07:40] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:07:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:49] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:49] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 176 request id: 117
[2025-01-19 23:07:49] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 117 status: 0
[2025-01-19 23:07:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:50] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 177
[2025-01-19 23:07:50] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:07:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:52] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:52] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 178 request id: 118
[2025-01-19 23:07:52] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 118 status: 0
[2025-01-19 23:07:52] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:53] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:53] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:53] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 179
[2025-01-19 23:07:53] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 118 confirm status: 0
[2025-01-19 23:07:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:53] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 72
[2025-01-19 23:07:53] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:07:53] debug: 	zh:deconz: resolve request (72)
[2025-01-19 23:07:53] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:07:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:53] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:07:53] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 180
[2025-01-19 23:07:53] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 180 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 175
[2025-01-19 23:07:53] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:07:53] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:53] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:07:53] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:07:53] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:07:53] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:07:55] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:07:55] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:07:55] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 181 request id: 119
[2025-01-19 23:07:55] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 119 status: 0
[2025-01-19 23:07:55] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:55] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:07:55] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:55] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:07:55] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 182
[2025-01-19 23:07:55] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 119 confirm status: 0
[2025-01-19 23:07:55] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:07:55] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 73
[2025-01-19 23:07:55] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:07:55] debug: 	zh:deconz: resolve request (73)
[2025-01-19 23:08:00] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:00] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:00] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 183
[2025-01-19 23:08:00] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 117 confirm status: 0
[2025-01-19 23:08:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:00] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 71
[2025-01-19 23:08:00] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:08:00] debug: 	zh:deconz: resolve request (71)
[2025-01-19 23:08:00] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (71) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1198:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:08:00] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (71) Error: waiting for response TIMEOUT))
[2025-01-19 23:08:00] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 184
[2025-01-19 23:08:00] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:08:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:03] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (72) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1198:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:08:03] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (72) Error: waiting for response TIMEOUT))
[2025-01-19 23:08:05] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (73) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:08:05] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (73) Error: waiting for response TIMEOUT))
[2025-01-19 23:08:09] debug: 	z2m: Saving state to file /app/data/state.json
[2025-01-19 23:08:10] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 185
[2025-01-19 23:08:10] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:08:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:11] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 186 request id: 120
[2025-01-19 23:08:11] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 120 status: 0
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:11] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 187
[2025-01-19 23:08:11] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 120 confirm status: 0
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:11] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 74
[2025-01-19 23:08:11] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:08:11] debug: 	zh:deconz: resolve request (74)
[2025-01-19 23:08:11] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 188
[2025-01-19 23:08:11] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 188 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 167
[2025-01-19 23:08:11] debug: 	zh:deconz:frameparser: response payload: 084a010000002069
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:11] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=167, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":74,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":105}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:08:11] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":74,"writeUndiv":false})
[2025-01-19 23:08:11] debug: 	zh:deconz: no response expected (74)
[2025-01-19 23:08:11] debug: 	zh:deconz: response received (74)
[2025-01-19 23:08:11] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":105}' from endpoint 1 with groupID 0
[2025-01-19 23:08:11] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":167,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 189 request id: 121
[2025-01-19 23:08:11] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 121 status: 0
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:11] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 190
[2025-01-19 23:08:11] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 121 confirm status: 0
[2025-01-19 23:08:11] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:11] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 74
[2025-01-19 23:08:11] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:08:11] debug: 	zh:deconz: resolve request (74)
[2025-01-19 23:08:16] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 191 request id: 122
[2025-01-19 23:08:16] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 122 status: 0
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:16] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 192
[2025-01-19 23:08:16] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 122 confirm status: 0
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:16] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 75
[2025-01-19 23:08:16] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:08:16] debug: 	zh:deconz: resolve request (75)
[2025-01-19 23:08:16] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 193
[2025-01-19 23:08:16] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 193 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 175
[2025-01-19 23:08:16] debug: 	zh:deconz:frameparser: response payload: 084b010000002069
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:16] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=175, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":75,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":105}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:08:16] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":75,"writeUndiv":false})
[2025-01-19 23:08:16] debug: 	zh:deconz: no response expected (75)
[2025-01-19 23:08:16] debug: 	zh:deconz: response received (75)
[2025-01-19 23:08:16] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":105}' from endpoint 1 with groupID 0
[2025-01-19 23:08:16] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":175,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 194 request id: 123
[2025-01-19 23:08:16] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 123 status: 0
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:16] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 195
[2025-01-19 23:08:16] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 123 confirm status: 0
[2025-01-19 23:08:16] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:16] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 75
[2025-01-19 23:08:16] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:08:16] debug: 	zh:deconz: resolve request (75)
[2025-01-19 23:08:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:08:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 196 request id: 124
[2025-01-19 23:08:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 124 status: 0
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 197 request id: 125
[2025-01-19 23:08:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 125 status: 0
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 198
[2025-01-19 23:08:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 125 confirm status: 0
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 77
[2025-01-19 23:08:18] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:08:18] debug: 	zh:deconz: resolve request (77)
[2025-01-19 23:08:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 199
[2025-01-19 23:08:18] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 199 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 175
[2025-01-19 23:08:18] debug: 	zh:deconz:frameparser: response payload: 084d010000002069
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:18] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=175, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":77,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":105}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:08:18] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":77,"writeUndiv":false})
[2025-01-19 23:08:18] debug: 	zh:deconz: no response expected (77)
[2025-01-19 23:08:18] debug: 	zh:deconz: response received (77)
[2025-01-19 23:08:18] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":105}' from endpoint 1 with groupID 0
[2025-01-19 23:08:18] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":175,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 200 request id: 126
[2025-01-19 23:08:18] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 126 status: 0
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:18] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 201
[2025-01-19 23:08:18] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 126 confirm status: 0
[2025-01-19 23:08:18] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:18] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 77
[2025-01-19 23:08:18] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:08:18] debug: 	zh:deconz: resolve request (77)
[2025-01-19 23:08:20] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x267f EP:0 SeqNr. 202 request id: 127
[2025-01-19 23:08:20] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 127 status: 0
[2025-01-19 23:08:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 203
[2025-01-19 23:08:20] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:08:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:21] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:08:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:21] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:08:21] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 204
[2025-01-19 23:08:21] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 204 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:08:21] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:08:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:21] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:08:21] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:08:21] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:08:21] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:08:22] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:08:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:22] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:08:22] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 205
[2025-01-19 23:08:22] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 205 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:08:22] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 23:08:22] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:22] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:08:22] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 23:08:22] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 23:08:22] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 23:08:23] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:08:23] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:08:23] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 206 request id: 128
[2025-01-19 23:08:23] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 128 status: 0
[2025-01-19 23:08:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:23] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:23] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:23] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 207
[2025-01-19 23:08:23] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 128 confirm status: 0
[2025-01-19 23:08:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:23] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 78
[2025-01-19 23:08:23] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:08:23] debug: 	zh:deconz: resolve request (78)
[2025-01-19 23:08:24] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 23:08:24] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:08:24] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 208 request id: 129
[2025-01-19 23:08:24] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 129 status: 0
[2025-01-19 23:08:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:24] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:24] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:24] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 209
[2025-01-19 23:08:24] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 129 confirm status: 0
[2025-01-19 23:08:24] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:24] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 79
[2025-01-19 23:08:24] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:08:24] debug: 	zh:deconz: resolve request (79)
[2025-01-19 23:08:28] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:28] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:28] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:28] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 210
[2025-01-19 23:08:28] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 124 confirm status: 0
[2025-01-19 23:08:28] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:28] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 76
[2025-01-19 23:08:28] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:08:28] debug: 	zh:deconz: resolve request (76)
[2025-01-19 23:08:28] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (76) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1198:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:08:28] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (76) Error: waiting for response TIMEOUT))
[2025-01-19 23:08:30] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:30] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:30] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 211
[2025-01-19 23:08:30] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x267f request id: 127 confirm status: 0
[2025-01-19 23:08:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:30] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 212
[2025-01-19 23:08:30] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:08:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:31] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 213 request id: 130
[2025-01-19 23:08:31] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 130 status: 0
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:31] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 214
[2025-01-19 23:08:31] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 130 confirm status: 0
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:31] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 80
[2025-01-19 23:08:31] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:08:31] debug: 	zh:deconz: resolve request (80)
[2025-01-19 23:08:31] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 215
[2025-01-19 23:08:31] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 215 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 167
[2025-01-19 23:08:31] debug: 	zh:deconz:frameparser: response payload: 0850010000002069
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:31] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=167, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":80,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":105}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:08:31] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":80,"writeUndiv":false})
[2025-01-19 23:08:31] debug: 	zh:deconz: no response expected (80)
[2025-01-19 23:08:31] debug: 	zh:deconz: response received (80)
[2025-01-19 23:08:31] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":105}' from endpoint 1 with groupID 0
[2025-01-19 23:08:31] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":167,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 216 request id: 131
[2025-01-19 23:08:31] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 131 status: 0
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:31] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 217
[2025-01-19 23:08:31] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 131 confirm status: 0
[2025-01-19 23:08:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:31] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 80
[2025-01-19 23:08:31] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:08:31] debug: 	zh:deconz: resolve request (80)
[2025-01-19 23:08:33] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (78) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:08:33] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (78) Error: waiting for response TIMEOUT))
[2025-01-19 23:08:34] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (79) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:08:34] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (79) Error: waiting for response TIMEOUT))
[2025-01-19 23:08:39] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 218 request id: 132
[2025-01-19 23:08:39] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 219 request id: 133
[2025-01-19 23:08:39] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 132 status: 0
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:39] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 133 status: 0
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:39] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 220
[2025-01-19 23:08:39] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 133 confirm status: 0
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:39] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 82
[2025-01-19 23:08:39] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:08:39] debug: 	zh:deconz: resolve request (82)
[2025-01-19 23:08:39] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 221
[2025-01-19 23:08:39] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 221 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 175
[2025-01-19 23:08:39] debug: 	zh:deconz:frameparser: response payload: 0852010000002069
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:39] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=175, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":82,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":105}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:08:39] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":82,"writeUndiv":false})
[2025-01-19 23:08:39] debug: 	zh:deconz: no response expected (82)
[2025-01-19 23:08:39] debug: 	zh:deconz: response received (82)
[2025-01-19 23:08:39] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":105}' from endpoint 1 with groupID 0
[2025-01-19 23:08:39] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":175,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 222 request id: 134
[2025-01-19 23:08:39] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 134 status: 0
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:39] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 223
[2025-01-19 23:08:39] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 134 confirm status: 0
[2025-01-19 23:08:39] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:39] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 82
[2025-01-19 23:08:39] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:08:39] debug: 	zh:deconz: resolve request (82)
[2025-01-19 23:08:40] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 224
[2025-01-19 23:08:40] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:08:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:40] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:08:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:40] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:08:40] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 225
[2025-01-19 23:08:40] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 225 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 175
[2025-01-19 23:08:40] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:08:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:40] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:08:40] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:08:40] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:08:41] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:08:41] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:08:41] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:41] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:08:41] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 226
[2025-01-19 23:08:41] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 226 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 23:08:41] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 23:08:41] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:41] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:08:41] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 23:08:41] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 23:08:41] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 23:08:41] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:08:41] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:41] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:08:41] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 227
[2025-01-19 23:08:41] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 227 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 23:08:41] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:08:41] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:41] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:08:41] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:08:41] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:08:41] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:08:43] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 23:08:43] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:08:43] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 228 request id: 135
[2025-01-19 23:08:43] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 135 status: 0
[2025-01-19 23:08:43] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:43] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:43] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:43] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:43] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 229
[2025-01-19 23:08:43] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 135 confirm status: 0
[2025-01-19 23:08:43] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:43] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 83
[2025-01-19 23:08:43] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:08:43] debug: 	zh:deconz: resolve request (83)
[2025-01-19 23:08:43] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:08:43] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:08:43] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 230 request id: 136
[2025-01-19 23:08:43] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 136 status: 0
[2025-01-19 23:08:43] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:43] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:43] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:43] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:43] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 231
[2025-01-19 23:08:43] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 136 confirm status: 0
[2025-01-19 23:08:43] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:44] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 84
[2025-01-19 23:08:44] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:08:44] debug: 	zh:deconz: resolve request (84)
[2025-01-19 23:08:49] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:49] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:49] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 232
[2025-01-19 23:08:49] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 132 confirm status: 0
[2025-01-19 23:08:49] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:49] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 81
[2025-01-19 23:08:49] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:08:49] debug: 	zh:deconz: resolve request (81)
[2025-01-19 23:08:49] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (81) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1198:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:08:49] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (81) Error: waiting for response TIMEOUT))
[2025-01-19 23:08:50] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 233
[2025-01-19 23:08:50] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:08:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:54] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (84) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:08:54] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (83) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:08:54] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (84) Error: waiting for response TIMEOUT))
[2025-01-19 23:08:54] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (83) Error: waiting for response TIMEOUT))
[2025-01-19 23:08:56] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 234 request id: 137
[2025-01-19 23:08:56] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 137 status: 0
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:56] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 235
[2025-01-19 23:08:56] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 137 confirm status: 0
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:56] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 85
[2025-01-19 23:08:56] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:08:56] debug: 	zh:deconz: resolve request (85)
[2025-01-19 23:08:56] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 236
[2025-01-19 23:08:56] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 236 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 175
[2025-01-19 23:08:56] debug: 	zh:deconz:frameparser: response payload: 0855010000002069
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:56] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=175, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":85,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":105}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:08:56] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":85,"writeUndiv":false})
[2025-01-19 23:08:56] debug: 	zh:deconz: no response expected (85)
[2025-01-19 23:08:56] debug: 	zh:deconz: response received (85)
[2025-01-19 23:08:56] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":105}' from endpoint 1 with groupID 0
[2025-01-19 23:08:56] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":175,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 237 request id: 138
[2025-01-19 23:08:56] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 138 status: 0
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:56] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 238
[2025-01-19 23:08:56] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 138 confirm status: 0
[2025-01-19 23:08:56] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:56] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 85
[2025-01-19 23:08:56] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:08:56] debug: 	zh:deconz: resolve request (85)
[2025-01-19 23:08:57] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:08:57] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 239 request id: 139
[2025-01-19 23:08:57] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 139 status: 0
[2025-01-19 23:08:57] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:58] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:08:58] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:58] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:08:58] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 240
[2025-01-19 23:08:58] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 240 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 167
[2025-01-19 23:08:58] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:08:58] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:58] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:08:58] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:08:58] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:08:58] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:08:59] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:08:59] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:59] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:08:59] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 241
[2025-01-19 23:08:59] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 241 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 23:08:59] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 23:08:59] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:08:59] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:08:59] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 23:08:59] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 23:08:59] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 23:09:00] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 242
[2025-01-19 23:09:00] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:09:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:00] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:09:00] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:09:00] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 243 request id: 140
[2025-01-19 23:09:00] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 140 status: 0
[2025-01-19 23:09:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:00] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:09:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:00] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:09:00] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 244
[2025-01-19 23:09:00] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 140 confirm status: 0
[2025-01-19 23:09:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:00] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 87
[2025-01-19 23:09:00] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:09:00] debug: 	zh:deconz: resolve request (87)
[2025-01-19 23:09:01] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 23:09:01] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:09:01] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 245 request id: 141
[2025-01-19 23:09:01] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 141 status: 0
[2025-01-19 23:09:01] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:01] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:09:01] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:01] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:09:01] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 246
[2025-01-19 23:09:01] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 141 confirm status: 0
[2025-01-19 23:09:01] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:01] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 88
[2025-01-19 23:09:01] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:09:01] debug: 	zh:deconz: resolve request (88)
[2025-01-19 23:09:06] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 247 request id: 142
[2025-01-19 23:09:06] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 142 status: 0
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:06] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 248
[2025-01-19 23:09:06] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 142 confirm status: 0
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:06] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 89
[2025-01-19 23:09:06] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:09:06] debug: 	zh:deconz: resolve request (89)
[2025-01-19 23:09:06] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 249
[2025-01-19 23:09:06] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 249 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 175
[2025-01-19 23:09:06] debug: 	zh:deconz:frameparser: response payload: 0859010000002069
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:06] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=175, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":89,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":105}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:09:06] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":89,"writeUndiv":false})
[2025-01-19 23:09:06] debug: 	zh:deconz: no response expected (89)
[2025-01-19 23:09:06] debug: 	zh:deconz: response received (89)
[2025-01-19 23:09:06] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":105}' from endpoint 1 with groupID 0
[2025-01-19 23:09:06] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":175,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 250 request id: 143
[2025-01-19 23:09:06] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 143 status: 0
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:06] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 251
[2025-01-19 23:09:06] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 143 confirm status: 0
[2025-01-19 23:09:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:06] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 89
[2025-01-19 23:09:06] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:09:06] debug: 	zh:deconz: resolve request (89)
[2025-01-19 23:09:07] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (86) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1198:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:09:07] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (86) Error: waiting for response TIMEOUT))
[2025-01-19 23:09:07] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:09:07] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:07] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:09:07] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 252
[2025-01-19 23:09:07] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 139 confirm status: 0
[2025-01-19 23:09:07] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:07] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 86
[2025-01-19 23:09:07] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:09:07] debug: 	zh:deconz: resolve request (86)
[2025-01-19 23:09:08] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:09:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:08] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:09:08] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 253
[2025-01-19 23:09:08] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 253 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x6 lqi: 167
[2025-01-19 23:09:08] debug: 	zh:deconz:frameparser: response payload: 01fdff040101190000
[2025-01-19 23:09:08] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:08] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - Error: Unsupported response reading for cluster ID '6'.
[2025-01-19 23:09:09] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:09:09] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:09] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:09:09] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 254
[2025-01-19 23:09:09] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 254 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x19 lqi: 175
[2025-01-19 23:09:09] debug: 	zh:deconz:frameparser: response payload: 010301018911a000107319030200
[2025-01-19 23:09:09] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:09] debug: 	zh:controller: Received payload: clusterID=25, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=175, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":0,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":3,"commandIdentifier":1},"payload":{"fieldControl":1,"manufacturerCode":4489,"imageType":160,"fileVersion":51999504},"command":{"ID":1,"response":2,"parameters":[{"name":"fieldControl","type":32},{"name":"manufacturerCode","type":33},{"name":"imageType","type":33},{"name":"fileVersion","type":35}],"name":"queryNextImageRequest"}}
[2025-01-19 23:09:09] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'commandQueryNextImageRequest', cluster 'genOta', data '{"fieldControl":1,"fileVersion":51999504,"imageType":160,"manufacturerCode":4489}' from endpoint 1 with groupID 0
[2025-01-19 23:09:09] debug: 	z2m: Device 'Bogenlampe' requested OTA
[2025-01-19 23:09:10] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 1 request id: 144
[2025-01-19 23:09:10] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 144 status: 0
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:10] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 2
[2025-01-19 23:09:10] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 144 confirm status: 0
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:10] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 90
[2025-01-19 23:09:10] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:09:10] debug: 	zh:deconz: resolve request (90)
[2025-01-19 23:09:10] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 3
[2025-01-19 23:09:10] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 3 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 167
[2025-01-19 23:09:10] debug: 	zh:deconz:frameparser: response payload: 085a010000002069
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:10] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=167, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":90,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":105}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:09:10] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":90,"writeUndiv":false})
[2025-01-19 23:09:10] debug: 	zh:deconz: no response expected (90)
[2025-01-19 23:09:10] debug: 	zh:deconz: response received (90)
[2025-01-19 23:09:10] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":105}' from endpoint 1 with groupID 0
[2025-01-19 23:09:10] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":167,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 4 request id: 145
[2025-01-19 23:09:10] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 145 status: 0
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:10] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 5
[2025-01-19 23:09:10] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 145 confirm status: 0
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:10] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 90
[2025-01-19 23:09:10] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:09:10] debug: 	zh:deconz: resolve request (90)
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 6
[2025-01-19 23:09:10] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:09:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:11] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (88) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:09:11] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (87) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:09:11] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (88) Error: waiting for response TIMEOUT))
[2025-01-19 23:09:11] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (87) Error: waiting for response TIMEOUT))
[2025-01-19 23:09:12] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:09:12] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:12] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:09:12] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 7
[2025-01-19 23:09:12] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 7 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x19 lqi: 167
[2025-01-19 23:09:12] debug: 	zh:deconz:frameparser: response payload: 010401018911a000107319030200
[2025-01-19 23:09:12] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:12] debug: 	zh:controller: Received payload: clusterID=25, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=167, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":0,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":4,"commandIdentifier":1},"payload":{"fieldControl":1,"manufacturerCode":4489,"imageType":160,"fileVersion":51999504},"command":{"ID":1,"response":2,"parameters":[{"name":"fieldControl","type":32},{"name":"manufacturerCode","type":33},{"name":"imageType","type":33},{"name":"fileVersion","type":35}],"name":"queryNextImageRequest"}}
[2025-01-19 23:09:12] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'commandQueryNextImageRequest', cluster 'genOta', data '{"fieldControl":1,"fileVersion":51999504,"imageType":160,"manufacturerCode":4489}' from endpoint 1 with groupID 0
[2025-01-19 23:09:13] debug: 	z2m: Device 'Bogenlampe' requested OTA
[2025-01-19 23:09:16] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:09:16] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:16] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:09:16] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 8
[2025-01-19 23:09:16] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 8 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x19 lqi: 167
[2025-01-19 23:09:16] debug: 	zh:deconz:frameparser: response payload: 010501018911a000107319030200
[2025-01-19 23:09:16] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:16] debug: 	zh:controller: Received payload: clusterID=25, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=167, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":0,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":5,"commandIdentifier":1},"payload":{"fieldControl":1,"manufacturerCode":4489,"imageType":160,"fileVersion":51999504},"command":{"ID":1,"response":2,"parameters":[{"name":"fieldControl","type":32},{"name":"manufacturerCode","type":33},{"name":"imageType","type":33},{"name":"fileVersion","type":35}],"name":"queryNextImageRequest"}}
[2025-01-19 23:09:16] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'commandQueryNextImageRequest', cluster 'genOta', data '{"fieldControl":1,"fileVersion":51999504,"imageType":160,"manufacturerCode":4489}' from endpoint 1 with groupID 0
[2025-01-19 23:09:16] debug: 	z2m: Device 'Bogenlampe' requested OTA
[2025-01-19 23:09:19] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:09:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:19] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:09:19] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 9
[2025-01-19 23:09:19] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 9 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x19 lqi: 175
[2025-01-19 23:09:19] debug: 	zh:deconz:frameparser: response payload: 010601018911a000107319030200
[2025-01-19 23:09:19] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:19] debug: 	zh:controller: Received payload: clusterID=25, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=175, frame={"header":{"frameControl":{"frameType":1,"manufacturerSpecific":false,"direction":0,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":6,"commandIdentifier":1},"payload":{"fieldControl":1,"manufacturerCode":4489,"imageType":160,"fileVersion":51999504},"command":{"ID":1,"response":2,"parameters":[{"name":"fieldControl","type":32},{"name":"manufacturerCode","type":33},{"name":"imageType","type":33},{"name":"fileVersion","type":35}],"name":"queryNextImageRequest"}}
[2025-01-19 23:09:19] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'commandQueryNextImageRequest', cluster 'genOta', data '{"fieldControl":1,"fileVersion":51999504,"imageType":160,"manufacturerCode":4489}' from endpoint 1 with groupID 0
[2025-01-19 23:09:19] debug: 	z2m: Device 'Bogenlampe' requested OTA
[2025-01-19 23:09:20] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:09:20] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 10 request id: 146
[2025-01-19 23:09:20] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 146 status: 0
[2025-01-19 23:09:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:20] error: 	z2m: Failed to execute LQI for 'Flur'
[2025-01-19 23:09:20] debug: 	z2m: Error: waiting for response TIMEOUT
    at DeconzAdapter.checkReceivedDataPayload (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:703:28)
    at Timeout._onTimeout (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:75:18)
    at listOnTimeout (node:internal/timers:569:17)
    at processTimers (node:internal/timers:512:7)
[2025-01-19 23:09:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 11
[2025-01-19 23:09:20] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:09:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:21] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x1c3 EP:0 SeqNr. 12 request id: 147
[2025-01-19 23:09:21] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 147 status: 0
[2025-01-19 23:09:21] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:23] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:09:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:23] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:09:23] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 13
[2025-01-19 23:09:23] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 13 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 175
[2025-01-19 23:09:23] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:09:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:23] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:09:23] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:09:23] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:09:23] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:09:23] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:09:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:23] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:09:23] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 14
[2025-01-19 23:09:23] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 14 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 23:09:23] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 23:09:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:23] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:09:23] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 23:09:23] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 23:09:23] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 23:09:25] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:09:25] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:09:25] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 15 request id: 148
[2025-01-19 23:09:25] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 148 status: 0
[2025-01-19 23:09:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:25] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:09:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:25] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:09:25] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 16
[2025-01-19 23:09:25] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 148 confirm status: 0
[2025-01-19 23:09:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:25] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 92
[2025-01-19 23:09:25] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:09:25] debug: 	zh:deconz: resolve request (92)
[2025-01-19 23:09:25] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 23:09:25] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:09:25] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 17 request id: 149
[2025-01-19 23:09:25] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 149 status: 0
[2025-01-19 23:09:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:25] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:09:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:25] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:09:25] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 18
[2025-01-19 23:09:25] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 149 confirm status: 0
[2025-01-19 23:09:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:25] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 93
[2025-01-19 23:09:25] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:09:25] debug: 	zh:deconz: resolve request (93)
[2025-01-19 23:09:30] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (91) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1198:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:09:30] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (91) Error: waiting for response TIMEOUT))
[2025-01-19 23:09:30] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:09:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:30] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:09:30] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 19
[2025-01-19 23:09:30] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 146 confirm status: 0
[2025-01-19 23:09:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:30] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 91
[2025-01-19 23:09:30] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:09:30] debug: 	zh:deconz: resolve request (91)
[2025-01-19 23:09:30] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 20
[2025-01-19 23:09:30] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:09:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:31] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:09:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:31] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:09:31] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 21
[2025-01-19 23:09:31] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x1c3 request id: 147 confirm status: 0
[2025-01-19 23:09:31] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:35] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (92) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:09:35] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (92) Error: waiting for response TIMEOUT))
[2025-01-19 23:09:36] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (93) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:09:36] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (93) Error: waiting for response TIMEOUT))
[2025-01-19 23:09:40] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 22
[2025-01-19 23:09:40] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:09:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:50] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 23
[2025-01-19 23:09:50] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:09:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:51] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 24 request id: 150
[2025-01-19 23:09:51] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 150 status: 0
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:51] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 25
[2025-01-19 23:09:51] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 150 confirm status: 0
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:51] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 94
[2025-01-19 23:09:51] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:09:51] debug: 	zh:deconz: resolve request (94)
[2025-01-19 23:09:51] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 26
[2025-01-19 23:09:51] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 26 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 167
[2025-01-19 23:09:51] debug: 	zh:deconz:frameparser: response payload: 085e010000002069
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:51] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=167, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":94,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":105}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:09:51] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":94,"writeUndiv":false})
[2025-01-19 23:09:51] debug: 	zh:deconz: no response expected (94)
[2025-01-19 23:09:51] debug: 	zh:deconz: response received (94)
[2025-01-19 23:09:51] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":105}' from endpoint 1 with groupID 0
[2025-01-19 23:09:51] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":167,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 27 request id: 151
[2025-01-19 23:09:51] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 151 status: 0
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:51] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 28
[2025-01-19 23:09:51] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 151 confirm status: 0
[2025-01-19 23:09:51] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:09:51] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 94
[2025-01-19 23:09:51] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:09:51] debug: 	zh:deconz: resolve request (94)
[2025-01-19 23:10:00] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 29
[2025-01-19 23:10:00] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:10:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:04] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:10:04] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:04] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:10:04] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 30
[2025-01-19 23:10:04] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 30 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 175
[2025-01-19 23:10:04] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:10:04] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:04] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:10:04] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:10:04] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:10:04] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:10:06] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:10:06] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:10:06] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 31 request id: 152
[2025-01-19 23:10:06] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 152 status: 0
[2025-01-19 23:10:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:06] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:10:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:06] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:10:06] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 32
[2025-01-19 23:10:06] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 152 confirm status: 0
[2025-01-19 23:10:06] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:06] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 95
[2025-01-19 23:10:06] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:10:06] debug: 	zh:deconz: resolve request (95)
[2025-01-19 23:10:10] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 33
[2025-01-19 23:10:10] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:10:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:16] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (95) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:10:16] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (95) Error: waiting for response TIMEOUT))
[2025-01-19 23:10:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 34
[2025-01-19 23:10:20] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:10:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:25] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:10:25] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 35 request id: 153
[2025-01-19 23:10:25] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 153 status: 0
[2025-01-19 23:10:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:25] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:10:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:25] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:10:25] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 36
[2025-01-19 23:10:25] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 153 confirm status: 0
[2025-01-19 23:10:25] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:25] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 96
[2025-01-19 23:10:25] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:10:25] debug: 	zh:deconz: resolve request (96)
[2025-01-19 23:10:26] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 37 request id: 154
[2025-01-19 23:10:26] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 154 status: 0
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:26] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 38
[2025-01-19 23:10:26] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 154 confirm status: 0
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:26] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 97
[2025-01-19 23:10:26] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:10:26] debug: 	zh:deconz: resolve request (97)
[2025-01-19 23:10:26] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 39
[2025-01-19 23:10:26] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 39 srcAddr: 0x45e destAddr: 0x0 profile id: 0x104 cluster id: 0x8 lqi: 167
[2025-01-19 23:10:26] debug: 	zh:deconz:frameparser: response payload: 0861010000002069
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:26] debug: 	zh:controller: Received payload: clusterID=8, address=1118, groupID=0, endpoint=1, destinationEndpoint=1, wasBroadcast=false, linkQuality=167, frame={"header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":false,"reservedBits":0},"transactionSequenceNumber":97,"commandIdentifier":1},"payload":[{"attrId":0,"status":0,"dataType":32,"attrData":105}],"command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}}
[2025-01-19 23:10:26] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genLevelCtrl.defaultRsp({"cmdId":1,"statusCode":0}, {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":1,"reservedBits":0,"transactionSequenceNumber":97,"writeUndiv":false})
[2025-01-19 23:10:26] debug: 	zh:deconz: no response expected (97)
[2025-01-19 23:10:26] debug: 	zh:deconz: response received (97)
[2025-01-19 23:10:26] debug: 	z2m: Received Zigbee message from 'Bogenlampe', type 'readResponse', cluster 'genLevelCtrl', data '{"currentLevel":105}' from endpoint 1 with groupID 0
[2025-01-19 23:10:26] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/Bogenlampe', payload '{"brightness":105,"color":{"x":0.4599,"y":0.4106},"color_mode":"color_temp","color_temp":370,"effect":null,"linkquality":167,"state":"ON","update":{"installed_version":51999504,"latest_version":51999504,"state":"idle"}}'
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 40 request id: 155
[2025-01-19 23:10:26] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 155 status: 0
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x1c3 EP:0 SeqNr. 41 request id: 156
[2025-01-19 23:10:26] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 156 status: 0
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:26] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 42
[2025-01-19 23:10:26] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 155 confirm status: 0
[2025-01-19 23:10:26] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:26] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 97
[2025-01-19 23:10:26] debug: 	zh:deconz: false, true, false, 10000
[2025-01-19 23:10:26] debug: 	zh:deconz: resolve request (97)
[2025-01-19 23:10:30] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 43
[2025-01-19 23:10:30] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:10:30] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:35] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (96) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at runNextTicks (node:internal/process/task_queues:60:5)
    at processTimers (node:internal/timers:509:9)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1198:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:10:35] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genLevelCtrl.read(["currentLevel"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (96) Error: waiting for response TIMEOUT))
[2025-01-19 23:10:36] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:10:36] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:36] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:10:36] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 44
[2025-01-19 23:10:36] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x1c3 request id: 156 confirm status: 0
[2025-01-19 23:10:36] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:38] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:10:38] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:38] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:10:38] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 45
[2025-01-19 23:10:38] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 45 srcAddr: 0x45e destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 175
[2025-01-19 23:10:38] debug: 	zh:deconz:frameparser: response payload: 815e04f2fc1f0000b8d1f08e
[2025-01-19 23:10:38] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:38] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":1118,"eui64":"0xf0d1b800001ffcf2","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:10:38] debug: 	zh:controller: Device announce from '0xf0d1b800001ffcf2:1118'
[2025-01-19 23:10:38] debug: 	z2m: Device 'Bogenlampe' announced itself
[2025-01-19 23:10:38] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Bogenlampe","ieee_address":"0xf0d1b800001ffcf2"},"type":"device_announce"}'
[2025-01-19 23:10:38] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10101010
[2025-01-19 23:10:38] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 1 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:38] debug: 	zh:deconz:driver: query aps data indication
[2025-01-19 23:10:38] debug: 	zh:deconz:driver: DATA_INDICATION - sending read data request - SeqNr. 46
[2025-01-19 23:10:38] debug: 	zh:deconz:frameparser: DATA_INDICATION RESPONSE - seqNr. 46 srcAddr: 0xb9ef destAddr: 0xfffd profile id: 0x0 cluster id: 0x13 lqi: 255
[2025-01-19 23:10:38] debug: 	zh:deconz:frameparser: response payload: 81efb9f088130000b8d1f08e
[2025-01-19 23:10:38] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:38] debug: 	zh:controller: Received ZDO response: clusterId=END_DEVICE_ANNOUNCE, status=SUCCESS, payload={"nwkAddress":47599,"eui64":"0xf0d1b800001388f0","capabilities":{"alternatePANCoordinator":0,"deviceType":1,"powerSource":1,"rxOnWhenIdle":1,"reserved1":0,"reserved2":0,"securityCapability":0,"allocateAddress":1}}
[2025-01-19 23:10:38] debug: 	zh:controller: Device announce from '0xf0d1b800001388f0:47599'
[2025-01-19 23:10:38] debug: 	z2m: Device 'Flurlicht' announced itself
[2025-01-19 23:10:38] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/event', payload '{"data":{"friendly_name":"Flurlicht","ieee_address":"0xf0d1b800001388f0"},"type":"device_announce"}'
[2025-01-19 23:10:40] debug: 	z2m: Retrieving state of 'Bogenlampe' after reconnect
[2025-01-19 23:10:40] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0x45e EP:1 SeqNr. 47 request id: 157
[2025-01-19 23:10:40] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 157 status: 0
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:40] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 48
[2025-01-19 23:10:40] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0x45e request id: 157 confirm status: 0
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:40] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 98
[2025-01-19 23:10:40] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:10:40] debug: 	zh:deconz: resolve request (98)
[2025-01-19 23:10:40] debug: 	z2m: Retrieving state of 'Flurlicht' after reconnect
[2025-01-19 23:10:40] debug: 	zh:controller:endpoint: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false})
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xb9ef EP:1 SeqNr. 49 request id: 158
[2025-01-19 23:10:40] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 158 status: 0
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:40] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 50
[2025-01-19 23:10:40] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xb9ef request id: 158 confirm status: 0
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:40] debug: 	zh:deconz: sendZclFrameToEndpoint - message send with transSeq Nr.: 99
[2025-01-19 23:10:40] debug: 	zh:deconz: true, true, false, 10000
[2025-01-19 23:10:40] debug: 	zh:deconz: resolve request (99)
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 51
[2025-01-19 23:10:40] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:10:40] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:50] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 52
[2025-01-19 23:10:50] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:10:50] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:10:50] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (99) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:10:50] debug: 	zh:controller:endpoint: Error: ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (98) Error: waiting for response TIMEOUT)
    at DeconzAdapter.sendZclFrameToEndpoint (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/adapter/deconz/adapter/deconzAdapter.ts:475:19)
    at Request.send (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/helpers/request.ts:82:20)
    at Endpoint.sendRequest (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:324:20)
    at Endpoint.zclCommand (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:949:28)
    at Endpoint.read (/app/node_modules/.pnpm/zigbee-herdsman@3.2.1/node_modules/zigbee-herdsman/src/controller/model/endpoint.ts:445:29)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:58:13)
    at Object.convertGet (/app/node_modules/.pnpm/zigbee-herdsman-converters@21.12.0/node_modules/src/converters/toZigbee.ts:1200:17)
    at Object.<anonymous> (/app/lib/extension/availability.ts:251:25)
[2025-01-19 23:10:50] error: 	z2m: Failed to read state of 'Flurlicht' after reconnect (ZCL command 0xf0d1b800001388f0/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (99) Error: waiting for response TIMEOUT))
[2025-01-19 23:10:50] error: 	z2m: Failed to read state of 'Bogenlampe' after reconnect (ZCL command 0xf0d1b800001ffcf2/1 genOnOff.read(["onOff"], {"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"reservedBits":0,"writeUndiv":false}) failed (no response received (98) Error: waiting for response TIMEOUT))
[2025-01-19 23:11:00] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 53
[2025-01-19 23:11:00] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:11:00] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:11:10] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 54
[2025-01-19 23:11:10] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:11:10] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:11:20] debug: 	zh:deconz:driver: send read device state from queue. seqNr: 55
[2025-01-19 23:11:20] debug: 	zh:deconz:frameparser: device state: 10100010
[2025-01-19 23:11:20] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:11:23] debug: 	z2m: Saving state to file /app/data/state.json
[2025-01-19 23:11:23] info: 	z2m:mqtt: MQTT publish: topic 'zigbee2mqtt/bridge/state', payload '{"state":"offline"}'
[2025-01-19 23:11:23] info: 	z2m: Disconnecting from MQTT server
[2025-01-19 23:11:23] info: 	z2m: Stopping zigbee-herdsman...
[2025-01-19 23:11:23] debug: 	zh:controller: Disable joining
[2025-01-19 23:11:23] debug: 	zh:deconz: zclFrame to all - 242
[2025-01-19 23:11:23] debug: 	zh:deconz: sendZclFrameToAll - message send
[2025-01-19 23:11:23] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xfffd EP:242 SeqNr. 56 request id: 159
[2025-01-19 23:11:23] debug: 	zh:deconz:frameparser: DATA_REQUEST RESPONSE - request id: 159 status: 0
[2025-01-19 23:11:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:11:23] debug: 	zh:deconz:frameparser: DEVICE_STATE changed: 10100110
[2025-01-19 23:11:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 1 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:11:23] debug: 	zh:deconz:driver: query aps data confirm
[2025-01-19 23:11:23] debug: 	zh:deconz:driver: DATA_CONFIRM - sending data state request - SeqNr. 57
[2025-01-19 23:11:23] debug: 	zh:deconz:frameparser: DATA_CONFIRM RESPONSE - destAddr: 0xfffd request id: 159 confirm status: 0
[2025-01-19 23:11:23] debug: 	zh:deconz:driver: networkstate: 2 apsDataConfirm: 0 apsDataIndication: 0 configChanged: 0 apsRequestFreeSlots: 1
[2025-01-19 23:11:23] debug: 	zh:deconz:driver: send write parameter request from queue. seqNr: 58 paramId: 33 param: 0
[2025-01-19 23:11:23] debug: 	zh:deconz:frameparser: write parameter response - parameter id: 33 - status: 0
[2025-01-19 23:11:23] debug: 	zh:deconz: Permit joining on coordinator for 0 sec.
[2025-01-19 23:11:23] debug: 	zh:controller:database: Writing database to '/app/data/database.db'
[2025-01-19 23:11:23] debug: 	zh:deconz:driver: DATA_REQUEST - destAddr: 0xfffc EP:0 SeqNr. 59 request id: 160
[2025-01-19 23:11:23] info: 	z2m: Stopped zigbee-herdsman
[2025-01-19 23:11:23] info: 	z2m: Stopped Zigbee2MQTT
